# Polarity

The Polarity View provides polarity switch for each devices input. The DSP for this polarity switch is after the physical input and this is designed to aide in troubleshooting wiring issues that can happen in powered systems without having to physically access the array. In a typical work flow, the polarity switch should not need to be utilized.

Cardioid presets for subwoofers include all processing required to create a cardioid array. Toggling the user facing polarity switch is not required.

To toggle the polarity of a device, select the image of that device in the Workspace. When connected and in-sync, the changes made to the devices are in real-time, if the system is disconnected, the changes will be sent to the devices once they are connected.

## Polarity Indicators

Indicator | Description
--- | ---
| Input polarity in a normal state
| Input polarity is reversed