# Delay View

The Delay view displays an adjustable delay setting for each respective Array or in some cases, individual devices in the Workspace. When connected and in-sync, the changes made to the devices are in real-time, if the system is disconnected, the changes will be sent to the devices once they are connected.

## Adjusting a Delay Control

Any delay control can be adjusted using the or the buttons located next to the delay value.

A delay value can also be manually entered by double clicking on the delay time and typing in a new one using the onscreen numeric keypad or a keyboard.

## Relative Delay Controls

The icon in the array header can be selected to make relative delay adjustments to all members of a System Group. The Relative Gain control will increment all members of an array by the value entered in the Relative Delay adjustment control box, preserving any offset that may exist between individual arrays. The Relative Delay control will only be displayed in the first Array Header of a group of arrays in the same System Group.

## Subwoofer Group Delays

The resolution of delay controls displayed on a subwoofer array varies based on the quantity of subwoofer arrays in a Subwoofer System Group.

#### Subwoofer System Groups with 1 Array

Single, Row Array Subwoofer System Groups will have a delay control per subwoofer within the array .

#### Subwoofer System Groups with Greater than 1 Array

Multi- Array Subwoofer System Groups, or column oriented groups, will display a single delay control per subwoofer array.

## Unequal DSP Indicator

In the event that one (or multiple) Subwoofers within an Array have a grouped delay value that is not equal to the delay value of the rest of the array, a small yellow indicator will appear next to that delay value. This unequal DSP situation can be resolved by re-entering the intended value and hitting enter, the software will resend the correct value to all devices within the array and as a result the devices which previously had differing values will be re-aligned with the rest of the array. In most cases, the Unequal DSP indicator will be triggered when a delay setting is manually changed via the LCD screen on a single device or in the Device Panel utility. The Device Panel Utility can always be used to interrogate individual devices and locate the device with the DSP value offset.