# Temperature View

The Temperature view shows the real-time reported temperature for each device in terms of thermal headroom. Each device's thermal capabilities could be different in absolute terms so the % remaining before thermal fault is displayed. A value of 100% would mean the device has entered a thermal fault and has stopped working to allow the device to cool down to a safe temperature. The color state of each device is determined by the reported value and the state is indicated by a simple red, yellow or green color.

## Temperature States

Indicator | Color | Description
--- | --- | ---
| Green | Temperature is within the device's normal operating limits.
| Yellow | Temperature is approaching 80-90% of the limit and may begin limiting performance to avoid thermal shutdown.
| Red | Temperature has reached 90% and is close to exceeding the safe operating range. As the device approaches 100%, it will enter a thermal shutdown to protect itself.