# Load Monitoring View

The Load Monitoring View reports the measured load from the amplifier as a 3 color state. The data is derived from taking real time impedance values from the system. The reliability of the values returned are based upon the program material. The spectral content and level of the signal going to the transducers must be loud enough and full spectrum enough to return a valid result. The load monitoring view will report the measured load automatically when the view is active and devices are connected.

## Load Monitoring Results

Image | Color | Status
--- | --- | ---
| Green | Everything is working within expected range.
| Yellow | The real-time impedance values are on the edges of the expected tolerances. If the signal being provided is low level or not full spectrum, this can provide a false reading.
| Red | The real-time impedance values are outside the expected tolerances. If the signal being provided is low level or not full spectrum, this can provide a false reading, otherwise there may be a hardware fault.