# Output Meters

The Output Meters View overlays the information from the connected devices amplifier output meter directly over the virtual system in the Workspace with each amplifier bandpass having its own meter. The keyboard shortcut to enter Output Meter View is `O` . Pressing `O` again will toggle between array level and circuit level meters.

## Meter Types

The output meters can be displayed at the device or array level by selecting the corresponding meter view button from the top of the application window.

| Array Meter | Device Meter
--- | --- | ---
Button |  |
Display |  |

## Meter Data

The scale of the meter in the workspace is from -48 to 0 dBu before limit with the marks roughly every 6 dB, the meter is a system headroom meter and contains an RMS meter, a Peak Meter, A Limit LED and a clip LED. The limit LED will light when the system is 3 dB into limit and the Clip LED will light if the amplifier output reports a clip.

Normal | Limit | Clip
--- | --- | ---