# Voltage

The Voltage view shows the real-time reported input mains voltage for each device. The color state of each device is determined by the device's input voltage capabilities and the state is indicated by a simple red, yellow or green color.

## Voltage States

Image | Color | Description
--- | --- | ---
| Green | The voltage at the device is within normal operating limits.
| Yellow | The mains voltage is at the edges of the normal operating voltage.
| Red | The voltage is outside the normal operating voltage.