# Tune Mode

After verifying the functionality of all devices in Test Mode, users are able to enter Tune Mode where they can use the various System Views to modify device DSP parameters such as Gain, Delay, EQ, etc to acoustically optimize an audio system for use.

## Tune Mode Screen Overview

| Name | Function
--- | --- | ---
1 | Groups Panel | Provides mute and selection controls at various system levels as well as access to a custom group creator.
2 | Tune Mode Views | Switches between the various System Views available.

## Tune Mode System Views

View | Shortcut | Use
--- | --- | ---
| M | Use this view to mute or un-mute Groups, Arrays, or individual bandpasses.
| P | Change Speaker Presets, Speaker Crossover, and Subwoofer Orientation.
| G | Adjust device gain settings, this is the default workspace view in Test Mode.
| Y | Provides device level polarity toggle controls.
| D | Adjust array level delay values.
| C | Apply and adjust Array Calibration filters such as Array size compensation and Throw Distance Compensation.
| E | Adjust user EQ filters.