# EQ View

EQ View provides an intuitive interface to access, add, or adjust parametric EQ filters in a devices DSP. Similar to Calibration View, EQ View leverages the Groups Panel to insert EQ filters at various levels within the grouping hierarchy, with the possibilities ranging from all devices in the venue down to a single array. When connected and in-sync, the EQ changes made to the devices are in real-time, if the system is disconnected, the EQ changes will be sent to the devices once they are connected.

## Filter Types

5 EQ filter types are available

Symbol | Filter Type
--- | ---
| High Pass
| Low Shelf
| Bell Filter
| High Shelf
| Low Pass

##

## Apply EQ to Devices

To apply EQ to devices, expand the Groups Panel to expose System Groups or Arrays and select the desired group level to place or adjust an EQ filter. An EQ filter will affect all devices within the selected group. For example, a new filter at the array level will affect only the devices in that specific array and a new filter at the venue level will affect every device in the venue.

With a valid group selected, the workspace will change to display a frequency graph, any EQ filters that are active in the selected Group or any Parent Group above will visibly populate into the graph.

To add a new filter, drag and drop one of the five filter types from the top right into the EQ graph.

The filter gain and center frequency can be adjusted by clicking and dragging the filter to the desired location on the response graph, and filter Q can be adjusted by dragging the handles in or out from the filter apex.

Alternatively, filters can be adjusted manually in the parameter box below the response graph.

## Adjusting or Deleting Existing EQ Filters

To adjust an existing EQ filter, begin by selecting the Group from the Grouping Panel that the filter resides in.

Select the EQ Block above the filter to adjust, the selected block will highlight blue.

Ifa filter is selected that is defined as part of a different group, the filter block will still be visible but will not be selectable. The tool-tip will display the appropriate Grouping Panel selection required for adjustment.

Once a filter has been properly selected, the filter can be adjusted via either method described above in Applying EQ to Devices

## Bypassing EQ Filters

EQ filters can by bypassed individually or at the Group level. Group level EQ filter bypass with disable all filters in a selected Group.

#### Bypass Individual EQ Filters

Select an EQ filter and than toggle the Filter Enable switch underneath the frequency response graph next to the EQ parameter controls.

#### Bypass Group EQ Filters

All filters in a Group can be toggled at the same time by first selecting the Group from the grouping Panel and then toggling the grouped filter EQ Enable switch. This stitch will set the individual filters in the group to all be enabled or disabled.

## Individual Filter Options

With any single filter selected, clicking the button on the EQ parameters bar will expose additional EQ Filter Options

Option | Function
--- | ---
Copy | Copies the selected EQ Filter parameter data.
Paste as New Filter | Creates a new EQ filter with the EQ parameter data in the copy clipboard.
Paste as Filter Values | Replaces the selected EQ filter parameter data with the data from the clipboard.
Reset | Sets selected EQ to default parameter values.
Delete | Completely removes the selected filter from the EQ Group.
Delete All But This | Deletes every other filter in the EQ Group except for the filter selected.

## Group Filter Options

With any EQ Group selected from the Grouping Panel, clicking the button to the right of the New Filter selection will expose group level EQ filter options.

Option | Function
--- | ---
Copy All | Copies all EQ filters in the selected group.
Paste All | Adds all EQ Filters in the clipboard to the selected group.
Reset All | Sets all filters in the selected group to default values.
Delete All | Removes all filters in the selected group.