<Device xml:lang="en-US">
	<NODE>
		<Node Name="VRX900 Passive V5 R1" GroupPath="\VRX900 Passive V5 R1" ClassName="Crown I-Tech HD" ClassID="76" Address="1" Version="1">
			<ProductIndex>0</ProductIndex>
			<VIRTUAL_DEVICE VD_INDEX="0">
				<Object Name="VRX900 Passive V5 R1" Address="0" ClassID="76" Version="1">
					<OBJECT OBJ_CLASSID="8" OBJ_ADDR="67584">
						<Object Name="Analog Inputs" Address="67584" ClassID="8" Version="1">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Input 1 Peak Level Meter" ID="0" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Input 1 RMS Level Meter" ID="1" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="2">
								<StateVariable Name="Input 1 Clip Indicator" ID="2" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Input 1 Fader" ID="3" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>8.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Input 1 Mute Enable" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Input 1 Invert" ID="5" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Input 2 Peak Level Meter" ID="6" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Input 2 RMS Level Meter" ID="7" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Input 2 Clip Indicator" ID="8" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="9">
								<StateVariable Name="Input 2 Fader" ID="9" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>8.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Input 2 Mute Enable" ID="10" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Input 2 Invert" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="High Gain" ID="12" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="13">
								<StateVariable Name="Input 1 Nominal Sensitivity" ID="13" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="14">
								<StateVariable Name="Input 1 Nominal Gain" ID="14" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="15">
								<StateVariable Name="Input 2 Nominal Sensitivity" ID="15" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="16">
								<StateVariable Name="Input 2 Nominal Gain" ID="16" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Report Input 1 Clip Errors" ID="19" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="20">
								<StateVariable Name="Input 1 Clip Error Threshold" ID="20" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="21">
								<StateVariable Name="Input 1 Clip Error Time" ID="21" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Report Input 2 Clip Errors" ID="24" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="25">
								<StateVariable Name="Input 2 Clip Error Threshold" ID="25" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="26">
								<StateVariable Name="Input 2 Clip Error Time" ID="26" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="29">
								<StateVariable Name="Input 1 Post Fader Peak Level Meter" ID="29" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="30">
								<StateVariable Name="Input 1 Post Fader RMS Level Meter" ID="30" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="31">
								<StateVariable Name="Input 2 Post Fader Peak Level Meter" ID="31" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="32">
								<StateVariable Name="Input 2 Post Fader RMS Level Meter" ID="32" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="33">
								<StateVariable Name="Delay FIR Coeff Calculation" ID="33" ClassID="512" Version="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="34">
								<StateVariable Name="Input 1 Detector Threshold" ID="34" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="35">
								<StateVariable Name="Input 2 Detector Threshold" ID="35" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="36">
								<StateVariable Name="Input 1 Detector Hold Time" ID="36" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.03</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="37">
								<StateVariable Name="Input 2 Detector Hold Time" ID="37" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.03</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="38">
								<StateVariable Name="Input 1 Detector Status" ID="38" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="39">
								<StateVariable Name="Input 2 Detector Status" ID="39" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="9" OBJ_ADDR="133376">
						<Object Name="AES Inputs" Address="133376" ClassID="9" Version="1">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Input 1 Peak Level Meter" ID="0" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Input 1 RMS Level Meter" ID="1" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="2">
								<StateVariable Name="Input 1 Clip Indicator" ID="2" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Input 1 Fader" ID="3" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Input 1 Mute Enable" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Input 1 Invert" ID="5" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Input 2 Peak Level Meter" ID="6" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Input 2 RMS Level Meter" ID="7" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Input 2 Clip Indicator" ID="8" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="9">
								<StateVariable Name="Input 2 Fader" ID="9" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Input 2 Mute Enable" ID="10" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Input 2 Invert" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="14">
								<StateVariable Name="Report Input 1 Clip Errors" ID="14" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Input 1 Clip Error Threshold" ID="15" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="16">
								<StateVariable Name="Input 1 Clip Error Time" ID="16" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Report Input 2 Clip Errors" ID="19" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="20">
								<StateVariable Name="Input 2 Clip Error Threshold" ID="20" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="21">
								<StateVariable Name="Input 2 Clip Error Time" ID="21" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="24">
								<StateVariable Name="Status" ID="24" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="25">
								<StateVariable Name="Input 1 Post Fader Peak Level Meter" ID="25" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="26">
								<StateVariable Name="Input 1 Post Fader RMS Level Meter" ID="26" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="27">
								<StateVariable Name="Input 2 Post Fader Peak Level Meter" ID="27" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="28">
								<StateVariable Name="Input 2 Post Fader RMS Level Meter" ID="28" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="29">
								<StateVariable Name="Receive Error" ID="29" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Input 1 Detector Threshold" ID="30" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Input 2 Detector Threshold" ID="31" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Input 1 Detector Hold Time" ID="32" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.02</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Input 2 Detector Hold Time" ID="33" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.02</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="34">
								<StateVariable Name="Input 1 Detector Status" ID="34" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="35">
								<StateVariable Name="Input 2 Detector Status" ID="35" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="10" OBJ_ADDR="199168">
						<Object Name="CobraNet Inputs" Address="199168" ClassID="10" Version="1">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Input 1 Peak Level Meter" ID="0" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Input 1 RMS Level Meter" ID="1" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="2">
								<StateVariable Name="Input 1 Clip Indicator" ID="2" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Input 1 Fader" ID="3" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Input 1 Mute Enable" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Input 1 Invert" ID="5" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Input 2 Peak Level Meter" ID="6" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Input 2 RMS Level Meter" ID="7" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Input 2 Clip Indicator" ID="8" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="9">
								<StateVariable Name="Input 2 Fader" ID="9" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Input 2 Mute Enable" ID="10" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Input 2 Invert" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="14">
								<StateVariable Name="Report Input 1 Clip Errors" ID="14" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Input 1 Clip Error Threshold" ID="15" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="16">
								<StateVariable Name="Input 1 Clip Error Time" ID="16" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Report Input 2 Clip Errors" ID="19" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="20">
								<StateVariable Name="Input 2 Clip Error Threshold" ID="20" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="21">
								<StateVariable Name="Input 2 Clip Error Time" ID="21" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="24">
								<StateVariable Name="Input 1 Status" ID="24" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="25">
								<StateVariable Name="Input 2 Status" ID="25" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="26">
								<StateVariable Name="Input 1 Post Fader Peak Level Meter" ID="26" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="27">
								<StateVariable Name="Input 1 Post Fader RMS Level Meter" ID="27" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="28">
								<StateVariable Name="Input 2 Post Fader Peak Level Meter" ID="28" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="29">
								<StateVariable Name="Input 2 Post Fader RMS Level Meter" ID="29" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Input 1 Detector Threshold" ID="30" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Input 2 Detector Threshold" ID="31" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Input 1 Detector Hold Time" ID="32" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Input 2 Detector Hold Time" ID="33" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="34">
								<StateVariable Name="Input 1 Detector Status" ID="34" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="35">
								<StateVariable Name="Input 2 Detector Status" ID="35" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="6" OBJ_ADDR="263680">
						<Object Name="CobraNet Receive" Address="263680" ClassID="6" Version="1">
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="0">
								<StateVariable Name="RxA Bundle" ID="0" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="1">
								<StateVariable Name="RxA Status" ID="1" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="10">
								<StateVariable Name="RxB Bundle" ID="10" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="11">
								<StateVariable Name="RxB Status" ID="11" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="20">
								<StateVariable Name="RxC Bundle" ID="20" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="21">
								<StateVariable Name="RxC Status" ID="21" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="30">
								<StateVariable Name="RxD Bundle" ID="30" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="31">
								<StateVariable Name="RxD Status" ID="31" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="40">
								<StateVariable Name="Input 1 Label" ID="40" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="26">SQBuAHAAdQB0ACAAMQAgAEwAYQBiAGUAbAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="631" SV_ID="41">
								<StateVariable Name="Input 1" ID="41" ClassID="631" Version="1">
									<Min>0</Min>
									<Max>32</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="42">
								<StateVariable Name="Input 1 Meter" ID="42" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="43">
								<StateVariable Name="Input 2 Label" ID="43" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="26">SQBuAHAAdQB0ACAAMgAgAEwAYQBiAGUAbAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="631" SV_ID="44">
								<StateVariable Name="Input 2" ID="44" ClassID="631" Version="1">
									<Min>0</Min>
									<Max>32</Max>
									<Value>9</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="45">
								<StateVariable Name="Input 2 Meter" ID="45" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="46">
								<StateVariable Name="RxA Sub Format 1" ID="46" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="47">
								<StateVariable Name="RxA Sub Format 2" ID="47" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="48">
								<StateVariable Name="RxA Sub Format 3" ID="48" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="49">
								<StateVariable Name="RxA Sub Format 4" ID="49" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="50">
								<StateVariable Name="RxA Sub Format 5" ID="50" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="51">
								<StateVariable Name="RxA Sub Format 6" ID="51" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="52">
								<StateVariable Name="RxA Sub Format 7" ID="52" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="53">
								<StateVariable Name="RxA Sub Format 8" ID="53" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="54">
								<StateVariable Name="RxB Sub Format 1" ID="54" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="55">
								<StateVariable Name="RxB Sub Format 2" ID="55" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="56">
								<StateVariable Name="RxB Sub Format 3" ID="56" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="57">
								<StateVariable Name="RxB Sub Format 4" ID="57" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="58">
								<StateVariable Name="RxB Sub Format 5" ID="58" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="59">
								<StateVariable Name="RxB Sub Format 6" ID="59" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="60">
								<StateVariable Name="RxB Sub Format 7" ID="60" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="61">
								<StateVariable Name="RxB Sub Format 8" ID="61" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="62">
								<StateVariable Name="RxC Sub Format 1" ID="62" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="63">
								<StateVariable Name="RxC Sub Format 2" ID="63" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="64">
								<StateVariable Name="RxC Sub Format 3" ID="64" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="65">
								<StateVariable Name="RxC Sub Format 4" ID="65" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="66">
								<StateVariable Name="RxC Sub Format 5" ID="66" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="67">
								<StateVariable Name="RxC Sub Format 6" ID="67" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="68">
								<StateVariable Name="RxC Sub Format 7" ID="68" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="69">
								<StateVariable Name="RxC Sub Format 8" ID="69" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="70">
								<StateVariable Name="RxD Sub Format 1" ID="70" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="71">
								<StateVariable Name="RxD Sub Format 2" ID="71" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="72">
								<StateVariable Name="RxD Sub Format 3" ID="72" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="73">
								<StateVariable Name="RxD Sub Format 4" ID="73" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="74">
								<StateVariable Name="RxD Sub Format 5" ID="74" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="75">
								<StateVariable Name="RxD Sub Format 6" ID="75" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="76">
								<StateVariable Name="RxD Sub Format 7" ID="76" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="77">
								<StateVariable Name="RxD Sub Format 8" ID="77" ClassID="630" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="7" OBJ_ADDR="263936">
						<Object Name="CobraNet Transmit" Address="263936" ClassID="7" Version="1">
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="0">
								<StateVariable Name="TxA Bundle" ID="0" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="1">
								<StateVariable Name="TxA Priority" ID="1" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="2">
								<StateVariable Name="TxA Position" ID="2" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="3">
								<StateVariable Name="TxA Channel Receiver Count" ID="3" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="4">
								<StateVariable Name="TxB Bundle" ID="4" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="5">
								<StateVariable Name="TxB Priority" ID="5" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="6">
								<StateVariable Name="TxB Position" ID="6" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="7">
								<StateVariable Name="TxB Channel Receiver Count" ID="7" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="8">
								<StateVariable Name="TxC Bundle" ID="8" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="9">
								<StateVariable Name="TxC Priority" ID="9" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="10">
								<StateVariable Name="TxC Position" ID="10" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="11">
								<StateVariable Name="TxC Channel Receiver Count" ID="11" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="12">
								<StateVariable Name="TxD Bundle" ID="12" ClassID="664" Version="1">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="13">
								<StateVariable Name="TxD Priority" ID="13" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="14">
								<StateVariable Name="TxD Position" ID="14" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="15">
								<StateVariable Name="TxD Channel Receiver Count" ID="15" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="16">
								<StateVariable Name="TxA Slot 1 Switched Output Channel Num" ID="16" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="17">
								<StateVariable Name="TxA Slot 2 Switched Output Channel Num" ID="17" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="18">
								<StateVariable Name="TxA Slot 3 Switched Output Channel Num" ID="18" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="19">
								<StateVariable Name="TxA Slot 4 Switched Output Channel Num" ID="19" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="20">
								<StateVariable Name="TxA Slot 5 Switched Output Channel Num" ID="20" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="21">
								<StateVariable Name="TxA Slot 6 Switched Output Channel Num" ID="21" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="22">
								<StateVariable Name="TxA Slot 7 Switched Output Channel Num" ID="22" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="23">
								<StateVariable Name="TxA Slot 8 Switched Output Channel Num" ID="23" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="24">
								<StateVariable Name="TxB Slot 1 Switched Output Channel Num" ID="24" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="25">
								<StateVariable Name="TxB Slot 2 Switched Output Channel Num" ID="25" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="26">
								<StateVariable Name="TxB Slot 3 Switched Output Channel Num" ID="26" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="27">
								<StateVariable Name="TxB Slot 4 Switched Output Channel Num" ID="27" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="28">
								<StateVariable Name="TxB Slot 5 Switched Output Channel Num" ID="28" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="29">
								<StateVariable Name="TxB Slot 6 Switched Output Channel Num" ID="29" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="30">
								<StateVariable Name="TxB Slot 7 Switched Output Channel Num" ID="30" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="31">
								<StateVariable Name="TxB Slot 8 Switched Output Channel Num" ID="31" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="32">
								<StateVariable Name="TxC Slot 1 Switched Output Channel Num" ID="32" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="33">
								<StateVariable Name="TxC Slot 2 Switched Output Channel Num" ID="33" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="34">
								<StateVariable Name="TxC Slot 3 Switched Output Channel Num" ID="34" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="35">
								<StateVariable Name="TxC Slot 4 Switched Output Channel Num" ID="35" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="36">
								<StateVariable Name="TxC Slot 5 Switched Output Channel Num" ID="36" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="37">
								<StateVariable Name="TxC Slot 6 Switched Output Channel Num" ID="37" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="38">
								<StateVariable Name="TxC Slot 7 Switched Output Channel Num" ID="38" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="39">
								<StateVariable Name="TxC Slot 8 Switched Output Channel Num" ID="39" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="40">
								<StateVariable Name="TxD Slot 1 Switched Output Channel Num" ID="40" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="41">
								<StateVariable Name="TxD Slot 2 Switched Output Channel Num" ID="41" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="42">
								<StateVariable Name="TxD Slot 3 Switched Output Channel Num" ID="42" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="43">
								<StateVariable Name="TxD Slot 4 Switched Output Channel Num" ID="43" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="44">
								<StateVariable Name="TxD Slot 5 Switched Output Channel Num" ID="44" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="45">
								<StateVariable Name="TxD Slot 6 Switched Output Channel Num" ID="45" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="46">
								<StateVariable Name="TxD Slot 7 Switched Output Channel Num" ID="46" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="47">
								<StateVariable Name="TxD Slot 8 Switched Output Channel Num" ID="47" ClassID="738" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="48">
								<StateVariable Name="Output 1 Meter" ID="48" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="49">
								<StateVariable Name="Output 2 Meter" ID="49" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="50">
								<StateVariable Name="Output 3 Meter" ID="50" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="51">
								<StateVariable Name="Output 4 Meter" ID="51" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="12" OBJ_ADDR="330753">
						<Object Name="Ch 1 Input Router" Address="330753" ClassID="12" Version="1">
							<STATE_VARIABLE SV_CLASSID="734" SV_ID="0">
								<StateVariable Name="Mode" ID="0" ClassID="734" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="735" SV_ID="1">
								<StateVariable Name="Analog Source" ID="1" ClassID="735" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="736" SV_ID="2">
								<StateVariable Name="Digital Source" ID="2" ClassID="736" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="748" SV_ID="3">
								<StateVariable Name="AES Source" ID="3" ClassID="748" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="749" SV_ID="4">
								<StateVariable Name="CobraNet Source" ID="4" ClassID="749" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Analog Signal Detector Threshold" ID="5" ClassID="546" Version="1">
									<Min>80</Min>
									<Max>200</Max>
									<Value>140</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Analog Signal Detector Hold Time" ID="6" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>60</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="7">
								<StateVariable Name="Analog Signal Detector Status" ID="7" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Digital Source Status" ID="8" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Mute" ID="9" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="10">
								<StateVariable Name="Fader" ID="10" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Invert" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="12">
								<StateVariable Name="Peak Level Meter" ID="12" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="13">
								<StateVariable Name="RMS Level Meter" ID="13" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="14">
								<StateVariable Name="Clip Indicator" ID="14" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="15">
								<StateVariable Name="Signal Generator Fader" ID="15" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="16">
								<StateVariable Name="Signal Generator Mute" ID="16" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="17">
								<StateVariable Name="Low Priority Input" ID="17" ClassID="787" Version="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="18">
								<StateVariable Name="Medium Priority Input" ID="18" ClassID="787" Version="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="19">
								<StateVariable Name="High Priority Input" ID="19" ClassID="787" Version="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="20">
								<StateVariable Name="Analog Input 1 Fader" ID="20" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="21">
								<StateVariable Name="Analog Input 2 Fader" ID="21" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="22">
								<StateVariable Name="AES Input 1 Fader" ID="22" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="AES Input 2 Fader" ID="23" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="24">
								<StateVariable Name="Cobranet Input 1 Fader" ID="24" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="25">
								<StateVariable Name="Cobranet Input 2 Fader" ID="25" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="26">
								<StateVariable Name="Analog Input 1 Depth Of Cut" ID="26" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="27">
								<StateVariable Name="Analog Input 2 Depth Of Cut" ID="27" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="28">
								<StateVariable Name="AES Input 1 Depth Of Cut" ID="28" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="29">
								<StateVariable Name="AES Input 2 Depth Of Cut" ID="29" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Cobranet Input 1 Depth Of Cut" ID="30" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Cobranet Input 2 Depth Of Cut" ID="31" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Analog Input 1 Attack" ID="32" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Analog Input 2 Attack" ID="33" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="34">
								<StateVariable Name="AES Input 1 Attack" ID="34" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="35">
								<StateVariable Name="AES Input 2 Attack" ID="35" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="36">
								<StateVariable Name="Cobranet Input 1 Attack" ID="36" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="37">
								<StateVariable Name="Cobranet Input 2 Attack" ID="37" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="38">
								<StateVariable Name="Analog Input 1 Release" ID="38" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="39">
								<StateVariable Name="Analog Input 2 Release" ID="39" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="40">
								<StateVariable Name="AES Input 1 Release" ID="40" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="41">
								<StateVariable Name="AES Input 2 Release" ID="41" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="42">
								<StateVariable Name="Cobranet Input 1 Release" ID="42" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="43">
								<StateVariable Name="Cobranet Input 2 Release" ID="43" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="44">
								<StateVariable Name="Analog Input 1 Gain Meter" ID="44" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="45">
								<StateVariable Name="Analog Input 2 Gain Meter" ID="45" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="46">
								<StateVariable Name="AES Input 1 Gain Meter" ID="46" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="47">
								<StateVariable Name="AES Input 2 Gain Meter" ID="47" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="48">
								<StateVariable Name="Cobranet Input 1 Gain Meter" ID="48" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="49">
								<StateVariable Name="Cobranet Input 2 Gain Meter" ID="49" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="788" SV_ID="50">
								<StateVariable Name="Priority Input Status" ID="50" ClassID="788" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="800" SV_ID="51">
								<StateVariable Name="Sum To Mono Detector Mode" ID="51" ClassID="800" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="12" OBJ_ADDR="330754">
						<Object Name="Ch 2 Input Router" Address="330754" ClassID="12" Version="1">
							<STATE_VARIABLE SV_CLASSID="734" SV_ID="0">
								<StateVariable Name="Mode" ID="0" ClassID="734" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="735" SV_ID="1">
								<StateVariable Name="Analog Source" ID="1" ClassID="735" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="736" SV_ID="2">
								<StateVariable Name="Digital Source" ID="2" ClassID="736" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="748" SV_ID="3">
								<StateVariable Name="AES Source" ID="3" ClassID="748" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="749" SV_ID="4">
								<StateVariable Name="CobraNet Source" ID="4" ClassID="749" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Analog Signal Detector Threshold" ID="5" ClassID="546" Version="1">
									<Min>80</Min>
									<Max>200</Max>
									<Value>140</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Analog Signal Detector Hold Time" ID="6" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>60</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="7">
								<StateVariable Name="Analog Signal Detector Status" ID="7" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Digital Source Status" ID="8" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Mute" ID="9" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="10">
								<StateVariable Name="Fader" ID="10" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Invert" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="12">
								<StateVariable Name="Peak Level Meter" ID="12" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="13">
								<StateVariable Name="RMS Level Meter" ID="13" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="14">
								<StateVariable Name="Clip Indicator" ID="14" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="15">
								<StateVariable Name="Signal Generator Fader" ID="15" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="16">
								<StateVariable Name="Signal Generator Mute" ID="16" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="17">
								<StateVariable Name="Low Priority Input" ID="17" ClassID="787" Version="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="18">
								<StateVariable Name="Medium Priority Input" ID="18" ClassID="787" Version="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="19">
								<StateVariable Name="High Priority Input" ID="19" ClassID="787" Version="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="20">
								<StateVariable Name="Analog Input 1 Fader" ID="20" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="21">
								<StateVariable Name="Analog Input 2 Fader" ID="21" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="22">
								<StateVariable Name="AES Input 1 Fader" ID="22" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="AES Input 2 Fader" ID="23" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="24">
								<StateVariable Name="Cobranet Input 1 Fader" ID="24" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="25">
								<StateVariable Name="Cobranet Input 2 Fader" ID="25" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="26">
								<StateVariable Name="Analog Input 1 Depth Of Cut" ID="26" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="27">
								<StateVariable Name="Analog Input 2 Depth Of Cut" ID="27" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="28">
								<StateVariable Name="AES Input 1 Depth Of Cut" ID="28" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="29">
								<StateVariable Name="AES Input 2 Depth Of Cut" ID="29" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Cobranet Input 1 Depth Of Cut" ID="30" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Cobranet Input 2 Depth Of Cut" ID="31" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Analog Input 1 Attack" ID="32" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Analog Input 2 Attack" ID="33" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="34">
								<StateVariable Name="AES Input 1 Attack" ID="34" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="35">
								<StateVariable Name="AES Input 2 Attack" ID="35" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="36">
								<StateVariable Name="Cobranet Input 1 Attack" ID="36" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="37">
								<StateVariable Name="Cobranet Input 2 Attack" ID="37" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="38">
								<StateVariable Name="Analog Input 1 Release" ID="38" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="39">
								<StateVariable Name="Analog Input 2 Release" ID="39" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="40">
								<StateVariable Name="AES Input 1 Release" ID="40" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="41">
								<StateVariable Name="AES Input 2 Release" ID="41" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="42">
								<StateVariable Name="Cobranet Input 1 Release" ID="42" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="43">
								<StateVariable Name="Cobranet Input 2 Release" ID="43" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="44">
								<StateVariable Name="Analog Input 1 Gain Meter" ID="44" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="45">
								<StateVariable Name="Analog Input 2 Gain Meter" ID="45" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="46">
								<StateVariable Name="AES Input 1 Gain Meter" ID="46" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="47">
								<StateVariable Name="AES Input 2 Gain Meter" ID="47" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="48">
								<StateVariable Name="Cobranet Input 1 Gain Meter" ID="48" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="49">
								<StateVariable Name="Cobranet Input 2 Gain Meter" ID="49" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="788" SV_ID="50">
								<StateVariable Name="Priority Input Status" ID="50" ClassID="788" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="800" SV_ID="51">
								<StateVariable Name="Sum To Mono Detector Mode" ID="51" ClassID="800" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="13" OBJ_ADDR="396545">
						<Object Name="Ch 1 Input Compressor" Address="396545" ClassID="13" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" ClassID="733" Version="1">
									<Min>2</Min>
									<Max>32</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>0.1</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>10</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Soft Knee Width" ID="5" ClassID="546" Version="1">
									<Min>200</Min>
									<Max>224</Max>
									<Value>212</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Make Up Gain" ID="7" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>20</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="8">
								<StateVariable Name="Signal Status" ID="8" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="13" OBJ_ADDR="396546">
						<Object Name="Ch 2 Input Compressor" Address="396546" ClassID="13" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" ClassID="733" Version="1">
									<Min>2</Min>
									<Max>32</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>0.1</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" ClassID="733" Version="1">
									<Min>0.01</Min>
									<Max>10</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Soft Knee Width" ID="5" ClassID="546" Version="1">
									<Min>200</Min>
									<Max>224</Max>
									<Value>212</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Make Up Gain" ID="7" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>20</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="8">
								<StateVariable Name="Signal Status" ID="8" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="14" OBJ_ADDR="462337">
						<Object Name="Ch 1 TLC Compressor" Address="462337" ClassID="14" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" ClassID="733" Version="1">
									<Data2 Len="4">AAAAQA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="14" OBJ_ADDR="462338">
						<Object Name="Ch 2 TLC Compressor" Address="462338" ClassID="14" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" ClassID="733" Version="1">
									<Data2 Len="4">AAAAQA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="529409">
						<Object Name="Ch1 Input Delay" Address="529409" ClassID="20" Version="1">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" ClassID="562" Version="1">
									<Min>0</Min>
									<Max>4</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" ClassID="561" Version="1">
									<Min>0</Min>
									<Max>0.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="529410">
						<Object Name="Ch2 Input Delay" Address="529410" ClassID="20" Version="1">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" ClassID="562" Version="1">
									<Min>0</Min>
									<Max>4</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" ClassID="561" Version="1">
									<Min>0</Min>
									<Max>0.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="35" OBJ_ADDR="598785">
						<Object Name="Ch1 Input EQ Filters" Address="598785" ClassID="35" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Enable 9" ID="48" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="49">
								<StateVariable Name="Frequency 9" ID="49" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="50">
								<StateVariable Name="Q 9" ID="50" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="51">
								<StateVariable Name="Slope 9" ID="51" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="52">
								<StateVariable Name="Gain 9" ID="52" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="53">
								<StateVariable Name="Type 9" ID="53" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="54">
								<StateVariable Name="Enable 10" ID="54" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="55">
								<StateVariable Name="Frequency 10" ID="55" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="56">
								<StateVariable Name="Q 10" ID="56" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="57">
								<StateVariable Name="Slope 10" ID="57" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="58">
								<StateVariable Name="Gain 10" ID="58" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="59">
								<StateVariable Name="Type 10" ID="59" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="60">
								<StateVariable Name="Enable 11" ID="60" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="61">
								<StateVariable Name="Frequency 11" ID="61" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="62">
								<StateVariable Name="Q 11" ID="62" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="63">
								<StateVariable Name="Slope 11" ID="63" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="64">
								<StateVariable Name="Gain 11" ID="64" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="65">
								<StateVariable Name="Type 11" ID="65" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="66">
								<StateVariable Name="Enable 12" ID="66" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="67">
								<StateVariable Name="Frequency 12" ID="67" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="68">
								<StateVariable Name="Q 12" ID="68" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="69">
								<StateVariable Name="Slope 12" ID="69" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="70">
								<StateVariable Name="Gain 12" ID="70" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="71">
								<StateVariable Name="Type 12" ID="71" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="72">
								<StateVariable Name="Enable 13" ID="72" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="73">
								<StateVariable Name="Frequency 13" ID="73" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="74">
								<StateVariable Name="Q 13" ID="74" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="75">
								<StateVariable Name="Slope 13" ID="75" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="76">
								<StateVariable Name="Gain 13" ID="76" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="77">
								<StateVariable Name="Type 13" ID="77" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="78">
								<StateVariable Name="Enable 14" ID="78" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="79">
								<StateVariable Name="Frequency 14" ID="79" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="80">
								<StateVariable Name="Q 14" ID="80" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="81">
								<StateVariable Name="Slope 14" ID="81" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="82">
								<StateVariable Name="Gain 14" ID="82" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="83">
								<StateVariable Name="Type 14" ID="83" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="84">
								<StateVariable Name="Enable 15" ID="84" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="85">
								<StateVariable Name="Frequency 15" ID="85" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="86">
								<StateVariable Name="Q 15" ID="86" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="87">
								<StateVariable Name="Slope 15" ID="87" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="88">
								<StateVariable Name="Gain 15" ID="88" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="89">
								<StateVariable Name="Type 15" ID="89" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="90">
								<StateVariable Name="Enable 16" ID="90" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="91">
								<StateVariable Name="Frequency 16" ID="91" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="92">
								<StateVariable Name="Q 16" ID="92" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="93">
								<StateVariable Name="Slope 16" ID="93" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="94">
								<StateVariable Name="Gain 16" ID="94" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="95">
								<StateVariable Name="Type 16" ID="95" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="96">
								<StateVariable Name="Bypass 1 Thru 8" ID="96" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="97">
								<StateVariable Name="Bypass 9 Thru 16" ID="97" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="35" OBJ_ADDR="598786">
						<Object Name="Ch2 Input EQ Filters" Address="598786" ClassID="35" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Enable 9" ID="48" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="49">
								<StateVariable Name="Frequency 9" ID="49" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="50">
								<StateVariable Name="Q 9" ID="50" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="51">
								<StateVariable Name="Slope 9" ID="51" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="52">
								<StateVariable Name="Gain 9" ID="52" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="53">
								<StateVariable Name="Type 9" ID="53" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="54">
								<StateVariable Name="Enable 10" ID="54" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="55">
								<StateVariable Name="Frequency 10" ID="55" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="56">
								<StateVariable Name="Q 10" ID="56" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="57">
								<StateVariable Name="Slope 10" ID="57" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="58">
								<StateVariable Name="Gain 10" ID="58" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="59">
								<StateVariable Name="Type 10" ID="59" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="60">
								<StateVariable Name="Enable 11" ID="60" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="61">
								<StateVariable Name="Frequency 11" ID="61" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="62">
								<StateVariable Name="Q 11" ID="62" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="63">
								<StateVariable Name="Slope 11" ID="63" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="64">
								<StateVariable Name="Gain 11" ID="64" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="65">
								<StateVariable Name="Type 11" ID="65" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="66">
								<StateVariable Name="Enable 12" ID="66" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="67">
								<StateVariable Name="Frequency 12" ID="67" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="68">
								<StateVariable Name="Q 12" ID="68" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="69">
								<StateVariable Name="Slope 12" ID="69" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="70">
								<StateVariable Name="Gain 12" ID="70" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="71">
								<StateVariable Name="Type 12" ID="71" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="72">
								<StateVariable Name="Enable 13" ID="72" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="73">
								<StateVariable Name="Frequency 13" ID="73" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="74">
								<StateVariable Name="Q 13" ID="74" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="75">
								<StateVariable Name="Slope 13" ID="75" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="76">
								<StateVariable Name="Gain 13" ID="76" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="77">
								<StateVariable Name="Type 13" ID="77" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="78">
								<StateVariable Name="Enable 14" ID="78" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="79">
								<StateVariable Name="Frequency 14" ID="79" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="80">
								<StateVariable Name="Q 14" ID="80" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="81">
								<StateVariable Name="Slope 14" ID="81" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="82">
								<StateVariable Name="Gain 14" ID="82" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="83">
								<StateVariable Name="Type 14" ID="83" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="84">
								<StateVariable Name="Enable 15" ID="84" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="85">
								<StateVariable Name="Frequency 15" ID="85" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="86">
								<StateVariable Name="Q 15" ID="86" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="87">
								<StateVariable Name="Slope 15" ID="87" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="88">
								<StateVariable Name="Gain 15" ID="88" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="89">
								<StateVariable Name="Type 15" ID="89" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="90">
								<StateVariable Name="Enable 16" ID="90" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="91">
								<StateVariable Name="Frequency 16" ID="91" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="92">
								<StateVariable Name="Q 16" ID="92" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="93">
								<StateVariable Name="Slope 16" ID="93" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="94">
								<StateVariable Name="Gain 16" ID="94" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="95">
								<StateVariable Name="Type 16" ID="95" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="96">
								<StateVariable Name="Bypass 1 Thru 8" ID="96" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="97">
								<StateVariable Name="Bypass 9 Thru 16" ID="97" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="36" OBJ_ADDR="664577">
						<Object Name="Ch1 IIR Crossover Filters" Address="664577" ClassID="36" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Highpass Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Highpass Frequency" ID="1" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AABwQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="667" SV_ID="2">
								<StateVariable Name="Highpass Type" ID="2" ClassID="667" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="3">
								<StateVariable Name="Highpass Q" ID="3" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="4">
								<StateVariable Name="Highpass Slope" ID="4" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Lowpass Enable" ID="5" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Lowpass Frequency" ID="6" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AECcRg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="666" SV_ID="7">
								<StateVariable Name="Lowpass Type" ID="7" ClassID="666" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Lowpass Q" ID="8" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Lowpass Slope" ID="9" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="36" OBJ_ADDR="664578">
						<Object Name="Ch2 IIR Crossover Filters" Address="664578" ClassID="36" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Highpass Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Highpass Frequency" ID="1" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AABwQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="667" SV_ID="2">
								<StateVariable Name="Highpass Type" ID="2" ClassID="667" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="3">
								<StateVariable Name="Highpass Q" ID="3" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="4">
								<StateVariable Name="Highpass Slope" ID="4" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Lowpass Enable" ID="5" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Lowpass Frequency" ID="6" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AECcRg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="666" SV_ID="7">
								<StateVariable Name="Lowpass Type" ID="7" ClassID="666" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Lowpass Q" ID="8" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Lowpass Slope" ID="9" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="37" OBJ_ADDR="730369">
						<Object Name="Ch1 FIR Filter" Address="730369" ClassID="37" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency" ID="1" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AIA7Rg==</Data3>
									<Data1 Len="4">AAD6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="752" SV_ID="2">
								<StateVariable Name="Mode" ID="2" ClassID="752" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="747" SV_ID="3">
								<StateVariable Name="Coeffs" ID="3" ClassID="747" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">AEA=</Data3>
									<Data1 Len="3592">[encoded data, 4792 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="754" SV_ID="7">
								<StateVariable Name="Latency48KHz" ID="7" ClassID="754" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="755" SV_ID="8">
								<StateVariable Name="Latency96KHz" ID="8" ClassID="755" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="751" SV_ID="9">
								<StateVariable Name="Type" ID="9" ClassID="751" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">Aw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="37" OBJ_ADDR="730370">
						<Object Name="Ch2 FIR Filter" Address="730370" ClassID="37" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency" ID="1" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AIA7Rg==</Data3>
									<Data1 Len="4">AAD6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="752" SV_ID="2">
								<StateVariable Name="Mode" ID="2" ClassID="752" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="747" SV_ID="3">
								<StateVariable Name="Coeffs" ID="3" ClassID="747" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">AEA=</Data3>
									<Data1 Len="3592">[encoded data, 4792 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="754" SV_ID="7">
								<StateVariable Name="Latency48KHz" ID="7" ClassID="754" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="755" SV_ID="8">
								<StateVariable Name="Latency96KHz" ID="8" ClassID="755" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="751" SV_ID="9">
								<StateVariable Name="Type" ID="9" ClassID="751" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">Aw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="34" OBJ_ADDR="795137">
						<Object Name="Ch1 Speaker EQ Filters" Address="795137" ClassID="34" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AACwQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">g8A6QA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACwQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAyQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">xSAIQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AADAPw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB0Qw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">CtcjQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">MzMzPw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AICsQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">fT9dQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">MzOzPw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AADcQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">WDmsQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">mpnZvw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAdRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">CKwcQQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AABAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AEAwRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">HVpUQQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">ZmYmwA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Bypass" ID="48" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="49">
								<StateVariable Name="Enable 9" ID="49" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="50">
								<StateVariable Name="Frequency 9" ID="50" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="51">
								<StateVariable Name="Q 9" ID="51" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="52">
								<StateVariable Name="Slope 9" ID="52" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="53">
								<StateVariable Name="Gain 9" ID="53" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="54">
								<StateVariable Name="Type 9" ID="54" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="55">
								<StateVariable Name="Enable 10" ID="55" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="56">
								<StateVariable Name="Frequency 10" ID="56" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="57">
								<StateVariable Name="Q 10" ID="57" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="58">
								<StateVariable Name="Slope 10" ID="58" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="59">
								<StateVariable Name="Gain 10" ID="59" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="60">
								<StateVariable Name="Type 10" ID="60" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="61">
								<StateVariable Name="Enable 11" ID="61" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="62">
								<StateVariable Name="Frequency 11" ID="62" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="63">
								<StateVariable Name="Q 11" ID="63" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="64">
								<StateVariable Name="Slope 11" ID="64" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="65">
								<StateVariable Name="Gain 11" ID="65" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="66">
								<StateVariable Name="Type 11" ID="66" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="67">
								<StateVariable Name="Enable 12" ID="67" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="68">
								<StateVariable Name="Frequency 12" ID="68" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="69">
								<StateVariable Name="Q 12" ID="69" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="70">
								<StateVariable Name="Slope 12" ID="70" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="71">
								<StateVariable Name="Gain 12" ID="71" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="72">
								<StateVariable Name="Type 12" ID="72" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="34" OBJ_ADDR="795138">
						<Object Name="Ch2 Speaker EQ Filters" Address="795138" ClassID="34" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AACwQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">g8A6QA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACwQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAyQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">xSAIQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AADAPw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB0Qw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">CtcjQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">MzMzPw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AICsQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">fT9dQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">MzOzPw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AADcQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">WDmsQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">mpnZvw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAdRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">CKwcQQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AABAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AEAwRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">HVpUQQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">ZmYmwA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Bypass" ID="48" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="49">
								<StateVariable Name="Enable 9" ID="49" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="50">
								<StateVariable Name="Frequency 9" ID="50" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="51">
								<StateVariable Name="Q 9" ID="51" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="52">
								<StateVariable Name="Slope 9" ID="52" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="53">
								<StateVariable Name="Gain 9" ID="53" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="54">
								<StateVariable Name="Type 9" ID="54" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="55">
								<StateVariable Name="Enable 10" ID="55" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="56">
								<StateVariable Name="Frequency 10" ID="56" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="57">
								<StateVariable Name="Q 10" ID="57" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="58">
								<StateVariable Name="Slope 10" ID="58" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="59">
								<StateVariable Name="Gain 10" ID="59" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="60">
								<StateVariable Name="Type 10" ID="60" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="61">
								<StateVariable Name="Enable 11" ID="61" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="62">
								<StateVariable Name="Frequency 11" ID="62" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="63">
								<StateVariable Name="Q 11" ID="63" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="64">
								<StateVariable Name="Slope 11" ID="64" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="65">
								<StateVariable Name="Gain 11" ID="65" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="66">
								<StateVariable Name="Type 11" ID="66" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="67">
								<StateVariable Name="Enable 12" ID="67" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="68">
								<StateVariable Name="Frequency 12" ID="68" ClassID="587" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="69">
								<StateVariable Name="Q 12" ID="69" ClassID="588" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="70">
								<StateVariable Name="Slope 12" ID="70" ClassID="668" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="71">
								<StateVariable Name="Gain 12" ID="71" ClassID="589" Version="1">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="72">
								<StateVariable Name="Type 12" ID="72" ClassID="665" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="857089">
						<Object Name="Ch1 Speaker Delay" Address="857089" ClassID="20" Version="1">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" ClassID="562" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAQA==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" ClassID="561" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="857090">
						<Object Name="Ch2 Speaker Delay" Address="857090" ClassID="20" Version="1">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" ClassID="562" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAQA==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" ClassID="561" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="15" OBJ_ADDR="921345">
						<Object Name="Ch 1 IOC Limiter" Address="921345" ClassID="15" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="5">
								<StateVariable Name="Status" ID="5" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Gain Meter" ID="6" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="15" OBJ_ADDR="921346">
						<Object Name="Ch 2 IOC Limiter" Address="921346" ClassID="15" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="5">
								<StateVariable Name="Status" ID="5" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Gain Meter" ID="6" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="16" OBJ_ADDR="987137">
						<Object Name="Ch 1 Limiter Suite" Address="987137" ClassID="16" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="757" SV_ID="1">
								<StateVariable Name="Mode" ID="1" ClassID="757" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="16" OBJ_ADDR="987138">
						<Object Name="Ch 2 Limiter Suite" Address="987138" ClassID="16" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="757" SV_ID="1">
								<StateVariable Name="Mode" ID="1" ClassID="757" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="17" OBJ_ADDR="1052929">
						<Object Name="Ch 1 Peak Limiter" Address="1052929" ClassID="17" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" ClassID="806" Version="1">
									<Min>1</Min>
									<Max>201.2</Max>
									<Value>140.9191</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="2">
								<StateVariable Name="Lookahead Delay" ID="2" ClassID="561" Version="1">
									<Min>0</Min>
									<Max>0.01</Max>
									<Value>0.0005</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Release" ID="3" ClassID="733" Version="1">
									<Min>0.0001</Min>
									<Max>10</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Gain Meter" ID="4" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Sidechain EQ Filters Enable 1" ID="5" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Sidechain EQ Filters Frequency 1" ID="6" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="7">
								<StateVariable Name="Sidechain EQ Filters Q 1" ID="7" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="8">
								<StateVariable Name="Sidechain EQ Filters Slope 1" ID="8" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="9">
								<StateVariable Name="Sidechain EQ Filters Gain 1" ID="9" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="10">
								<StateVariable Name="Sidechain EQ Filters Type 1" ID="10" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Sidechain EQ Filters Enable 2" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="12">
								<StateVariable Name="Sidechain EQ Filters Frequency 2" ID="12" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="13">
								<StateVariable Name="Sidechain EQ Filters Q 2" ID="13" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="14">
								<StateVariable Name="Sidechain EQ Filters Slope 2" ID="14" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Sidechain EQ Filters Gain 2" ID="15" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="16">
								<StateVariable Name="Sidechain EQ Filters Type 2" ID="16" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Sidechain EQ Filters Enable 3" ID="17" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="18">
								<StateVariable Name="Sidechain EQ Filters Frequency 3" ID="18" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="19">
								<StateVariable Name="Sidechain EQ Filters Q 3" ID="19" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="20">
								<StateVariable Name="Sidechain EQ Filters Slope 3" ID="20" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="21">
								<StateVariable Name="Sidechain EQ Filters Gain 3" ID="21" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="22">
								<StateVariable Name="Sidechain EQ Filters Type 3" ID="22" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="23">
								<StateVariable Name="Sidechain EQ Filters Bypass" ID="23" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="17" OBJ_ADDR="1052930">
						<Object Name="Ch 2 Peak Limiter" Address="1052930" ClassID="17" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" ClassID="806" Version="1">
									<Min>1</Min>
									<Max>201.2</Max>
									<Value>140.9191</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="2">
								<StateVariable Name="Lookahead Delay" ID="2" ClassID="561" Version="1">
									<Min>0</Min>
									<Max>0.01</Max>
									<Value>0.0005</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Release" ID="3" ClassID="733" Version="1">
									<Min>0.0001</Min>
									<Max>10</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Gain Meter" ID="4" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Sidechain EQ Filters Enable 1" ID="5" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Sidechain EQ Filters Frequency 1" ID="6" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="7">
								<StateVariable Name="Sidechain EQ Filters Q 1" ID="7" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="8">
								<StateVariable Name="Sidechain EQ Filters Slope 1" ID="8" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="9">
								<StateVariable Name="Sidechain EQ Filters Gain 1" ID="9" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="10">
								<StateVariable Name="Sidechain EQ Filters Type 1" ID="10" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Sidechain EQ Filters Enable 2" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="12">
								<StateVariable Name="Sidechain EQ Filters Frequency 2" ID="12" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="13">
								<StateVariable Name="Sidechain EQ Filters Q 2" ID="13" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="14">
								<StateVariable Name="Sidechain EQ Filters Slope 2" ID="14" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Sidechain EQ Filters Gain 2" ID="15" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="16">
								<StateVariable Name="Sidechain EQ Filters Type 2" ID="16" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Sidechain EQ Filters Enable 3" ID="17" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="18">
								<StateVariable Name="Sidechain EQ Filters Frequency 3" ID="18" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="19">
								<StateVariable Name="Sidechain EQ Filters Q 3" ID="19" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="20">
								<StateVariable Name="Sidechain EQ Filters Slope 3" ID="20" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="21">
								<StateVariable Name="Sidechain EQ Filters Gain 3" ID="21" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="22">
								<StateVariable Name="Sidechain EQ Filters Type 3" ID="22" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="23">
								<StateVariable Name="Sidechain EQ Filters Bypass" ID="23" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="18" OBJ_ADDR="1118721">
						<Object Name="Ch 1 RMS Limiter" Address="1118721" ClassID="18" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Detector Time Constant" ID="1" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.002886751</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" ClassID="806" Version="1">
									<Min>1</Min>
									<Max>400</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" ClassID="733" Version="1">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.15</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" ClassID="733" Version="1">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.3138591</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="Gain Meter" ID="5" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="18" OBJ_ADDR="1118722">
						<Object Name="Ch 2 RMS Limiter" Address="1118722" ClassID="18" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Detector Time Constant" ID="1" ClassID="733" Version="1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.002886751</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" ClassID="806" Version="1">
									<Min>1</Min>
									<Max>400</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" ClassID="733" Version="1">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.15</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" ClassID="733" Version="1">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.3138591</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="Gain Meter" ID="5" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="19" OBJ_ADDR="1184513">
						<Object Name="Ch 1 Speaker Thermal Limiter" Address="1184513" ClassID="19" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Time Constant" ID="1" ClassID="733" Version="1">
									<Min>1</Min>
									<Max>600</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" ClassID="806" Version="1">
									<Min>1</Min>
									<Max>500</Max>
									<Value>45.6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Proportional K" ID="3" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.849485</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Integral K" ID="4" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.169897</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Thermal Voltage" ID="5" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="RMS Limiter Threshold Adjust" ID="6" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="7">
								<StateVariable Name="RMS Limiter Threshold Adjust dB" ID="7" ClassID="535" Version="1">
									<Data2 Len="4">AAAgwg==</Data2>
									<Data3 Len="4">AAAAAA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="8">
								<StateVariable Name="Gain Meter" ID="8" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="19" OBJ_ADDR="1184514">
						<Object Name="Ch 2 Speaker Thermal Limiter" Address="1184514" ClassID="19" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Time Constant" ID="1" ClassID="733" Version="1">
									<Min>1</Min>
									<Max>600</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" ClassID="806" Version="1">
									<Min>1</Min>
									<Max>500</Max>
									<Value>45.6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Proportional K" ID="3" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.849485</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Integral K" ID="4" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.169897</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Thermal Voltage" ID="5" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="RMS Limiter Threshold Adjust" ID="6" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="7">
								<StateVariable Name="RMS Limiter Threshold Adjust dB" ID="7" ClassID="535" Version="1">
									<Data2 Len="4">AAAgwg==</Data2>
									<Data3 Len="4">AAAAAA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="8">
								<StateVariable Name="Gain Meter" ID="8" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="21" OBJ_ADDR="1250561">
						<Object Name="Ch 1 Processing Output" Address="1250561" ClassID="21" Version="1">
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="0">
								<StateVariable Name="Fader" ID="0" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="1">
								<StateVariable Name="Invert" ID="1" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Mute Enable" ID="2" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Attenuator Limit" ID="3" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Peak Level Meter" ID="4" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="RMS Level Meter" ID="5" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Clip Indicator" ID="6" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Gain Meter" ID="7" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Report Clip Errors" ID="10" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="11">
								<StateVariable Name="Clip Error Threshold" ID="11" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="12">
								<StateVariable Name="Clip Error Time" ID="12" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Band Gain" ID="15" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="16">
								<StateVariable Name="Highpass Family" ID="16" ClassID="753" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="17">
								<StateVariable Name="Lowpass Family" ID="17" ClassID="753" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="21" OBJ_ADDR="1250562">
						<Object Name="Ch 2 Processing Output" Address="1250562" ClassID="21" Version="1">
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="0">
								<StateVariable Name="Fader" ID="0" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="1">
								<StateVariable Name="Invert" ID="1" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Mute Enable" ID="2" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Attenuator Limit" ID="3" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Peak Level Meter" ID="4" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="RMS Level Meter" ID="5" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Clip Indicator" ID="6" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Gain Meter" ID="7" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Report Clip Errors" ID="10" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="11">
								<StateVariable Name="Clip Error Threshold" ID="11" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="12">
								<StateVariable Name="Clip Error Time" ID="12" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Band Gain" ID="15" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="16">
								<StateVariable Name="Highpass Family" ID="16" ClassID="753" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="17">
								<StateVariable Name="Lowpass Family" ID="17" ClassID="753" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="22" OBJ_ADDR="1316353">
						<Object Name="Ch 1 Amp Output" Address="1316353" ClassID="22" Version="1">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Current Peak Level Meter" ID="0" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Current RMS Level Meter" ID="1" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="2">
								<StateVariable Name="Voltage Peak Level Meter" ID="2" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="3">
								<StateVariable Name="Voltage RMS Level Meter" ID="3" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Enable" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Temperature" ID="5" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Sleeping" ID="6" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="8">
								<StateVariable Name="Temperature Deg C" ID="8" ClassID="535" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Report Thermal Errors" ID="9" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="10">
								<StateVariable Name="Thermal Error Threshold" ID="10" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>100</Max>
									<Value>70</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="13">
								<StateVariable Name="Report Clip Errors" ID="13" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="14">
								<StateVariable Name="Clip Error Threshold" ID="14" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Clip Error Time" ID="15" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="18">
								<StateVariable Name="RMS Amp Meter" ID="18" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="19">
								<StateVariable Name="RMS Volt Meter" ID="19" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="20">
								<StateVariable Name="Peak Amp Meter" ID="20" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="21">
								<StateVariable Name="Peak Volt Meter" ID="21" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="22">
								<StateVariable Name="Auto Standby Turn Off Delay" ID="22" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="Auto Standby Threshold" ID="23" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="22" OBJ_ADDR="1316354">
						<Object Name="Ch 2 Amp Output" Address="1316354" ClassID="22" Version="1">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Current Peak Level Meter" ID="0" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Current RMS Level Meter" ID="1" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="2">
								<StateVariable Name="Voltage Peak Level Meter" ID="2" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="3">
								<StateVariable Name="Voltage RMS Level Meter" ID="3" ClassID="646" Version="1">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Enable" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Temperature" ID="5" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Sleeping" ID="6" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="8">
								<StateVariable Name="Temperature Deg C" ID="8" ClassID="535" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Report Thermal Errors" ID="9" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="10">
								<StateVariable Name="Thermal Error Threshold" ID="10" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>100</Max>
									<Value>70</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="13">
								<StateVariable Name="Report Clip Errors" ID="13" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="14">
								<StateVariable Name="Clip Error Threshold" ID="14" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Clip Error Time" ID="15" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="18">
								<StateVariable Name="RMS Amp Meter" ID="18" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="19">
								<StateVariable Name="RMS Volt Meter" ID="19" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="20">
								<StateVariable Name="Peak Amp Meter" ID="20" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="21">
								<StateVariable Name="Peak Volt Meter" ID="21" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="22">
								<StateVariable Name="Auto Standby Turn Off Delay" ID="22" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="Auto Standby Threshold" ID="23" ClassID="546" Version="1">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="25" OBJ_ADDR="1382657">
						<Object Name="Ch 1 Load Supervision" Address="1382657" ClassID="25" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Low Limit" ID="1" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>250</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="High Limit" ID="2" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>250</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="3">
								<StateVariable Name="Testing" ID="3" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="585" SV_ID="4">
								<StateVariable Name="Status" ID="4" ClassID="585" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="Nominal Load Impedance" ID="5" ClassID="733" Version="1">
									<Min>1</Min>
									<Max>250</Max>
									<Value>8</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="Average Impedance" ID="6" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAB6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Report Errors" ID="7" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="25" OBJ_ADDR="1382658">
						<Object Name="Ch 2 Load Supervision" Address="1382658" ClassID="25" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Low Limit" ID="1" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>250</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="High Limit" ID="2" ClassID="733" Version="1">
									<Min>0</Min>
									<Max>250</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="3">
								<StateVariable Name="Testing" ID="3" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="585" SV_ID="4">
								<StateVariable Name="Status" ID="4" ClassID="585" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="Nominal Load Impedance" ID="5" ClassID="733" Version="1">
									<Min>1</Min>
									<Max>250</Max>
									<Value>8</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="Average Impedance" ID="6" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAB6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Report Errors" ID="7" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="26" OBJ_ADDR="1448449">
						<Object Name="Ch 1 Sweep Load Monitoring" Address="1448449" ClassID="26" Version="1">
							<STATE_VARIABLE SV_CLASSID="622" SV_ID="0">
								<StateVariable Name="Acquire Mode" ID="0" ClassID="622" Version="1">
									<Min>0</Min>
									<Max>5</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Start Freq" ID="1" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="2">
								<StateVariable Name="Stop Freq" ID="2" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="3">
								<StateVariable Name="Impedance Reference" ID="3" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="4">
								<StateVariable Name="Impedance Response" ID="4" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="5">
								<StateVariable Name="Frequency Reference" ID="5" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="6">
								<StateVariable Name="Frequency Response" ID="6" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="7">
								<StateVariable Name="Impedance PassFail" ID="7" ClassID="625" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="8">
								<StateVariable Name="Freq Resp PassFail" ID="8" ClassID="625" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="649" SV_ID="9">
								<StateVariable Name="Curve Notes" ID="9" ClassID="649" Version="1">
									<Min>0</Min>
									<Max>514</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="26" OBJ_ADDR="1448450">
						<Object Name="Ch 2 Sweep Load Monitoring" Address="1448450" ClassID="26" Version="1">
							<STATE_VARIABLE SV_CLASSID="622" SV_ID="0">
								<StateVariable Name="Acquire Mode" ID="0" ClassID="622" Version="1">
									<Min>0</Min>
									<Max>5</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Start Freq" ID="1" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="2">
								<StateVariable Name="Stop Freq" ID="2" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="3">
								<StateVariable Name="Impedance Reference" ID="3" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="4">
								<StateVariable Name="Impedance Response" ID="4" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="5">
								<StateVariable Name="Frequency Reference" ID="5" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="6">
								<StateVariable Name="Frequency Response" ID="6" ClassID="648" Version="1">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="7">
								<StateVariable Name="Impedance PassFail" ID="7" ClassID="625" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="8">
								<StateVariable Name="Freq Resp PassFail" ID="8" ClassID="625" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="649" SV_ID="9">
								<StateVariable Name="Curve Notes" ID="9" ClassID="649" Version="1">
									<Min>0</Min>
									<Max>514</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="27" OBJ_ADDR="1448704">
						<Object Name="Common Sweep Load Monitoring" Address="1448704" ClassID="27" Version="1">
							<STATE_VARIABLE SV_CLASSID="623" SV_ID="0">
								<StateVariable Name="Sweep Resolution" ID="0" ClassID="623" Version="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Sweep Start Freq" ID="1" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="2">
								<StateVariable Name="Sweep Stop Freq" ID="2" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="3">
								<StateVariable Name="Test in progress" ID="3" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Report Slm Errors" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="550" SV_ID="5">
								<StateVariable Name="Impedance Test Tolerance" ID="5" ClassID="550" Version="1">
									<Min>10</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="624" SV_ID="6">
								<StateVariable Name="Frequency Response Test Tolerance" ID="6" ClassID="624" Version="1">
									<Min>3</Min>
									<Max>25</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Start Sweep" ID="7" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="8">
								<StateVariable Name="Abort Sweep" ID="8" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="11" OBJ_ADDR="1510144">
						<Object Name="Signal Generator" Address="1510144" ClassID="11" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="737" SV_ID="1">
								<StateVariable Name="Mode" ID="1" ClassID="737" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="2">
								<StateVariable Name="Master Gain" ID="2" ClassID="546" Version="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="3">
								<StateVariable Name="Frequency" ID="3" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="33" OBJ_ADDR="1581312">
						<Object Name="Signal Generator EQ Filters" Address="1581312" ClassID="33" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" ClassID="587" Version="1">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" ClassID="588" Version="1">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" ClassID="668" Version="1">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" ClassID="589" Version="1">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" ClassID="665" Version="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="31" OBJ_ADDR="1646336">
						<Object Name="Error Reporting" Address="1646336" ClassID="31" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Report Line Voltage Errors" ID="0" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Low Line Voltage Error Threshold" ID="1" ClassID="733" Version="1">
									<Min>85</Min>
									<Max>277</Max>
									<Value>90</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="High Line Voltage Error Threshold" ID="2" ClassID="733" Version="1">
									<Min>85</Min>
									<Max>277</Max>
									<Value>265</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Report Power Supply Thermal Errors" ID="7" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="8">
								<StateVariable Name="Power Supply Thermal Error Threshold" ID="8" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>100</Max>
									<Value>70</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Report Fan Errors" ID="11" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="15">
								<StateVariable Name="Amp Output Clip Log Display Control" ID="15" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="16">
								<StateVariable Name="Analog Input Clip Log Display Control" ID="16" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Amp Output Thermal Log Display Control" ID="17" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Load Supervision Low Log Display Control" ID="18" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Load Supervision High Log Display Control" ID="19" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="20">
								<StateVariable Name="Slm Log Display Control" ID="20" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="21">
								<StateVariable Name="Line Voltage Log Display Control" ID="21" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="22">
								<StateVariable Name="Fan Log Display Control" ID="22" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="23">
								<StateVariable Name="Clear All Log Display Control" ID="23" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Report Source Change via Network" ID="24" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="0" OBJ_ADDR="1703936">
						<Object Name="Amp Global" Address="1703936" ClassID="0" Version="1">
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="0">
								<StateVariable Name="Model" ID="0" ClassID="616" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="740" SV_ID="1">
								<StateVariable Name="Mode" ID="1" ClassID="740" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Compressor Tie" ID="2" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Limiter Tie" ID="3" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Attenuator Link" ID="4" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="FF Voltage Scale Factor" ID="5" ClassID="733" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="515" SV_ID="9">
								<StateVariable Name="Front Panel Lockout" ID="9" ClassID="515" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Display Led Type" ID="12" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="743" SV_ID="13">
								<StateVariable Name="Display Bar Meter Type" ID="13" ClassID="743" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Locate" ID="17" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="689" SV_ID="18">
								<StateVariable Name="Front Panel Blackout" ID="18" ClassID="689" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Usb Lockout" ID="19" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="746" SV_ID="21">
								<StateVariable Name="Fixed Gain Mode" ID="21" ClassID="746" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="22">
								<StateVariable Name="InternalPassword" ID="22" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">EgA=</Data3>
									<Data1 Len="16">YQB1ADYAYgBhAHQAZAB4AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="23">
								<StateVariable Name="Usb Overcurrent" ID="23" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="24">
								<StateVariable Name="Usb Device Detected" ID="24" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="756" SV_ID="25">
								<StateVariable Name="Disable Protocol" ID="25" ClassID="756" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="26">
								<StateVariable Name="Hiqnet Address Display Control" ID="26" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="27">
								<StateVariable Name="DHCP Display Control" ID="27" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="28">
								<StateVariable Name="IP Address Display Control" ID="28" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="29">
								<StateVariable Name="Subnet Mask Display Control" ID="29" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Preset Recall Display Control" ID="30" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="31">
								<StateVariable Name="Delay FIR Coeff Calculation" ID="31" ClassID="512" Version="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="32">
								<StateVariable Name="Front Panel Display Home Screen" ID="32" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="794" SV_ID="33">
								<StateVariable Name="VRACKPrimaryInput" ID="33" ClassID="794" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Dw==</Data3>
									<Data1 Len="1">CQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="794" SV_ID="34">
								<StateVariable Name="VRACKSecondaryInput" ID="34" ClassID="794" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Dw==</Data3>
									<Data1 Len="1">Ag==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="795" SV_ID="35">
								<StateVariable Name="VRACKOutputConfig" ID="35" ClassID="795" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">DA==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="36">
								<StateVariable Name="Restore All SVs To Default" ID="36" ClassID="616" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="1" OBJ_ADDR="1704192">
						<Object Name="Amp Info" Address="1704192" ClassID="1" Version="1">
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="0">
								<StateVariable Name="User Label 1" ID="0" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="1">
								<StateVariable Name="User Label 2" ID="1" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="2">
								<StateVariable Name="Date Code" ID="2" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="4">
								<StateVariable Name="Model" ID="4" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="5">
								<StateVariable Name="Serial Number" ID="5" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Data LED" ID="6" ClassID="512" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="7">
								<StateVariable Name="Firmware Version Timestamp" ID="7" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="12">
								<StateVariable Name="Operating Time" ID="12" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="13">
								<StateVariable Name="Display Firmware Version String" ID="13" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="14">
								<StateVariable Name="Firmware Version String" ID="14" ClassID="517" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="2" OBJ_ADDR="1704448">
						<Object Name="Miscellaneous" Address="1704448" ClassID="2" Version="1">
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="0">
								<StateVariable Name="DSP Crunch CPU Utilization" ID="0" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="1">
								<StateVariable Name="DSP Process CPU Utilization" ID="1" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="2">
								<StateVariable Name="DSP Workload" ID="2" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="3">
								<StateVariable Name="DSP Warped Workload" ID="3" ClassID="533" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="3" OBJ_ADDR="1704704">
						<Object Name="CobraNet General" Address="1704704" ClassID="3" Version="1">
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="0">
								<StateVariable Name="System Name" ID="0" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>System Name</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="758" SV_ID="1">
								<StateVariable Name="System Description" ID="1" ClassID="758" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">gAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="2">
								<StateVariable Name="System Location" ID="2" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>System Location</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="3">
								<StateVariable Name="System Contact" ID="3" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>System Contact</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="4">
								<StateVariable Name="Firmware Protocol Version" ID="4" ClassID="609" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="5">
								<StateVariable Name="Firmware Major Version" ID="5" ClassID="609" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="6">
								<StateVariable Name="Firmware Minor Version" ID="6" ClassID="609" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="628" SV_ID="7">
								<StateVariable Name="Error Indicators" ID="7" ClassID="628" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">DQAHAA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Conductor Indicator" ID="8" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="9">
								<StateVariable Name="Conductor Priority" ID="9" ClassID="616" Version="1">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="629" SV_ID="10">
								<StateVariable Name="Ethernet Status" ID="10" ClassID="629" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="11">
								<StateVariable Name="Ethernet Rx Activity" ID="11" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="12">
								<StateVariable Name="Ethernet Tx Activity" ID="12" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="684" SV_ID="13">
								<StateVariable Name="Static IP Address" ID="13" ClassID="684" Version="1">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="684" SV_ID="14">
								<StateVariable Name="IP Address" ID="14" ClassID="684" Version="1">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="654" SV_ID="15">
								<StateVariable Name="MAC Address" ID="15" ClassID="654" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">JAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="656" SV_ID="16">
								<StateVariable Name="Sample Rate" ID="16" ClassID="656" Version="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="655" SV_ID="17">
								<StateVariable Name="Latency" ID="17" ClassID="655" Version="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="19">
								<StateVariable Name="TxA Slot 1 Bit Resolution" ID="19" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="20">
								<StateVariable Name="TxA Slot 2 Bit Resolution" ID="20" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="21">
								<StateVariable Name="TxA Slot 3 Bit Resolution" ID="21" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="22">
								<StateVariable Name="TxA Slot 4 Bit Resolution" ID="22" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="23">
								<StateVariable Name="TxA Slot 5 Bit Resolution" ID="23" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="24">
								<StateVariable Name="TxA Slot 6 Bit Resolution" ID="24" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="25">
								<StateVariable Name="TxA Slot 7 Bit Resolution" ID="25" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="26">
								<StateVariable Name="TxA Slot 8 Bit Resolution" ID="26" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="27">
								<StateVariable Name="TxB Slot 1 Bit Resolution" ID="27" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="28">
								<StateVariable Name="TxB Slot 2 Bit Resolution" ID="28" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="29">
								<StateVariable Name="TxB Slot 3 Bit Resolution" ID="29" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="30">
								<StateVariable Name="TxB Slot 4 Bit Resolution" ID="30" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="31">
								<StateVariable Name="TxB Slot 5 Bit Resolution" ID="31" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="32">
								<StateVariable Name="TxB Slot 6 Bit Resolution" ID="32" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="33">
								<StateVariable Name="TxB Slot 7 Bit Resolution" ID="33" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="34">
								<StateVariable Name="TxB Slot 8 Bit Resolution" ID="34" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="35">
								<StateVariable Name="TxC Slot 1 Bit Resolution" ID="35" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="36">
								<StateVariable Name="TxC Slot 2 Bit Resolution" ID="36" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="37">
								<StateVariable Name="TxC Slot 3 Bit Resolution" ID="37" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="38">
								<StateVariable Name="TxC Slot 4 Bit Resolution" ID="38" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="39">
								<StateVariable Name="TxC Slot 5 Bit Resolution" ID="39" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="40">
								<StateVariable Name="TxC Slot 6 Bit Resolution" ID="40" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="41">
								<StateVariable Name="TxC Slot 7 Bit Resolution" ID="41" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="42">
								<StateVariable Name="TxC Slot 8 Bit Resolution" ID="42" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="43">
								<StateVariable Name="TxD Slot 1 Bit Resolution" ID="43" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="44">
								<StateVariable Name="TxD Slot 2 Bit Resolution" ID="44" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="45">
								<StateVariable Name="TxD Slot 3 Bit Resolution" ID="45" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="46">
								<StateVariable Name="TxD Slot 4 Bit Resolution" ID="46" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="47">
								<StateVariable Name="TxD Slot 5 Bit Resolution" ID="47" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="48">
								<StateVariable Name="TxD Slot 6 Bit Resolution" ID="48" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="49">
								<StateVariable Name="TxD Slot 7 Bit Resolution" ID="49" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="50">
								<StateVariable Name="TxD Slot 8 Bit Resolution" ID="50" ClassID="626" Version="1">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="52">
								<StateVariable Name="TxA Max Packet Size Reached" ID="52" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="53">
								<StateVariable Name="TxB Max Packet Size Reached" ID="53" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="54">
								<StateVariable Name="TxC Max Packet Size Reached" ID="54" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="55">
								<StateVariable Name="TxD Max Packet Size Reached" ID="55" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="4" OBJ_ADDR="1704960">
						<Object Name="Presets" Address="1704960" ClassID="4" Version="1">
							<STATE_VARIABLE SV_CLASSID="747" SV_ID="0">
								<StateVariable Name="Preset Colors" ID="0" ClassID="747" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">MgA=</Data3>
									<Data1 Len="50">AAICAgAAAAECAgIAAAABAgICAAAAAQQEBgYBBAQEBAQEBgYGBgYGAQEBAQEBAQEBAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="1">
								<StateVariable Name="Preset Valid" ID="1" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="2">
								<StateVariable Name="Current Preset" ID="2" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>50</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="635" SV_ID="3">
								<StateVariable Name="Store Preset" ID="3" ClassID="635" Version="1">
									<Data2 Len="1">Ag==</Data2>
									<Data3 Len="1">Mg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="635" SV_ID="4">
								<StateVariable Name="Recall Preset" ID="4" ClassID="635" Version="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">Mg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="5">
								<StateVariable Name="Current Preset Name" ID="5" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="6">
								<StateVariable Name="Preset 1 Blob" ID="6" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="7">
								<StateVariable Name="Preset 1 Name" ID="7" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Default</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="8">
								<StateVariable Name="Preset 2 Blob" ID="8" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8665">[encoded data, 11556 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="9">
								<StateVariable Name="Preset 2 Name" ID="9" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="10">
								<StateVariable Name="Preset 3 Blob" ID="10" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8687">[encoded data, 11584 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="11">
								<StateVariable Name="Preset 3 Name" ID="11" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 2x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="12">
								<StateVariable Name="Preset 4 Blob" ID="12" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8687">[encoded data, 11584 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="13">
								<StateVariable Name="Preset 4 Name" ID="13" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 3x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="14">
								<StateVariable Name="Preset 5 Blob" ID="14" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8755">[encoded data, 11676 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="15">
								<StateVariable Name="Preset 5 Name" ID="15" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 1x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="16">
								<StateVariable Name="Preset 6 Blob" ID="16" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8695">[encoded data, 11596 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="17">
								<StateVariable Name="Preset 6 Name" ID="17" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 2x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="18">
								<StateVariable Name="Preset 7 Blob" ID="18" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8777">[encoded data, 11704 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="19">
								<StateVariable Name="Preset 7 Name" ID="19" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 3x Passive ST</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="20">
								<StateVariable Name="Preset 8 Blob" ID="20" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="21">
								<StateVariable Name="Preset 8 Name" ID="21" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 8</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="22">
								<StateVariable Name="Preset 9 Blob" ID="22" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8741">[encoded data, 11656 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="23">
								<StateVariable Name="Preset 9 Name" ID="23" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x Passive LT</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="24">
								<StateVariable Name="Preset 10 Blob" ID="24" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8763">[encoded data, 11684 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="25">
								<StateVariable Name="Preset 10 Name" ID="25" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 2x Passive LT</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="26">
								<StateVariable Name="Preset 11 Blob" ID="26" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8763">[encoded data, 11684 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="27">
								<StateVariable Name="Preset 11 Name" ID="27" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 3x Passive LT</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="28">
								<StateVariable Name="Preset 12 Blob" ID="28" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8831">[encoded data, 11776 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="29">
								<StateVariable Name="Preset 12 Name" ID="29" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 1x Passive LT</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="30">
								<StateVariable Name="Preset 13 Blob" ID="30" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8771">[encoded data, 11696 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="31">
								<StateVariable Name="Preset 13 Name" ID="31" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 2x Passive LT</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="32">
								<StateVariable Name="Preset 14 Blob" ID="32" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8853">[encoded data, 11804 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="33">
								<StateVariable Name="Preset 14 Name" ID="33" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 3x Passive LT</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="34">
								<StateVariable Name="Preset 15 Blob" ID="34" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="35">
								<StateVariable Name="Preset 15 Name" ID="35" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 15</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="36">
								<StateVariable Name="Preset 16 Blob" ID="36" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8677">[encoded data, 11572 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="37">
								<StateVariable Name="Preset 16 Name" ID="37" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x Passive LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="38">
								<StateVariable Name="Preset 17 Blob" ID="38" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8699">[encoded data, 11600 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="39">
								<StateVariable Name="Preset 17 Name" ID="39" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 2x Passive LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="40">
								<StateVariable Name="Preset 18 Blob" ID="40" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8759">[encoded data, 11680 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="41">
								<StateVariable Name="Preset 18 Name" ID="41" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 3x Passive LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="42">
								<StateVariable Name="Preset 19 Blob" ID="42" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8685">[encoded data, 11580 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="43">
								<StateVariable Name="Preset 19 Name" ID="43" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 1x Passive LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="44">
								<StateVariable Name="Preset 20 Blob" ID="44" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8625">[encoded data, 11500 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="45">
								<StateVariable Name="Preset 20 Name" ID="45" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 2x Passive LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="46">
								<StateVariable Name="Preset 21 Blob" ID="46" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="8789">[encoded data, 11720 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="47">
								<StateVariable Name="Preset 21 Name" ID="47" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 3x Passive LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="48">
								<StateVariable Name="Preset 22 Blob" ID="48" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="49">
								<StateVariable Name="Preset 22 Name" ID="49" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 22</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="50">
								<StateVariable Name="Preset 23 Blob" ID="50" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="1255">AEwAAQgAAAMGAAAAAAABCAAACQYAAAAAAAEIAAAMAQAABQwBAA8ByAAFDAIADwHIAAUMAgASAQEABQwCABMBBAAJIwEAAAEBAAkjAQAGAQEACSMBAAwBAQAJIwEAEgEBAAkjAQAYAQEACSMBAB4BAQAJIwEAJAEBAAkjAQAqAQEACSMBADABAQAJIwEANgEBAAkjAQA8AQEACSMBAEIBAQAJIwEASAEBAAkjAQBOAQEACSMBAFQBAQAJIwEAWgEBAAkjAgAAAQEACSMCAAYBAQAJIwIADAEBAAkjAgASAQEACSMCABgBAQAJIwIAHgEBAAkjAgAkAQEACSMCACoBAQAJIwIAMAEBAAkjAgA2AQEACSMCADwBAQAJIwIAQgEBAAkjAgBIAQEACSMCAE4BAQAJIwIAVAEBAAkjAgBaAQEACiQBAAABAQAKJAEAAQZB8AAAAAokAQAFAQEACiQBAAYGQqAAAAAKJAIAAAEBAAokAgABBkHwAAAACiQCAAUBAQAKJAIABgZCoAAAAAwiAQAAAQEADCIBAAEGQkAAAAAMIgEAAgY/49cKAAwiAQAEBkDGZmYADCIBAAYBAQAMIgEABwZCrgAAAAwiAQAIBkBwAAAADCIBAAoGQEZmZgAMIgEADAEBAAwiAQANBkKKAAAADCIBAA4GQIgAAAAMIgEAEAY/szMzAAwiAQASAQEADCIBABMGQnAAAAAMIgEAFAY9zMzNAAwiAQAWBsAAAAAADCICAAABAQAMIgIAAQZCQAAAAAwiAgACBj/j1woADCICAAQGQMZmZgAMIgIABgEBAAwiAgAHBkKuAAAADCICAAgGQHAAAAAMIgIACgZARmZmAAwiAgAMAQEADCICAA0GQooAAAAMIgIADgZAiAAAAAwiAgAQBj+zMzMADCICABIBAQAMIgIAEwZCcAAAAAwiAgAUBj3MzM0ADCICABYGwAAAAAANFAEAAQY7raufAA0UAgABBjutq58ADxABAAABAQAPEAEAAQECAA8QAgAAAQEADxACAAEBAgAQEQEAAAEBABARAQABBkLHhrgAEBEBAAMGPkzMzQAQEQIAAAEBABARAgABBkLHhrgAEBECAAMGPkzMzQAREgEAAAEBABESAQABBjynN+8AERIBAAIGQkgAAAAREgEAAwY+mZmaABESAQAEBj8bONMAERICAAABAQAREgIAAQY8pzfvABESAgACBkJIAAAAERICAAMGPpmZmgAREgIABAY/GzjTABITAQAAAQEAEhMBAAEGQOAAAAASEwEAAgZCPZmaABITAQADBj9sLCwAEhMBAAQGPgb0qwASEwIAAAEBABITAgABBkDgAAAAEhMCAAIGQj2ZmgASEwIAAwY/bCwsABITAgAEBj4G9KsAExUBAAAByAATFQEADwZBIAAAABMVAQAQAQEAExUBABEBAQATFQIAAAHIABMVAgAPBkEgAAAAExUCABABAQATFQIAEQEBABUZAQAAAQEAFRkBAAUGQIAAAAAVGQIAAAEBABUZAgAFBkCAAAAAFwsAAAEBAQAaAAAAFQEBABoAAAAWCQASAGEAdQA2AGIAYQB0AGQAeAAAABoAAAAZAQEAGgEAAAAJABAAVgBSAFgAOQAxADUAUwAAABoBAAABCQAQAFYAUgBYADkAMQA1AFMAAA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="51">
								<StateVariable Name="Preset 23 Name" ID="51" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX915S / VRX915S 928LA LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="52">
								<StateVariable Name="Preset 24 Blob" ID="52" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="1375">AEwAAQgAAAMGAAAAAAABCAAACQYAAAAAAAEIAAAMAQAABQwBAA8ByAAFDAIADwHIAAUMAgASAQEABQwCABMBBAAJIwEAAAEBAAkjAQAGAQEACSMBAAwBAQAJIwEAEgEBAAkjAQAYAQEACSMBAB4BAQAJIwEAJAEBAAkjAQAqAQEACSMBADABAQAJIwEANgEBAAkjAQA8AQEACSMBAEIBAQAJIwEASAEBAAkjAQBOAQEACSMBAFQBAQAJIwEAWgEBAAkjAgAAAQEACSMCAAYBAQAJIwIADAEBAAkjAgASAQEACSMCABgBAQAJIwIAHgEBAAkjAgAkAQEACSMCACoBAQAJIwIAMAEBAAkjAgA2AQEACSMCADwBAQAJIwIAQgEBAAkjAgBIAQEACSMCAE4BAQAJIwIAVAEBAAkjAgBaAQEACiQBAAABAQAKJAEAAQZB8AAAAAokAQAFAQEACiQBAAYGQqAAAAAKJAIAAAEBAAokAgABBkHwAAAACiQCAAUBAQAKJAIABgZCoAAAAAwiAQAAAQEADCIBAAEGQlAAAAAMIgEAAgZAOZmaAAwiAQAEBkB5mZoADCIBAAYBAQAMIgEABwZDIQAAAAwiAQAIBkAAo9cADCIBAAoGP8zMzQAMIgEADAEBAAwiAQANBkKiAAAADCIBAA4GQBFHrgAMIgEAEAZAoAAAAAwiAQASAQEADCIBABMGQoIAAAAMIgEAFgY/TMzNAAwiAQAYAQEADCIBABkGQjQAAAAMIgEAGgZAsAAAAAwiAQAcBkAAAAAADCIBAB4BAQAMIgEAHwZCcAAAAAwiAQAgBj3MzM0ADCIBACIGwAAAAAAMIgIAAAEBAAwiAgABBkJQAAAADCICAAIGQDmZmgAMIgIABAZAeZmaAAwiAgAGAQEADCICAAcGQyEAAAAMIgIACAZAAKPXAAwiAgAKBj/MzM0ADCICAAwBAQAMIgIADQZCogAAAAwiAgAOBkARR64ADCICABAGQKAAAAAMIgIAEgEBAAwiAgATBkKCAAAADCICABYGP0zMzQAMIgIAGAEBAAwiAgAZBkI0AAAADCICABoGQLAAAAAMIgIAHAZAAAAAAAwiAgAeAQEADCICAB8GQnAAAAAMIgIAIAY9zMzNAAwiAgAiBsAAAAAADRQBAAEGO62rnwANFAIAAQY7raufAA8QAQAAAQEADxABAAEBAgAPEAIAAAEBAA8QAgABAQIAEBEBAAABAQAQEQEAAQZC72ZmABARAQADBj5MzM0AEBECAAABAQAQEQIAAQZC72ZmABARAgADBj5MzM0AERIBAAABAQAREgEAAQY8pzfvABESAQACBkJwAAAAERIBAAMGPpmZmgAREgEABAY/GzjTABESAgAAAQEAERICAAEGPKc37QAREgIAAgZCcAAAABESAgADBj6ZmZoAERICAAQGPxs40wASEwEAAAEBABITAQABBkDAAAAAEhMBAAIGQmLMzQASEwEAAwY/Y5p2ABITAQAEBj4XvE8AEhMCAAABAQASEwIAAQZAwAAAABITAgACBkJizM0AEhMCAAMGP2OadQASEwIABAY+F7xQABMVAQAAAcgAExUBAA8GQSAAAAATFQEAEAEBABMVAQARAQEAExUCAAAByAATFQIADwZBIAAAABMVAgAQAQEAExUCABEBAQAVGQEAAAEBABUZAgAAAQEAFwsAAAEBAQAaAAAAFQEBABoAAAAWCQASAGEAdQA2AGIAYQB0AGQAeAAAABoAAAAZAQEAGgEAAAAJABAAVgBSAFgAOQAxADgAUwAAABoBAAABCQAQAFYAUgBYADkAMQA4AFMAAA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="53">
								<StateVariable Name="Preset 24 Name" ID="53" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX918S / VRX918S 928LA LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="54">
								<StateVariable Name="Preset 25 Blob" ID="54" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="1255">AEwAAQgAAAMGAAAAAAABCAAACQYAAAAAAAEIAAAMAQAABQwBAA8ByAAFDAIADwHIAAUMAgASAQEABQwCABMBBAAJIwEAAAEBAAkjAQAGAQEACSMBAAwBAQAJIwEAEgEBAAkjAQAYAQEACSMBAB4BAQAJIwEAJAEBAAkjAQAqAQEACSMBADABAQAJIwEANgEBAAkjAQA8AQEACSMBAEIBAQAJIwEASAEBAAkjAQBOAQEACSMBAFQBAQAJIwEAWgEBAAkjAgAAAQEACSMCAAYBAQAJIwIADAEBAAkjAgASAQEACSMCABgBAQAJIwIAHgEBAAkjAgAkAQEACSMCACoBAQAJIwIAMAEBAAkjAgA2AQEACSMCADwBAQAJIwIAQgEBAAkjAgBIAQEACSMCAE4BAQAJIwIAVAEBAAkjAgBaAQEACiQBAAABAQAKJAEAAQZB8AAAAAokAQAFAQEACiQBAAYGQqAAAAAKJAIAAAEBAAokAgABBkHwAAAACiQCAAUBAQAKJAIABgZCoAAAAAwiAQAAAQEADCIBAAEGQjgAAAAMIgEAAgZAjXCkAAwiAQAEBkCAAAAADCIBAAYBAQAMIgEABwZCWAAAAAwiAQAIBkBAo9cADCIBAAoGQFMzMwAMIgEADAEBAAwiAQANBkKiAAAADCIBAA4GQCAAAAAMIgEAEAZAtmZmAAwiAQASAQEADCIBABMGQnAAAAAMIgEAFAY9zMzNAAwiAQAWBsAAAAAADCICAAABAQAMIgIAAQZCOAAAAAwiAgACBkCNcKQADCICAAQGQIAAAAAMIgIABgEBAAwiAgAHBkJYAAAADCICAAgGQECj1wAMIgIACgZAUzMzAAwiAgAMAQEADCICAA0GQqIAAAAMIgIADgZAIAAAAAwiAgAQBkC2ZmYADCICABIBAQAMIgIAEwZCcAAAAAwiAgAUBj3MzM0ADCICABYGwAAAAAANFAEAAQY76+36AA0UAgABBjvr7foADxABAAABAQAPEAEAAQECAA8QAgAAAQEADxACAAEBAgAQEQEAAAEBABARAQABBkLHhrgAEBEBAAMGPkzMzQAQEQIAAAEBABARAgABBkLHhrgAEBECAAMGPkzMzQAREgEAAAEBABESAQABBjynN+0AERIBAAIGQkgAAAAREgEAAwY+mZmaABESAQAEBj8bONMAERICAAABAQAREgIAAQY8pzftABESAgACBkJIAAAAERICAAMGPpmZmgAREgIABAY/GzjTABITAQAAAQEAEhMBAAEGQOAAAAASEwEAAgZCPZmaABITAQADBj9sLCwAEhMBAAQGPgb0qgASEwIAAAEBABITAgABBkDgAAAAEhMCAAIGQj2ZmgASEwIAAwY/bCwsABITAgAEBj4G9KoAExUBAAAByAATFQEADwZBIAAAABMVAQAQAQEAExUBABEBAQATFQIAAAHIABMVAgAPBkEgAAAAExUCABABAQATFQIAEQEBABUZAQAAAQEAFRkBAAUGQIAAAAAVGQIAAAEBABUZAgAFBkCAAAAAFwsAAAEBAQAaAAAAFQEBABoAAAAWCQASAGEAdQA2AGIAYQB0AGQAeAAAABoAAAAZAQEAGgEAAAAJABAAVgBSAFgAOQAxADUAUwAAABoBAAABCQAQAFYAUgBYADkAMQA1AFMAAA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="55">
								<StateVariable Name="Preset 25 Name" ID="55" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX915S / VRX915S 932LA-1 LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="56">
								<StateVariable Name="Preset 26 Blob" ID="56" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="1375">AEwAAQgAAAMGAAAAAAABCAAACQYAAAAAAAEIAAAMAQAABQwBAA8ByAAFDAIADwHIAAUMAgASAQEABQwCABMBBAAJIwEAAAEBAAkjAQAGAQEACSMBAAwBAQAJIwEAEgEBAAkjAQAYAQEACSMBAB4BAQAJIwEAJAEBAAkjAQAqAQEACSMBADABAQAJIwEANgEBAAkjAQA8AQEACSMBAEIBAQAJIwEASAEBAAkjAQBOAQEACSMBAFQBAQAJIwEAWgEBAAkjAgAAAQEACSMCAAYBAQAJIwIADAEBAAkjAgASAQEACSMCABgBAQAJIwIAHgEBAAkjAgAkAQEACSMCACoBAQAJIwIAMAEBAAkjAgA2AQEACSMCADwBAQAJIwIAQgEBAAkjAgBIAQEACSMCAE4BAQAJIwIAVAEBAAkjAgBaAQEACiQBAAABAQAKJAEAAQZB8AAAAAokAQAFAQEACiQBAAYGQqAAAAAKJAIAAAEBAAokAgABBkHwAAAACiQCAAUBAQAKJAIABgZCoAAAAAwiAQAAAQEADCIBAAEGQkgAAAAMIgEAAgZAO4UfAAwiAQAEBkBgAAAADCIBAAYBAQAMIgEABwZCggAAAAwiAQAKBj+AAAAADCIBAAwBAQAMIgEADQZCpAAAAAwiAQAOBj/mZmYADCIBABAGQKAAAAAMIgEAEgEBAAwiAQATBkI0AAAADCIBABQGQLAAAAAMIgEAFgZAAAAAAAwiAQAYAQEADCIBABkGQrQAAAAMIgEAGgZAoAAAAAwiAQAcBj9MzM0ADCIBAB4BAQAMIgEAHwZCcAAAAAwiAQAgBj3MzM0ADCIBACIGwAAAAAAMIgIAAAEBAAwiAgABBkJIAAAADCICAAIGQDuFHwAMIgIABAZAYAAAAAwiAgAGAQEADCICAAcGQoIAAAAMIgIACgY/gAAAAAwiAgAMAQEADCICAA0GQqQAAAAMIgIADgY/5mZmAAwiAgAQBkCgAAAADCICABIBAQAMIgIAEwZCNAAAAAwiAgAUBkCwAAAADCICABYGQAAAAAAMIgIAGAEBAAwiAgAZBkK0AAAADCICABoGQKAAAAAMIgIAHAY/TMzNAAwiAgAeAQEADCICAB8GQnAAAAAMIgIAIAY9zMzNAAwiAgAiBsAAAAAADRQBAAEGO+vt+gANFAIAAQY76+36AA8QAQAAAQEADxABAAEBAgAPEAIAAAEBAA8QAgABAQIAEBEBAAABAQAQEQEAAQZC725wABARAQADBj5MzM0AEBECAAABAQAQEQIAAQZC725wABARAgADBj5MzM0AERIBAAABAQAREgEAAQY8pzftABESAQACBkJwAAAAERIBAAMGPpmZmgAREgEABAY/GzjTABESAgAAAQEAERICAAEGPKc37QAREgIAAgZCcAAAABESAgADBj6ZmZoAERICAAQGPxs40wASEwEAAAEBABITAQABBkDAAAAAEhMBAAIGQmLMzQASEwEAAwY/Y5p1ABITAQAEBj4XvFAAEhMCAAABAQASEwIAAQZAwAAAABITAgACBkJizM0AEhMCAAMGP2OadQASEwIABAY+F7xQABMVAQAAAcgAExUBAA8GQSAAAAATFQEAEAEBABMVAQARAQEAExUCAAAByAATFQIADwZBIAAAABMVAgAQAQEAExUCABEBAQAVGQEAAAEBABUZAgAAAQEAFwsAAAEBAQAaAAAAFQEBABoAAAAWCQASAGEAdQA2AGIAYQB0AGQAeAAAABoAAAAZAQEAGgEAAAAJABAAVgBSAFgAOQAxADgAUwAAABoBAAABCQAQAFYAUgBYADkAMQA4AFMAAA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="57">
								<StateVariable Name="Preset 26 Name" ID="57" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX918S / VRX918S 932LA-1 LT 80</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="58">
								<StateVariable Name="Preset 27 Blob" ID="58" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="59">
								<StateVariable Name="Preset 27 Name" ID="59" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 27</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="60">
								<StateVariable Name="Preset 28 Blob" ID="60" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4966">[encoded data, 6624 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="61">
								<StateVariable Name="Preset 28 Name" ID="61" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x LT 80 / VRX915S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="62">
								<StateVariable Name="Preset 29 Blob" ID="62" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4977">[encoded data, 6636 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="63">
								<StateVariable Name="Preset 29 Name" ID="63" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 2x LT 80 / VRX915S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="64">
								<StateVariable Name="Preset 30 Blob" ID="64" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5007">[encoded data, 6676 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="65">
								<StateVariable Name="Preset 30 Name" ID="65" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 3x LT 80 / VRX915S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="66">
								<StateVariable Name="Preset 31 Blob" ID="66" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5026">[encoded data, 6704 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="67">
								<StateVariable Name="Preset 31 Name" ID="67" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 1x LT 80 / VRX918S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="68">
								<StateVariable Name="Preset 32 Blob" ID="68" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5037">[encoded data, 6716 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="69">
								<StateVariable Name="Preset 32 Name" ID="69" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 2x LT 80 / VRX918S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="70">
								<StateVariable Name="Preset 33 Blob" ID="70" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5067">[encoded data, 6756 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="71">
								<StateVariable Name="Preset 33 Name" ID="71" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX928LA 3x LT 80 / VRX918S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="72">
								<StateVariable Name="Preset 34 Blob" ID="72" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4970">[encoded data, 6628 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="73">
								<StateVariable Name="Preset 34 Name" ID="73" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 1x LT 80 / VRX915S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="74">
								<StateVariable Name="Preset 35 Blob" ID="74" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4940">[encoded data, 6588 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="75">
								<StateVariable Name="Preset 35 Name" ID="75" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 2x LT 80 / VRX915S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="76">
								<StateVariable Name="Preset 36 Blob" ID="76" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5022">[encoded data, 6696 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="77">
								<StateVariable Name="Preset 36 Name" ID="77" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 3x LT 80 / VRX915S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="78">
								<StateVariable Name="Preset 37 Blob" ID="78" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5030">[encoded data, 6708 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="79">
								<StateVariable Name="Preset 37 Name" ID="79" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 1x LT 80 / VRX918S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="80">
								<StateVariable Name="Preset 38 Blob" ID="80" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5000">[encoded data, 6668 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="81">
								<StateVariable Name="Preset 38 Name" ID="81" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 2x LT 80 / VRX918S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="82">
								<StateVariable Name="Preset 39 Blob" ID="82" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="5082">[encoded data, 6776 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="83">
								<StateVariable Name="Preset 39 Name" ID="83" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VRX932LA-1 3x LT 80 / VRX918S</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="84">
								<StateVariable Name="Preset 40 Blob" ID="84" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="85">
								<StateVariable Name="Preset 40 Name" ID="85" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 40</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="86">
								<StateVariable Name="Preset 41 Blob" ID="86" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="87">
								<StateVariable Name="Preset 41 Name" ID="87" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 41</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="88">
								<StateVariable Name="Preset 42 Blob" ID="88" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="89">
								<StateVariable Name="Preset 42 Name" ID="89" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 42</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="90">
								<StateVariable Name="Preset 43 Blob" ID="90" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="91">
								<StateVariable Name="Preset 43 Name" ID="91" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 43</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="92">
								<StateVariable Name="Preset 44 Blob" ID="92" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="93">
								<StateVariable Name="Preset 44 Name" ID="93" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 44</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="94">
								<StateVariable Name="Preset 45 Blob" ID="94" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="95">
								<StateVariable Name="Preset 45 Name" ID="95" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 45</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="96">
								<StateVariable Name="Preset 46 Blob" ID="96" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="97">
								<StateVariable Name="Preset 46 Name" ID="97" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 46</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="98">
								<StateVariable Name="Preset 47 Blob" ID="98" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="99">
								<StateVariable Name="Preset 47 Name" ID="99" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 47</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="100">
								<StateVariable Name="Preset 48 Blob" ID="100" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="101">
								<StateVariable Name="Preset 48 Name" ID="101" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 48</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="102">
								<StateVariable Name="Preset 49 Blob" ID="102" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="103">
								<StateVariable Name="Preset 49 Name" ID="103" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 49</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="104">
								<StateVariable Name="Preset 50 Blob" ID="104" ClassID="518" Version="1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="98">AEwABQwBAA8ByAAFDAIAAQEAAAUMAgADAQAABQwCAAQBAAAFDAIADwHIAAUMAgASAQEABQwCABMBBAATFQEAAAEAABMVAQACAQEAExUCAAABAAATFQIAAgEBABcLAAABAQE=</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="105">
								<StateVariable Name="Preset 50 Name" ID="105" ClassID="517" Version="1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset 50</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="106">
								<StateVariable Name="Max Preset Number" ID="106" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>50</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="107">
								<StateVariable Name="Min Preset Number" ID="107" ClassID="616" Version="1">
									<Min>1</Min>
									<Max>50</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="23" OBJ_ADDR="1709824">
						<Object Name="Power Supply" Address="1709824" ClassID="23" Version="1">
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="0">
								<StateVariable Name="Line Voltage" ID="0" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AICPQw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="1">
								<StateVariable Name="Proportional Vcc" ID="1" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">w/XAQA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="2">
								<StateVariable Name="Temperature" ID="2" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="3">
								<StateVariable Name="Vcc" ID="3" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACWQw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="4">
								<StateVariable Name="Temperature Deg C" ID="4" ClassID="535" Version="1">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="24" OBJ_ADDR="1710080">
						<Object Name="Fan Control" Address="1710080" ClassID="24" Version="1">
							<STATE_VARIABLE SV_CLASSID="741" SV_ID="0">
								<StateVariable Name="Mode" ID="0" ClassID="741" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Aggressiveness" ID="1" ClassID="733" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AABwQQ==</Data3>
									<Data1 Len="4">AAAgQQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="2">
								<StateVariable Name="Amp Fan Setpoint" ID="2" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="3">
								<StateVariable Name="Amp Fan Process Variable" ID="3" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="4">
								<StateVariable Name="Power Supply Fan Setpoint" ID="4" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Power Supply Fan Process Variable" ID="5" ClassID="535" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Amp Fan Test Setpoint" ID="6" ClassID="733" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<Data1 Len="4">AAAAPw==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Power Supply Fan Test Setpoint" ID="7" ClassID="733" Version="1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<Data1 Len="4">AAAAPw==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="8">
								<StateVariable Name="Power Supply Fan Setpoint Multiplier" ID="8" ClassID="733" Version="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<Data1 Len="4">AACAPw==</Data1>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="9">
								<StateVariable Name="Error" ID="9" ClassID="531" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="28" OBJ_ADDR="1776640">
						<Object Name="Governor" Address="1776640" ClassID="28" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Threshold" ID="3" ClassID="733" Version="1">
									<Data2 Len="4">AAAgQQ==</Data2>
									<Data3 Len="4">AEAcRg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="7">
								<StateVariable Name="Ch1 Power Meter" ID="7" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="9">
								<StateVariable Name="Ch2 Power Meter" ID="9" ClassID="535" Version="1">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="29" OBJ_ADDR="1776896">
						<Object Name="Thermal Level Control" Address="1776896" ClassID="29" Version="1">
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="0">
								<StateVariable Name="Power Supply Temp Threshold" ID="0" ClassID="733" Version="1">
									<Data2 Len="4">AADIQQ==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Channel Temp Threshold" ID="3" ClassID="733" Version="1">
									<Data2 Len="4">AADIQQ==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="38" OBJ_ADDR="1779200">
						<Object Name="Vcc Droop Limiter" Address="1779200" ClassID="38" Version="1">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" ClassID="512" Version="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
				</Object>
				<VirtualDevice Index="0" Version="1" />
				<NodeManager Version="1" SoftwareVersion="1.1.2.2" DeveloperAccessRights="0" HopCount="5" VenueTableSize="512" UserNameA="" UserNameB="" UserNameC="" UserNameD="" DevFuncPermsA="0" DevFuncPermsB="0" DevFuncPermsC="0" DevFuncPermsD="0" AddressMode="1" DeviceState="0">
					<SerialNumber Len="16">AAAAAAAAAAAAAAAKQAD3Sg==</SerialNumber>
					<UserPasswordA Len="0"></UserPasswordA>
					<UserPasswordB Len="0"></UserPasswordB>
					<UserPasswordC Len="0"></UserPasswordC>
					<UserPasswordD Len="0"></UserPasswordD>
					<AdminPassword Len="0"></AdminPassword>
					<VenueRecallCollection />
				</NodeManager>
			</VIRTUAL_DEVICE>
		</Node>
	</NODE>
</Device>