File name		Description
KX200_DSP.bin		DSP Firmeare Image for manufacture.
KX200_MCU.bin		MCU Firmware Image for manufacture.
kx200-Utility.exe	Application to upgrade DSP & MCU.
kx200.exe		Application to set KX200 audio parameters.


======================================================================================================
GUI (kx200.exe) : 1.1.3.0
MCU Firmware	: 1.1.3.3
DSP Firmware 	: 1.1.3.0
kx200-utility	: 1.1.3.3

Release Time    : 07-12-2016

MCU: 
Version: 1.1.3.3
Modification:
    1. Fix bug: When adjust the volume of Music/MIC/EFFECT at KX200 (Not on GUI), the volume can exceed the max volume settings.

======================================================================================================
GUI (kx200.exe) : 1.1.3.0
MCU Firmware	: 1.1.3.2
DSP Firmware 	: 1.1.3.0
kx200-utility	: 1.1.3.2

Release Time    : 05-30-2016

MCU: 
Version: 1.1.3.2
Modification:
    1. Fix factory Test bug: can't process Audio test after SDRAM test. This bug is only exist at version 1.1.3.1.
    2. For the previous MCU software, the ESC led will be lighted on at factory test. From this version, it will be lighted off.

======================================================================================================
GUI (kx200.exe) : 1.1.3.0
MCU Firmware	: 1.1.3.1
DSP Firmware 	: 1.1.3.0
kx200-utility	: 1.1.3.1

Release Time    : 05-17-2016

MCU: 
Version: 1.1.3.1
Modification:
    1. When factroy test failed at "SDRAM Test Failed", all the LED will blink, and test won't go on any more.

======================================================================================================
GUI (kx200.exe) : 1.1.0.6
MCU Firmware	: 1.1.0.6
DSP Firmware 	: 1.1.0.6
kx200-utility	: 1.1.0.6

Release Time    : 12-21-2015

GUI
Version: 1.1.0.6
Modification:
    1. Change the right-click pop-up menu "Enable All" to "Bypass All" in EQ widget.
    2. Change "AFS" to "AFE"
    3. Fix the bug: when user select Chinese Language, the "User Preset" isn't been translated into Chinese.

MCU: 
Version: 1.1.0.6
Modification:
    1. Add Led indication when initializing software .
    2. Add ESC + SYS button to disable DSP from loading preset.
    3. Change "AFS" to "AFE" for all LCD displayer.
    4. Fix the bug: No AFS saving or clearing when user do the operation on the LCD displayer.
