<Device xml:lang="en-US">
	<NODE>
		<Node Name="VTX M Series V5 R1.1" HiQnetDeviceKey="43b1b35f-ba4d-4ef0-86fb-afed346f5efa" GroupPath="\Room 1\Rack 1\VTX M Series V5 R1.1" ClassName="Crown I-Tech HD" ClassID="76" Address="2" Version="1" WasMatched="True" ZOrderIndex="10" PresetProxy="0">
			<ProductIndex>0</ProductIndex>
			<X>0</X>
			<Y>0</Y>
			<VIRTUAL_DEVICE VD_INDEX="0">
				<Object Name="VTX M Series V5 R1.1" Address="0" ClassID="76" Version="1" HiQnetObjectKey="3cd87d49-ffdd-4937-8866-0841865b42e4">
					<OBJECT OBJ_CLASSID="8" OBJ_ADDR="67584">
						<Object Name="Analog Inputs" Address="67584" ClassID="8" Version="1" HiQnetObjectKey="05e6a7fe-97cc-4f19-963c-755a9ab285d4">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Input 1 Peak Level Meter" ID="0" HiQnetStateVariableKey="7f064dc2-cb95-49d6-8d70-95253953bfcd" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Input 1 RMS Level Meter" ID="1" HiQnetStateVariableKey="64bfc9f4-de7f-4710-9495-43427dfc9788" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="2">
								<StateVariable Name="Input 1 Clip Indicator" ID="2" HiQnetStateVariableKey="96452c7a-6ee2-42cf-acbe-0d213ef411f7" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Input 1 Fader" ID="3" HiQnetStateVariableKey="fd60d0da-8e4c-45d8-8f53-3c2657e6568d" ClassID="733" Version="1" DefaultValue="7.1">
									<Min>0</Min>
									<Max>8.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Input 1 Mute Enable" ID="4" HiQnetStateVariableKey="7e966d21-bcf4-4a75-b0a4-7a6954d703cf" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Input 1 Invert" ID="5" HiQnetStateVariableKey="016dfcbd-2bfc-4f3b-b631-409fc887ab11" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Input 2 Peak Level Meter" ID="6" HiQnetStateVariableKey="925cb015-5755-4765-83d7-c7f94240b7c3" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Input 2 RMS Level Meter" ID="7" HiQnetStateVariableKey="9003e1a1-14ed-4ec4-9bd1-61e526c923b7" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Input 2 Clip Indicator" ID="8" HiQnetStateVariableKey="9cf5c1f0-c02f-4afa-b1fe-c1b7b72247ec" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="9">
								<StateVariable Name="Input 2 Fader" ID="9" HiQnetStateVariableKey="ce413427-6d2a-49fb-bf5a-834212f0824e" ClassID="733" Version="1" DefaultValue="7.1">
									<Min>0</Min>
									<Max>8.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Input 2 Mute Enable" ID="10" HiQnetStateVariableKey="56e67d87-6d5d-4348-9b04-86e541994b5c" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Input 2 Invert" ID="11" HiQnetStateVariableKey="561cc58f-ca57-48fb-93a3-8618c796ddc3" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="High Gain" ID="12" HiQnetStateVariableKey="eb45f65b-325d-4edc-af3a-513e48546f77" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="13">
								<StateVariable Name="Input 1 Nominal Sensitivity" ID="13" HiQnetStateVariableKey="549cc71c-75ec-413f-8b54-ec82c32ff54b" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="14">
								<StateVariable Name="Input 1 Nominal Gain" ID="14" HiQnetStateVariableKey="64e65125-b3da-4a55-970c-0660e207dc6f" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AABIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="15">
								<StateVariable Name="Input 2 Nominal Sensitivity" ID="15" HiQnetStateVariableKey="72ff857d-e01c-41bd-968f-6433228bd879" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="16">
								<StateVariable Name="Input 2 Nominal Gain" ID="16" HiQnetStateVariableKey="bdd715a8-b382-4a9a-b4dd-d9441771cf4a" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AABIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="17">
								<StateVariable Name="Input 1 Clip Counter" ID="17" HiQnetStateVariableKey="b3c8a3c7-1117-459b-8fac-bcf822cf2f44" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="18">
								<StateVariable Name="Input 2 Clip Counter" ID="18" HiQnetStateVariableKey="d7c39585-68b4-4d51-9c9a-07bce37b7c71" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Report Input 1 Clip Errors" ID="19" HiQnetStateVariableKey="93ec1f49-3428-40fd-bcd8-8434c38c6245" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="20">
								<StateVariable Name="Input 1 Clip Error Threshold" ID="20" HiQnetStateVariableKey="a608d292-ce48-4864-9cf2-ecd12b5b130e" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="21">
								<StateVariable Name="Input 1 Clip Error Time" ID="21" HiQnetStateVariableKey="1e2452f4-cd66-4ba9-9a04-305cf2a2f36c" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="22">
								<StateVariable Name="Input 1 Clip Error Log" ID="22" HiQnetStateVariableKey="2da32b89-5ae1-4add-8512-25b8b11ff0d8" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="23">
								<StateVariable Name="Input 1 Clip Error Last" ID="23" HiQnetStateVariableKey="b7ff6d87-a5fd-42b3-b961-241a10369660" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Report Input 2 Clip Errors" ID="24" HiQnetStateVariableKey="118e72d4-4c4d-48aa-b816-2d4a6cb50843" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="25">
								<StateVariable Name="Input 2 Clip Error Threshold" ID="25" HiQnetStateVariableKey="d342a95a-8439-4fee-bc52-f2d71097d7f8" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="26">
								<StateVariable Name="Input 2 Clip Error Time" ID="26" HiQnetStateVariableKey="d6c7d689-0c06-46e8-98bb-796b88f45c58" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="27">
								<StateVariable Name="Input 2 Clip Error Log" ID="27" HiQnetStateVariableKey="da77b764-b0de-4747-a9a9-192b72ad6448" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="28">
								<StateVariable Name="Input 2 Clip Error Last" ID="28" HiQnetStateVariableKey="6122194e-d139-4790-86d8-e6b2fb7abed6" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="29">
								<StateVariable Name="Input 1 Post Fader Peak Level Meter" ID="29" HiQnetStateVariableKey="87634daa-f716-483e-8444-bb8bceabee6c" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="30">
								<StateVariable Name="Input 1 Post Fader RMS Level Meter" ID="30" HiQnetStateVariableKey="37138560-6fa7-404e-9ee1-ad9a21a60e1d" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="31">
								<StateVariable Name="Input 2 Post Fader Peak Level Meter" ID="31" HiQnetStateVariableKey="b721bf8a-ce5c-4289-9b33-b51fcfc778d1" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="32">
								<StateVariable Name="Input 2 Post Fader RMS Level Meter" ID="32" HiQnetStateVariableKey="2208fc74-4f70-4654-952f-0403982f2132" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="33">
								<StateVariable Name="Delay FIR Coeff Calculation" ID="33" HiQnetStateVariableKey="054f285f-cc6b-4e16-bacb-2919f13b6707" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="34">
								<StateVariable Name="Input 1 Detector Threshold" ID="34" HiQnetStateVariableKey="37c87c74-45e5-448a-913a-a548c473c05b" ClassID="546" Version="1" DefaultValue="80">
									<Min>40</Min>
									<Max>200</Max>
									<Value>80</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="35">
								<StateVariable Name="Input 2 Detector Threshold" ID="35" HiQnetStateVariableKey="552a72e4-0ef6-4cc1-a077-302398af23bd" ClassID="546" Version="1" DefaultValue="80">
									<Min>40</Min>
									<Max>200</Max>
									<Value>80</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="36">
								<StateVariable Name="Input 1 Detector Hold Time" ID="36" HiQnetStateVariableKey="5cbe87eb-ad75-49e0-83fe-6d25b14bdd0c" ClassID="733" Version="1" DefaultValue="0.03">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.03</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="37">
								<StateVariable Name="Input 2 Detector Hold Time" ID="37" HiQnetStateVariableKey="aee3cc65-9573-4b2d-9d9a-6c075f9ce3bb" ClassID="733" Version="1" DefaultValue="0.03">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.03</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="38">
								<StateVariable Name="Input 1 Detector Status" ID="38" HiQnetStateVariableKey="65d89487-cb2c-4b74-a5ea-fcef3530facc" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="39">
								<StateVariable Name="Input 2 Detector Status" ID="39" HiQnetStateVariableKey="23df11e2-834e-423a-94e4-f9abdbb5cf4a" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="9" OBJ_ADDR="133376">
						<Object Name="AES Inputs" Address="133376" ClassID="9" Version="1" HiQnetObjectKey="d2029472-fd41-49aa-8e7a-1dea3296fbd3">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Input 1 Peak Level Meter" ID="0" HiQnetStateVariableKey="64f9b187-a123-4f12-8b3e-c21340e58a84" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Input 1 RMS Level Meter" ID="1" HiQnetStateVariableKey="ee6cdbda-2785-46de-b535-92394dabaf85" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="2">
								<StateVariable Name="Input 1 Clip Indicator" ID="2" HiQnetStateVariableKey="bc6be75a-55ee-4632-9c54-92252838b242" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Input 1 Fader" ID="3" HiQnetStateVariableKey="5f3d8d95-d675-49fe-8d07-e8aab3c18570" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Input 1 Mute Enable" ID="4" HiQnetStateVariableKey="ef2205fa-7cab-49e7-9918-9eb91e131335" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Input 1 Invert" ID="5" HiQnetStateVariableKey="6909f945-8e68-43c1-ad05-09c247f82eb7" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Input 2 Peak Level Meter" ID="6" HiQnetStateVariableKey="3d1c8b6c-77e6-48f3-83c5-c451e3a6c992" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Input 2 RMS Level Meter" ID="7" HiQnetStateVariableKey="07f70b2b-5eca-447c-b33c-9a2a6ab41369" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Input 2 Clip Indicator" ID="8" HiQnetStateVariableKey="cc8c9b88-8fa6-481f-bde9-67d40123ab6b" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="9">
								<StateVariable Name="Input 2 Fader" ID="9" HiQnetStateVariableKey="84b027e8-65f5-4585-bea6-0d7de50594fb" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Input 2 Mute Enable" ID="10" HiQnetStateVariableKey="c4ce17d3-5dae-4d0d-afc1-f9756456a366" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Input 2 Invert" ID="11" HiQnetStateVariableKey="6a4b2949-7312-44ab-b493-cfa9a9c5f90e" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="12">
								<StateVariable Name="Input 1 Clip Counter" ID="12" HiQnetStateVariableKey="cacd5edc-0071-4cb7-a071-094afcc857e8" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="13">
								<StateVariable Name="Input 2 Clip Counter" ID="13" HiQnetStateVariableKey="80a88b7e-60d0-4f58-919b-9153dfc2a3f3" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="14">
								<StateVariable Name="Report Input 1 Clip Errors" ID="14" HiQnetStateVariableKey="b0e161cd-7ae9-4e33-a117-bd2fb07e198b" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Input 1 Clip Error Threshold" ID="15" HiQnetStateVariableKey="9e4e5036-efc8-4eea-8fb6-d95fd50f3c86" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="16">
								<StateVariable Name="Input 1 Clip Error Time" ID="16" HiQnetStateVariableKey="83701105-d485-4bdc-b1cf-e0550b6a45a3" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="17">
								<StateVariable Name="Input 1 Clip Error Log" ID="17" HiQnetStateVariableKey="9736d2cd-36ad-4952-beed-9577c44d9932" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="18">
								<StateVariable Name="Input 1 Clip Error Last" ID="18" HiQnetStateVariableKey="fc6cc8a4-f416-47fb-b6b0-6ce984e92a42" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Report Input 2 Clip Errors" ID="19" HiQnetStateVariableKey="f682ac27-ae15-4fed-876b-c6d0557dfe2c" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="20">
								<StateVariable Name="Input 2 Clip Error Threshold" ID="20" HiQnetStateVariableKey="048d9293-e3a2-41c8-83eb-ff84ae642e03" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="21">
								<StateVariable Name="Input 2 Clip Error Time" ID="21" HiQnetStateVariableKey="d9951289-7d6a-4065-b740-7b0e7e00725c" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="22">
								<StateVariable Name="Input 2 Clip Error Log" ID="22" HiQnetStateVariableKey="7cfc5172-0ca1-4a81-b43a-59ad2e7d548a" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="23">
								<StateVariable Name="Input 2 Clip Error Last" ID="23" HiQnetStateVariableKey="01b7d059-a609-4932-9bbc-99f396aef911" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="24">
								<StateVariable Name="Status" ID="24" HiQnetStateVariableKey="d2936ee6-d20e-4d84-ab2b-cf8334bc8220" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="25">
								<StateVariable Name="Input 1 Post Fader Peak Level Meter" ID="25" HiQnetStateVariableKey="ea319691-3644-4bf2-b9d4-a50b6f6710d7" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="26">
								<StateVariable Name="Input 1 Post Fader RMS Level Meter" ID="26" HiQnetStateVariableKey="339faaa1-c150-478b-a5ef-90e1991c5cd2" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="27">
								<StateVariable Name="Input 2 Post Fader Peak Level Meter" ID="27" HiQnetStateVariableKey="761fbab1-2d32-4b7f-91ff-12f2edb7faf8" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="28">
								<StateVariable Name="Input 2 Post Fader RMS Level Meter" ID="28" HiQnetStateVariableKey="6b8a2621-57fe-49a0-a936-9182d2db1337" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="29">
								<StateVariable Name="Receive Error" ID="29" HiQnetStateVariableKey="f2fa5784-3bf4-4186-82c6-2e369b1079ef" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Input 1 Detector Threshold" ID="30" HiQnetStateVariableKey="e74eca01-b9d7-4131-b42d-2e0cc9a6268e" ClassID="546" Version="1" DefaultValue="40">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Input 2 Detector Threshold" ID="31" HiQnetStateVariableKey="525dd745-d4aa-4f9e-9130-2a5396289f18" ClassID="546" Version="1" DefaultValue="40">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Input 1 Detector Hold Time" ID="32" HiQnetStateVariableKey="ab606041-fa2a-4b06-a2d3-855267d80cba" ClassID="733" Version="1" DefaultValue="0.02">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.02</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Input 2 Detector Hold Time" ID="33" HiQnetStateVariableKey="02492168-8430-4fb1-892d-5b81fda9c22b" ClassID="733" Version="1" DefaultValue="0.02">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.02</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="34">
								<StateVariable Name="Input 1 Detector Status" ID="34" HiQnetStateVariableKey="c4e1ca98-06fa-480e-88af-2894680f27fb" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="35">
								<StateVariable Name="Input 2 Detector Status" ID="35" HiQnetStateVariableKey="5249e113-247d-483a-bebe-0d265097f54b" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="10" OBJ_ADDR="199168">
						<Object Name="CobraNet Inputs" Address="199168" ClassID="10" Version="1" HiQnetObjectKey="b606977b-6879-41bf-b71f-5fca04501d4a">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Input 1 Peak Level Meter" ID="0" HiQnetStateVariableKey="180495f0-81da-43de-bba1-af12ff4e0bbf" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Input 1 RMS Level Meter" ID="1" HiQnetStateVariableKey="471956d1-d0ef-4a8b-877d-5788005332c1" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="2">
								<StateVariable Name="Input 1 Clip Indicator" ID="2" HiQnetStateVariableKey="fcefe266-746c-487e-be2b-d2a82df5db0b" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Input 1 Fader" ID="3" HiQnetStateVariableKey="ba6ad1b0-06fd-42db-a3c6-ffb5399647b6" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Input 1 Mute Enable" ID="4" HiQnetStateVariableKey="7e9e588d-0be0-4f16-9f9c-05486bc48eee" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Input 1 Invert" ID="5" HiQnetStateVariableKey="f1e998c2-ef7f-42ac-b217-bd4e89762c3b" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Input 2 Peak Level Meter" ID="6" HiQnetStateVariableKey="0b3e5aca-b03d-4bf9-9f8f-6b791737d9d3" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Input 2 RMS Level Meter" ID="7" HiQnetStateVariableKey="f1dc7dea-b443-42fd-8915-5e8a353c5546" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Input 2 Clip Indicator" ID="8" HiQnetStateVariableKey="3113964f-eab8-4e3f-9c39-f4827d8ee1d3" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="9">
								<StateVariable Name="Input 2 Fader" ID="9" HiQnetStateVariableKey="f7387d44-14a3-4af4-ba89-3ee78d4011ed" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Input 2 Mute Enable" ID="10" HiQnetStateVariableKey="c802b649-cdce-4d99-a0d6-4022662431f9" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Input 2 Invert" ID="11" HiQnetStateVariableKey="f7fd2e6c-9fc8-4551-afde-294609f208b9" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="12">
								<StateVariable Name="Input 1 Clip Counter" ID="12" HiQnetStateVariableKey="e214d1a3-da96-44f4-b5cd-bdd598989e4e" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="13">
								<StateVariable Name="Input 2 Clip Counter" ID="13" HiQnetStateVariableKey="9f34f318-09d0-416b-8044-07d25752b1c7" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="14">
								<StateVariable Name="Report Input 1 Clip Errors" ID="14" HiQnetStateVariableKey="af9c0834-0dea-48cd-95c0-d26043e8028d" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Input 1 Clip Error Threshold" ID="15" HiQnetStateVariableKey="931862ee-a523-4e09-b7c8-e723a447c17d" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="16">
								<StateVariable Name="Input 1 Clip Error Time" ID="16" HiQnetStateVariableKey="5b329dca-1e30-42cf-9be3-4e670642097f" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="17">
								<StateVariable Name="Input 1 Clip Error Log" ID="17" HiQnetStateVariableKey="b6122b7e-1f57-4db4-80e0-92b2bdc586e0" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="18">
								<StateVariable Name="Input 1 Clip Error Last" ID="18" HiQnetStateVariableKey="d2f30361-c595-4031-a64e-5e3125f84eb6" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Report Input 2 Clip Errors" ID="19" HiQnetStateVariableKey="8640e70d-5a51-4a2d-a20f-f4b51dca3805" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="20">
								<StateVariable Name="Input 2 Clip Error Threshold" ID="20" HiQnetStateVariableKey="3150e527-2b73-4fd5-ba52-d6b139fe83f9" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="21">
								<StateVariable Name="Input 2 Clip Error Time" ID="21" HiQnetStateVariableKey="635db925-528c-4ba8-b20b-71806eda988e" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="22">
								<StateVariable Name="Input 2 Clip Error Log" ID="22" HiQnetStateVariableKey="0805e2e1-fdd0-4c04-9578-8ebcf56a0150" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="23">
								<StateVariable Name="Input 2 Clip Error Last" ID="23" HiQnetStateVariableKey="960315f3-7f2c-496b-b798-2465e49f6218" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="24">
								<StateVariable Name="Input 1 Status" ID="24" HiQnetStateVariableKey="5ed91c69-faf6-4079-aae0-e0513f19a4c6" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="25">
								<StateVariable Name="Input 2 Status" ID="25" HiQnetStateVariableKey="7119136b-689b-4ce1-b616-09bc95b97ab5" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="26">
								<StateVariable Name="Input 1 Post Fader Peak Level Meter" ID="26" HiQnetStateVariableKey="96a12473-b4a1-47ff-9d09-93c125e44696" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="27">
								<StateVariable Name="Input 1 Post Fader RMS Level Meter" ID="27" HiQnetStateVariableKey="f964d564-6949-46cd-aa43-f6b8ecd6da71" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="28">
								<StateVariable Name="Input 2 Post Fader Peak Level Meter" ID="28" HiQnetStateVariableKey="45f003aa-fcf4-41cd-b600-395fadf544a7" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="29">
								<StateVariable Name="Input 2 Post Fader RMS Level Meter" ID="29" HiQnetStateVariableKey="43455b47-7afd-44f6-9981-d9a3df828387" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Input 1 Detector Threshold" ID="30" HiQnetStateVariableKey="c89953c3-9b46-4761-884a-733992e57057" ClassID="546" Version="1" DefaultValue="40">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Input 2 Detector Threshold" ID="31" HiQnetStateVariableKey="c971a0a7-9c16-4451-a6a3-29b8b20efc97" ClassID="546" Version="1" DefaultValue="40">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Input 1 Detector Hold Time" ID="32" HiQnetStateVariableKey="14b5b271-35a9-4a85-aa61-e3a9f29df8eb" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Input 2 Detector Hold Time" ID="33" HiQnetStateVariableKey="3376b01e-0c7f-4470-81ea-944d8f54a66e" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>0.01</Min>
									<Max>120</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="34">
								<StateVariable Name="Input 1 Detector Status" ID="34" HiQnetStateVariableKey="3559ba50-a35b-48ae-be3a-396e99d3cfdc" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="35">
								<StateVariable Name="Input 2 Detector Status" ID="35" HiQnetStateVariableKey="c69722e2-db07-48d3-ad76-d6ff96124474" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="6" OBJ_ADDR="263680">
						<Object Name="CobraNet Receive" Address="263680" ClassID="6" Version="1" HiQnetObjectKey="c62e5e26-1c40-4a25-b2ba-9d80fd59279c">
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="0">
								<StateVariable Name="RxA Bundle" ID="0" HiQnetStateVariableKey="ff493173-105e-4aa8-9104-683dbcb59349" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="1">
								<StateVariable Name="RxA Status" ID="1" HiQnetStateVariableKey="2dd00fbc-c0af-4cd6-b78a-480d0768f270" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="2">
								<StateVariable Name="RxA Slot 1" ID="2" HiQnetStateVariableKey="1b2a0c08-39d5-4319-9f32-6be1f7aa8a80" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="3">
								<StateVariable Name="RxA Slot 2" ID="3" HiQnetStateVariableKey="5c195041-c6f1-4bb8-80f5-25fe575980e0" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="4">
								<StateVariable Name="RxA Slot 3" ID="4" HiQnetStateVariableKey="30aaa032-985f-4778-924a-62e5f32ec587" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="5">
								<StateVariable Name="RxA Slot 4" ID="5" HiQnetStateVariableKey="c5830007-b658-4c00-931c-8d195e859642" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="6">
								<StateVariable Name="RxA Slot 5" ID="6" HiQnetStateVariableKey="3164d2ba-950a-47e0-bd42-7160463e41c5" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="7">
								<StateVariable Name="RxA Slot 6" ID="7" HiQnetStateVariableKey="fb5b857e-5e54-4752-bc92-5cbd3b159978" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="8">
								<StateVariable Name="RxA Slot 7" ID="8" HiQnetStateVariableKey="1c820d2d-d32c-4ea1-bf27-e77817d26955" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="9">
								<StateVariable Name="RxA Slot 8" ID="9" HiQnetStateVariableKey="ac9ffdd8-e8dc-4c51-a533-6b62a0cb0fd9" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="10">
								<StateVariable Name="RxB Bundle" ID="10" HiQnetStateVariableKey="d550e34c-1d42-47a9-b4ef-670aac134c66" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="11">
								<StateVariable Name="RxB Status" ID="11" HiQnetStateVariableKey="9d86430a-fb3a-412b-895c-054c65f7616b" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="12">
								<StateVariable Name="RxB Slot 1" ID="12" HiQnetStateVariableKey="7742aa66-7686-4650-b21d-39fcaa3a2a62" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="13">
								<StateVariable Name="RxB Slot 2" ID="13" HiQnetStateVariableKey="90f70498-0ca2-4229-99ae-9b972ec89ea7" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="14">
								<StateVariable Name="RxB Slot 3" ID="14" HiQnetStateVariableKey="eb7c8dfb-717b-49ea-8899-abcf686d3600" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="15">
								<StateVariable Name="RxB Slot 4" ID="15" HiQnetStateVariableKey="2cde2418-ad3e-44da-84fa-60e13fb5d8e0" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="16">
								<StateVariable Name="RxB Slot 5" ID="16" HiQnetStateVariableKey="d20113f3-63b6-4126-9296-b1ff4cdeedb6" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="17">
								<StateVariable Name="RxB Slot 6" ID="17" HiQnetStateVariableKey="4211a497-1495-4ebc-a486-de9ca2b74252" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="18">
								<StateVariable Name="RxB Slot 7" ID="18" HiQnetStateVariableKey="6d5636da-7aba-440b-aacf-0c6b2a7b5bdd" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="19">
								<StateVariable Name="RxB Slot 8" ID="19" HiQnetStateVariableKey="073a6e95-9fc6-43af-a96a-1239417ae9d6" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="20">
								<StateVariable Name="RxC Bundle" ID="20" HiQnetStateVariableKey="ba6da88a-25cd-42e0-93e1-d30bedcfa365" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="21">
								<StateVariable Name="RxC Status" ID="21" HiQnetStateVariableKey="f85d5f2e-73da-41a1-b005-42d86ce16ccc" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="22">
								<StateVariable Name="RxC Slot 1" ID="22" HiQnetStateVariableKey="c79c81b5-c20b-43d8-a862-2614788cd769" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="23">
								<StateVariable Name="RxC Slot 2" ID="23" HiQnetStateVariableKey="81a817dd-24b2-4cc8-940a-02f93064970f" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="24">
								<StateVariable Name="RxC Slot 3" ID="24" HiQnetStateVariableKey="cfb1f152-b082-40ea-bb08-311735cb5b57" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="25">
								<StateVariable Name="RxC Slot 4" ID="25" HiQnetStateVariableKey="336018dc-dc17-4f33-b132-30dc8016d3d9" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="26">
								<StateVariable Name="RxC Slot 5" ID="26" HiQnetStateVariableKey="55fd7843-f953-4c03-87ce-9d891f773082" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="27">
								<StateVariable Name="RxC Slot 6" ID="27" HiQnetStateVariableKey="563b7b64-7b3f-4c47-abfe-02efb4eb4f19" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="28">
								<StateVariable Name="RxC Slot 7" ID="28" HiQnetStateVariableKey="f70b13d7-9632-4f3e-a092-835e2617e67f" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="29">
								<StateVariable Name="RxC Slot 8" ID="29" HiQnetStateVariableKey="fbc3006b-295f-4a03-be70-2c67997ed29c" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="30">
								<StateVariable Name="RxD Bundle" ID="30" HiQnetStateVariableKey="c0c5fda8-559d-48d0-bd27-5331a388a7c7" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="31">
								<StateVariable Name="RxD Status" ID="31" HiQnetStateVariableKey="8e293086-f5e9-468b-a267-5509fef42a39" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="32">
								<StateVariable Name="RxD Slot 1" ID="32" HiQnetStateVariableKey="7792c8c0-d468-4fb5-8bb7-e1785e0ddb1e" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="33">
								<StateVariable Name="RxD Slot 2" ID="33" HiQnetStateVariableKey="5a982eb9-91fb-44c4-af5d-28a43a00319a" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="34">
								<StateVariable Name="RxD Slot 3" ID="34" HiQnetStateVariableKey="1175318a-9440-483c-9383-d8afd87ac41d" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="35">
								<StateVariable Name="RxD Slot 4" ID="35" HiQnetStateVariableKey="72f9d41c-56cd-49bc-887a-4fe219977d54" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="36">
								<StateVariable Name="RxD Slot 5" ID="36" HiQnetStateVariableKey="0714fba2-7ec6-4d16-937b-31be552a4743" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="37">
								<StateVariable Name="RxD Slot 6" ID="37" HiQnetStateVariableKey="e554d7c8-785b-4d7e-8aa8-38e0ab291d0c" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="38">
								<StateVariable Name="RxD Slot 7" ID="38" HiQnetStateVariableKey="14b8146a-9ff0-4e7b-87e6-e3c95ea9d470" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="662" SV_ID="39">
								<StateVariable Name="RxD Slot 8" ID="39" HiQnetStateVariableKey="4711a7c9-27a7-4049-9b29-fcd7c53ff23d" ClassID="662" Version="1" DefaultValue="33">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">KA==</Data3>
									<Data1 Len="1">IQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="40">
								<StateVariable Name="Input 1 Label" ID="40" HiQnetStateVariableKey="dfa9b555-e38f-4041-986c-a5770781b73a" ClassID="517" Version="1" DefaultValue="Input 1 Label">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="26">SQBuAHAAdQB0ACAAMQAgAEwAYQBiAGUAbAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="631" SV_ID="41">
								<StateVariable Name="Input 1" ID="41" HiQnetStateVariableKey="5afcc369-788d-496d-b181-cc18a6d6d421" ClassID="631" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>32</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="42">
								<StateVariable Name="Input 1 Meter" ID="42" HiQnetStateVariableKey="fb582df6-65b2-41e9-9e26-fcd59615aa1c" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="43">
								<StateVariable Name="Input 2 Label" ID="43" HiQnetStateVariableKey="0931638f-c049-4979-9b56-edd77442d734" ClassID="517" Version="1" DefaultValue="Input 2 Label">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="26">SQBuAHAAdQB0ACAAMgAgAEwAYQBiAGUAbAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="631" SV_ID="44">
								<StateVariable Name="Input 2" ID="44" HiQnetStateVariableKey="21329dad-64ef-4c8b-b3c3-f89f1ec79b20" ClassID="631" Version="1" DefaultValue="9">
									<Min>0</Min>
									<Max>32</Max>
									<Value>9</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="45">
								<StateVariable Name="Input 2 Meter" ID="45" HiQnetStateVariableKey="19eb6caa-b04f-4629-8fc1-bb1a95ba6683" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="46">
								<StateVariable Name="RxA Sub Format 1" ID="46" HiQnetStateVariableKey="9a23bcfc-bdb3-4c36-b1b0-a7aee8ace606" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="47">
								<StateVariable Name="RxA Sub Format 2" ID="47" HiQnetStateVariableKey="e422d4ac-5365-483b-a9eb-1d2d0a009282" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="48">
								<StateVariable Name="RxA Sub Format 3" ID="48" HiQnetStateVariableKey="2b8b4ada-68fa-4d40-ad47-e2797eea8cc1" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="49">
								<StateVariable Name="RxA Sub Format 4" ID="49" HiQnetStateVariableKey="1c97d2f0-dd49-414a-9f8e-d67fad798dbf" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="50">
								<StateVariable Name="RxA Sub Format 5" ID="50" HiQnetStateVariableKey="b01aae26-5c51-4f7e-8b6f-4cd83b7e9234" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="51">
								<StateVariable Name="RxA Sub Format 6" ID="51" HiQnetStateVariableKey="0a2a75ab-64e3-4299-8fba-ffd854960b2e" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="52">
								<StateVariable Name="RxA Sub Format 7" ID="52" HiQnetStateVariableKey="d6d27ea2-208d-4d07-aab6-e36943de84a3" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="53">
								<StateVariable Name="RxA Sub Format 8" ID="53" HiQnetStateVariableKey="60e90680-b08d-410a-aacc-ffac795cc272" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="54">
								<StateVariable Name="RxB Sub Format 1" ID="54" HiQnetStateVariableKey="7a9d33df-80dd-4136-a7b0-c27fbebc625e" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="55">
								<StateVariable Name="RxB Sub Format 2" ID="55" HiQnetStateVariableKey="685cadba-e2dd-4dc9-802f-52568bbe9e92" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="56">
								<StateVariable Name="RxB Sub Format 3" ID="56" HiQnetStateVariableKey="4c8a10a8-0287-40ab-8e24-616652c882e9" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="57">
								<StateVariable Name="RxB Sub Format 4" ID="57" HiQnetStateVariableKey="bccf9414-4170-436e-b981-027b8a764689" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="58">
								<StateVariable Name="RxB Sub Format 5" ID="58" HiQnetStateVariableKey="c60117a7-b481-4468-8537-ee1994b95525" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="59">
								<StateVariable Name="RxB Sub Format 6" ID="59" HiQnetStateVariableKey="1935622b-7337-43fb-9310-b6f612665ff8" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="60">
								<StateVariable Name="RxB Sub Format 7" ID="60" HiQnetStateVariableKey="3bc07db3-9a04-49bb-853d-dd74d3808d1f" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="61">
								<StateVariable Name="RxB Sub Format 8" ID="61" HiQnetStateVariableKey="2d175952-c71a-4573-b382-ad2b78c234fe" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="62">
								<StateVariable Name="RxC Sub Format 1" ID="62" HiQnetStateVariableKey="7d77d5cd-0081-478b-8ce0-7d60d2ba9b42" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="63">
								<StateVariable Name="RxC Sub Format 2" ID="63" HiQnetStateVariableKey="b8619da3-7663-418b-b3c1-9c26054a97b1" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="64">
								<StateVariable Name="RxC Sub Format 3" ID="64" HiQnetStateVariableKey="1b9680dd-ad3a-4aff-b292-31ee47e62d4b" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="65">
								<StateVariable Name="RxC Sub Format 4" ID="65" HiQnetStateVariableKey="e39cbbca-5ded-4e14-8c63-853fdf990ab9" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="66">
								<StateVariable Name="RxC Sub Format 5" ID="66" HiQnetStateVariableKey="6a498f26-7486-41de-844e-3699bb6eebc8" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="67">
								<StateVariable Name="RxC Sub Format 6" ID="67" HiQnetStateVariableKey="7c17e2f0-3843-488e-82b9-64596ce5bf95" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="68">
								<StateVariable Name="RxC Sub Format 7" ID="68" HiQnetStateVariableKey="93895a4a-bff9-4ab7-818e-a17ec964c645" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="69">
								<StateVariable Name="RxC Sub Format 8" ID="69" HiQnetStateVariableKey="38ccd228-e9d0-4549-8baa-eb6942f2bf27" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="70">
								<StateVariable Name="RxD Sub Format 1" ID="70" HiQnetStateVariableKey="8f2af989-ede7-4a1d-8624-4f722ba7e8b6" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="71">
								<StateVariable Name="RxD Sub Format 2" ID="71" HiQnetStateVariableKey="baf91394-029a-4479-aad7-46bddcab89c4" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="72">
								<StateVariable Name="RxD Sub Format 3" ID="72" HiQnetStateVariableKey="ddacebe8-21a1-4e4d-9a7b-cd6ca7fdd221" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="73">
								<StateVariable Name="RxD Sub Format 4" ID="73" HiQnetStateVariableKey="d63c53dd-6586-45b3-996a-2bd9195986e6" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="74">
								<StateVariable Name="RxD Sub Format 5" ID="74" HiQnetStateVariableKey="79d12775-39f4-4172-b334-716089af1e89" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="75">
								<StateVariable Name="RxD Sub Format 6" ID="75" HiQnetStateVariableKey="78764e08-d378-4af5-8c22-930626968d2c" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="76">
								<StateVariable Name="RxD Sub Format 7" ID="76" HiQnetStateVariableKey="04921cab-665f-46b9-83d8-3b6cbdc5725b" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="77">
								<StateVariable Name="RxD Sub Format 8" ID="77" HiQnetStateVariableKey="c925ba92-f5b6-44e1-9f92-e5ac2eb1a57b" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="7" OBJ_ADDR="263936">
						<Object Name="CobraNet Transmit" Address="263936" ClassID="7" Version="1" HiQnetObjectKey="725c1ae6-4c49-4b7b-9bf1-6c56e46376c7">
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="0">
								<StateVariable Name="TxA Bundle" ID="0" HiQnetStateVariableKey="3c4e8b3e-441f-4031-a30c-32befb40903d" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="1">
								<StateVariable Name="TxA Priority" ID="1" HiQnetStateVariableKey="7751c718-ef17-4a8d-a5a0-9398c7c97d54" ClassID="616" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="2">
								<StateVariable Name="TxA Position" ID="2" HiQnetStateVariableKey="6304f6e9-f009-4343-91dc-ba38a3096df7" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="3">
								<StateVariable Name="TxA Channel Receiver Count" ID="3" HiQnetStateVariableKey="7465466a-9229-43c4-b657-ef96aeb65004" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="4">
								<StateVariable Name="TxB Bundle" ID="4" HiQnetStateVariableKey="ade1f7bf-6263-4b0f-ba3d-fe2e1fc8979c" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="5">
								<StateVariable Name="TxB Priority" ID="5" HiQnetStateVariableKey="9a9ae94b-fad1-434f-8c4f-db081556c590" ClassID="616" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="6">
								<StateVariable Name="TxB Position" ID="6" HiQnetStateVariableKey="4026e28c-6456-47e2-a3f7-1a7d2822ca73" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="7">
								<StateVariable Name="TxB Channel Receiver Count" ID="7" HiQnetStateVariableKey="b3e5bcb9-226e-4070-9fd4-b5953c9e1ef1" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="8">
								<StateVariable Name="TxC Bundle" ID="8" HiQnetStateVariableKey="638a9f53-bc29-4f93-96cf-aa74f2b409d6" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="9">
								<StateVariable Name="TxC Priority" ID="9" HiQnetStateVariableKey="e78142dc-bd17-4aac-9feb-958b22a3e969" ClassID="616" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="10">
								<StateVariable Name="TxC Position" ID="10" HiQnetStateVariableKey="51ae68c3-1819-4903-9a77-3b9edb2eff0d" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="11">
								<StateVariable Name="TxC Channel Receiver Count" ID="11" HiQnetStateVariableKey="d5f58104-8087-4f5b-86e8-bb6632c5451a" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="664" SV_ID="12">
								<StateVariable Name="TxD Bundle" ID="12" HiQnetStateVariableKey="94cd6f7d-fee7-451e-8784-de4c338976ae" ClassID="664" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>65279</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="13">
								<StateVariable Name="TxD Priority" ID="13" HiQnetStateVariableKey="576f6642-1cad-4572-af8e-58bee75a2255" ClassID="616" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="14">
								<StateVariable Name="TxD Position" ID="14" HiQnetStateVariableKey="f9be25a0-014a-4cda-a597-a15f70dd579e" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="15">
								<StateVariable Name="TxD Channel Receiver Count" ID="15" HiQnetStateVariableKey="908006cf-6031-4bdc-86b3-8692fc473ed4" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="16">
								<StateVariable Name="TxA Slot 1 Switched Output Channel Num" ID="16" HiQnetStateVariableKey="ae581eda-8280-4f3d-85ed-5583cf5aa06b" ClassID="738" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="17">
								<StateVariable Name="TxA Slot 2 Switched Output Channel Num" ID="17" HiQnetStateVariableKey="c5218c03-34b3-4921-a13a-1b5599553878" ClassID="738" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="18">
								<StateVariable Name="TxA Slot 3 Switched Output Channel Num" ID="18" HiQnetStateVariableKey="d91c7bd0-8363-4c74-aec2-0d85f833c103" ClassID="738" Version="1" DefaultValue="3">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="19">
								<StateVariable Name="TxA Slot 4 Switched Output Channel Num" ID="19" HiQnetStateVariableKey="74c37cb8-5fc0-4fe3-93f4-a252e590405c" ClassID="738" Version="1" DefaultValue="4">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="20">
								<StateVariable Name="TxA Slot 5 Switched Output Channel Num" ID="20" HiQnetStateVariableKey="e581cd33-6542-44cb-b553-f172497ee5de" ClassID="738" Version="1" DefaultValue="5">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="21">
								<StateVariable Name="TxA Slot 6 Switched Output Channel Num" ID="21" HiQnetStateVariableKey="945bd45a-9c4c-4786-bd22-f6756ce643da" ClassID="738" Version="1" DefaultValue="6">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="22">
								<StateVariable Name="TxA Slot 7 Switched Output Channel Num" ID="22" HiQnetStateVariableKey="5474d630-990c-4fa2-824a-a3f22b0c2beb" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="23">
								<StateVariable Name="TxA Slot 8 Switched Output Channel Num" ID="23" HiQnetStateVariableKey="9a65998d-5c42-461e-b051-3dcc53660aaf" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="24">
								<StateVariable Name="TxB Slot 1 Switched Output Channel Num" ID="24" HiQnetStateVariableKey="18673677-2354-49d8-a0e9-562f98f504c1" ClassID="738" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="25">
								<StateVariable Name="TxB Slot 2 Switched Output Channel Num" ID="25" HiQnetStateVariableKey="aec70439-afd3-42d5-8844-5c2eea61facd" ClassID="738" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="26">
								<StateVariable Name="TxB Slot 3 Switched Output Channel Num" ID="26" HiQnetStateVariableKey="2d0302d1-4b80-45f5-a5d4-d677c09f5732" ClassID="738" Version="1" DefaultValue="3">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="27">
								<StateVariable Name="TxB Slot 4 Switched Output Channel Num" ID="27" HiQnetStateVariableKey="972d11c8-6989-4d59-9353-6dfe42cc8ac5" ClassID="738" Version="1" DefaultValue="4">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="28">
								<StateVariable Name="TxB Slot 5 Switched Output Channel Num" ID="28" HiQnetStateVariableKey="2bf59a7c-b250-44e8-a049-a8fec233af0d" ClassID="738" Version="1" DefaultValue="5">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="29">
								<StateVariable Name="TxB Slot 6 Switched Output Channel Num" ID="29" HiQnetStateVariableKey="979965c7-fc62-4653-86d4-83a0561b3649" ClassID="738" Version="1" DefaultValue="6">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="30">
								<StateVariable Name="TxB Slot 7 Switched Output Channel Num" ID="30" HiQnetStateVariableKey="96685e38-073f-4ab9-a36b-d9e78059fcb8" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="31">
								<StateVariable Name="TxB Slot 8 Switched Output Channel Num" ID="31" HiQnetStateVariableKey="0fad6a57-88b3-4b5a-bd88-410b9c852181" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="32">
								<StateVariable Name="TxC Slot 1 Switched Output Channel Num" ID="32" HiQnetStateVariableKey="f5de7b3c-c27b-4d37-a9f7-862905127b29" ClassID="738" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="33">
								<StateVariable Name="TxC Slot 2 Switched Output Channel Num" ID="33" HiQnetStateVariableKey="286dd3f0-e108-43b3-87f2-5040ced67420" ClassID="738" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="34">
								<StateVariable Name="TxC Slot 3 Switched Output Channel Num" ID="34" HiQnetStateVariableKey="14c2ad88-d938-4f2c-a2d5-0cd3b07f0bd3" ClassID="738" Version="1" DefaultValue="3">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="35">
								<StateVariable Name="TxC Slot 4 Switched Output Channel Num" ID="35" HiQnetStateVariableKey="b9d9e626-896c-4760-a06b-96c2e0a2a4f5" ClassID="738" Version="1" DefaultValue="4">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="36">
								<StateVariable Name="TxC Slot 5 Switched Output Channel Num" ID="36" HiQnetStateVariableKey="305f54e5-72a6-4fe7-aa81-d39a5e50d9b2" ClassID="738" Version="1" DefaultValue="5">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="37">
								<StateVariable Name="TxC Slot 6 Switched Output Channel Num" ID="37" HiQnetStateVariableKey="d6da947f-27f9-4836-ac79-a4b9b54c1394" ClassID="738" Version="1" DefaultValue="6">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="38">
								<StateVariable Name="TxC Slot 7 Switched Output Channel Num" ID="38" HiQnetStateVariableKey="cb561e33-4e09-4547-9a92-c43919c73b2c" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="39">
								<StateVariable Name="TxC Slot 8 Switched Output Channel Num" ID="39" HiQnetStateVariableKey="8fc2ad0a-8dbe-4e2b-892c-2fbc3fe8c5a9" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="40">
								<StateVariable Name="TxD Slot 1 Switched Output Channel Num" ID="40" HiQnetStateVariableKey="05b15306-5552-4c14-a584-84f2779786b9" ClassID="738" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>6</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="41">
								<StateVariable Name="TxD Slot 2 Switched Output Channel Num" ID="41" HiQnetStateVariableKey="41f8a96e-79e6-483c-a45f-e3b891a14553" ClassID="738" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>6</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="42">
								<StateVariable Name="TxD Slot 3 Switched Output Channel Num" ID="42" HiQnetStateVariableKey="f07ed01e-bbbe-49d8-8a56-41919b17264a" ClassID="738" Version="1" DefaultValue="3">
									<Min>0</Min>
									<Max>6</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="43">
								<StateVariable Name="TxD Slot 4 Switched Output Channel Num" ID="43" HiQnetStateVariableKey="803737c4-73d9-4268-ab8e-bd6e3ae9511b" ClassID="738" Version="1" DefaultValue="4">
									<Min>0</Min>
									<Max>6</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="44">
								<StateVariable Name="TxD Slot 5 Switched Output Channel Num" ID="44" HiQnetStateVariableKey="8d458913-7046-479e-94ed-ec84233ec4c0" ClassID="738" Version="1" DefaultValue="5">
									<Min>0</Min>
									<Max>6</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="45">
								<StateVariable Name="TxD Slot 6 Switched Output Channel Num" ID="45" HiQnetStateVariableKey="f8d8eb5b-bc78-43d1-80a6-fdb56c57c175" ClassID="738" Version="1" DefaultValue="6">
									<Min>0</Min>
									<Max>6</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="46">
								<StateVariable Name="TxD Slot 7 Switched Output Channel Num" ID="46" HiQnetStateVariableKey="3694fe2d-4081-4de7-955b-403317252378" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="738" SV_ID="47">
								<StateVariable Name="TxD Slot 8 Switched Output Channel Num" ID="47" HiQnetStateVariableKey="3021acc6-e443-489d-a4f9-209d9e3b2236" ClassID="738" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="48">
								<StateVariable Name="Output 1 Meter" ID="48" HiQnetStateVariableKey="89ba38de-e83f-4d92-adc9-b7d60861f002" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="49">
								<StateVariable Name="Output 2 Meter" ID="49" HiQnetStateVariableKey="40cfa616-8ee8-4521-8046-cc99b37a8050" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="50">
								<StateVariable Name="Output 3 Meter" ID="50" HiQnetStateVariableKey="9b78b1f3-f1bb-4fa1-8d69-32fbab21ffe3" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="51">
								<StateVariable Name="Output 4 Meter" ID="51" HiQnetStateVariableKey="7a919e89-9459-4dc2-9777-06933da2bd8b" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="52">
								<StateVariable Name="TxA Slot 1 Channel Information" ID="52" HiQnetStateVariableKey="eab87471-e80d-4f84-a272-3d936bbefa0d" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="53">
								<StateVariable Name="TxA Slot 2 Channel Information" ID="53" HiQnetStateVariableKey="def80253-2748-435c-a96a-75d6f4672a09" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="54">
								<StateVariable Name="TxA Slot 3 Channel Information" ID="54" HiQnetStateVariableKey="a15689b1-6b16-436d-adc1-2ee321cd407b" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="55">
								<StateVariable Name="TxA Slot 4 Channel Information" ID="55" HiQnetStateVariableKey="3fd5a1b1-64a3-4059-841b-1482a0208044" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="56">
								<StateVariable Name="TxA Slot 5 Channel Information" ID="56" HiQnetStateVariableKey="d71fd539-8be6-4718-8805-2126fc6a6631" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="57">
								<StateVariable Name="TxA Slot 6 Channel Information" ID="57" HiQnetStateVariableKey="b1d0751a-7a2a-4e64-8ac8-a91bdd88339c" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="58">
								<StateVariable Name="TxA Slot 7 Channel Information" ID="58" HiQnetStateVariableKey="79a39195-b82d-45cb-a637-57d77ef82d2c" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="59">
								<StateVariable Name="TxA Slot 8 Channel Information" ID="59" HiQnetStateVariableKey="59545a01-6e7e-415c-af94-cf27fefdd571" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="60">
								<StateVariable Name="TxB Slot 1 Channel Information" ID="60" HiQnetStateVariableKey="bc1ce7cb-63a5-42dc-a53d-ba2979d3a08c" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="61">
								<StateVariable Name="TxB Slot 2 Channel Information" ID="61" HiQnetStateVariableKey="a31347c3-811c-4864-844a-9e915db23b25" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="62">
								<StateVariable Name="TxB Slot 3 Channel Information" ID="62" HiQnetStateVariableKey="7ffbfb51-2df6-4bf2-b8d5-0eb4f78788db" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="63">
								<StateVariable Name="TxB Slot 4 Channel Information" ID="63" HiQnetStateVariableKey="bde454c6-d92d-4e41-8fb4-5d5c81c777ed" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="64">
								<StateVariable Name="TxB Slot 5 Channel Information" ID="64" HiQnetStateVariableKey="e282fd7a-101b-40d0-8e1c-084236608899" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="65">
								<StateVariable Name="TxB Slot 6 Channel Information" ID="65" HiQnetStateVariableKey="845bdcc6-581b-4aea-ad40-be4e78cfef43" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="66">
								<StateVariable Name="TxB Slot 7 Channel Information" ID="66" HiQnetStateVariableKey="d2b4b78e-6c63-477e-93ee-24ae586a8cae" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="67">
								<StateVariable Name="TxB Slot 8 Channel Information" ID="67" HiQnetStateVariableKey="c6041fb2-26ce-41a0-8835-115d92e2513d" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="68">
								<StateVariable Name="TxC Slot 1 Channel Information" ID="68" HiQnetStateVariableKey="925b64ac-177e-436e-a172-1141dfdeb08c" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="69">
								<StateVariable Name="TxC Slot 2 Channel Information" ID="69" HiQnetStateVariableKey="f2fdccad-4de5-4b10-939e-bf0f72c7bcec" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="70">
								<StateVariable Name="TxC Slot 3 Channel Information" ID="70" HiQnetStateVariableKey="edd6c230-e979-40d0-a703-294ff08dbd93" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="71">
								<StateVariable Name="TxC Slot 4 Channel Information" ID="71" HiQnetStateVariableKey="f700cd69-a89e-4458-b693-7620467fb39a" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="72">
								<StateVariable Name="TxC Slot 5 Channel Information" ID="72" HiQnetStateVariableKey="0d6e5215-51fd-48b8-a400-732974023e55" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="73">
								<StateVariable Name="TxC Slot 6 Channel Information" ID="73" HiQnetStateVariableKey="47c4fd98-b0ee-4fb0-aa71-ec20bbe91449" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="74">
								<StateVariable Name="TxC Slot 7 Channel Information" ID="74" HiQnetStateVariableKey="bfb80a36-1bb5-4117-8d3a-f46423602c9e" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="75">
								<StateVariable Name="TxC Slot 8 Channel Information" ID="75" HiQnetStateVariableKey="b764e725-9b23-4c7c-b1ed-9857b0ffa609" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="76">
								<StateVariable Name="TxD Slot 1 Channel Information" ID="76" HiQnetStateVariableKey="74e20f09-7d94-4bb4-a21f-a91f26a3ac42" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="77">
								<StateVariable Name="TxD Slot 2 Channel Information" ID="77" HiQnetStateVariableKey="2fdaecf8-8388-4d0a-9478-460c9c0a27fb" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="78">
								<StateVariable Name="TxD Slot 3 Channel Information" ID="78" HiQnetStateVariableKey="211f677b-5cce-470f-9eed-99b448f6d913" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="79">
								<StateVariable Name="TxD Slot 4 Channel Information" ID="79" HiQnetStateVariableKey="0aa56711-eab3-4d4f-913e-dc7ec78ced2e" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="80">
								<StateVariable Name="TxD Slot 5 Channel Information" ID="80" HiQnetStateVariableKey="30693b9b-eace-4c53-ae39-a09a5aff0df0" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="81">
								<StateVariable Name="TxD Slot 6 Channel Information" ID="81" HiQnetStateVariableKey="19db62d1-adf2-4b86-a007-67f468d15ace" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="82">
								<StateVariable Name="TxD Slot 7 Channel Information" ID="82" HiQnetStateVariableKey="a51665f2-8533-4eaf-9d68-a923b05e9168" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="83">
								<StateVariable Name="TxD Slot 8 Channel Information" ID="83" HiQnetStateVariableKey="6b8cd3fb-adae-4199-9e7d-2ba9ead67b9f" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="12" OBJ_ADDR="330753">
						<Object Name="Ch 1 Input Router" Address="330753" ClassID="12" Version="1" HiQnetObjectKey="3316f8c2-6160-49cf-a2cd-2cf8cb36a3f8">
							<STATE_VARIABLE SV_CLASSID="734" SV_ID="0">
								<StateVariable Name="Mode" ID="0" HiQnetStateVariableKey="5f8d280c-a670-409a-8d29-06adf30d2527" ClassID="734" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>3</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="735" SV_ID="1">
								<StateVariable Name="Analog Source" ID="1" HiQnetStateVariableKey="25ba45f5-1de7-466c-b48e-bb02402232fe" ClassID="735" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="736" SV_ID="2">
								<StateVariable Name="Digital Source" ID="2" HiQnetStateVariableKey="267ccefa-753f-420e-89f7-2e9f556b20bf" ClassID="736" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="748" SV_ID="3">
								<StateVariable Name="AES Source" ID="3" HiQnetStateVariableKey="0fb1b596-aa10-495e-9f29-7fd1e6fdc7ab" ClassID="748" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="749" SV_ID="4">
								<StateVariable Name="CobraNet Source" ID="4" HiQnetStateVariableKey="09efb671-24fe-4495-8d72-f3284e6f0a4a" ClassID="749" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Analog Signal Detector Threshold" ID="5" HiQnetStateVariableKey="c04f0b5e-2b9f-4772-b992-cd92639c615e" ClassID="546" Version="1" DefaultValue="140">
									<Min>80</Min>
									<Max>200</Max>
									<Value>140</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Analog Signal Detector Hold Time" ID="6" HiQnetStateVariableKey="e5aeb5ff-0654-4939-a6ee-352cb5941e6c" ClassID="733" Version="1" DefaultValue="10">
									<Min>0</Min>
									<Max>60</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="7">
								<StateVariable Name="Analog Signal Detector Status" ID="7" HiQnetStateVariableKey="2f542409-c26d-4b31-82c9-789ce65f8e41" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Digital Source Status" ID="8" HiQnetStateVariableKey="26d7c42a-125e-4db9-8a3f-68ee8cf66ee0" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Mute" ID="9" HiQnetStateVariableKey="e2548652-d64e-40d5-9357-2a1282d8f723" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="10">
								<StateVariable Name="Fader" ID="10" HiQnetStateVariableKey="9465fbcf-9670-4a78-aa6e-977a5b54627b" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Invert" ID="11" HiQnetStateVariableKey="8c6d5e26-3928-4c19-bfe8-35bf5f24fd68" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="12">
								<StateVariable Name="Peak Level Meter" ID="12" HiQnetStateVariableKey="ea726457-8b42-4ffa-85f9-9100869dd9a1" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="13">
								<StateVariable Name="RMS Level Meter" ID="13" HiQnetStateVariableKey="2178c281-5c6b-45d4-b7e4-05f5cc6332f2" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="14">
								<StateVariable Name="Clip Indicator" ID="14" HiQnetStateVariableKey="11cf06cb-29fa-4479-af7d-a4cb407af6ca" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="15">
								<StateVariable Name="Signal Generator Fader" ID="15" HiQnetStateVariableKey="3dcaa90d-c738-4574-b4e6-9c228d68cda5" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="16">
								<StateVariable Name="Signal Generator Mute" ID="16" HiQnetStateVariableKey="7f8ec197-89eb-48ef-8418-49e3e7187c20" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="17">
								<StateVariable Name="Low Priority Input" ID="17" HiQnetStateVariableKey="9468ffcb-90da-4b5c-a6aa-9459e4bbf92e" ClassID="787" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>9</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="18">
								<StateVariable Name="Medium Priority Input" ID="18" HiQnetStateVariableKey="ee2d6967-c809-4caf-824a-af4b54ff45be" ClassID="787" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>9</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="19">
								<StateVariable Name="High Priority Input" ID="19" HiQnetStateVariableKey="9f55086a-cc59-457b-bc3f-2859c434f5ec" ClassID="787" Version="1" DefaultValue="4">
									<Min>0</Min>
									<Max>9</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="20">
								<StateVariable Name="Analog Input 1 Fader" ID="20" HiQnetStateVariableKey="e2307d21-64a7-48f9-9175-62f6af4e7c4a" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="21">
								<StateVariable Name="Analog Input 2 Fader" ID="21" HiQnetStateVariableKey="f1d98f1c-df4e-4090-b3b7-ce761dae9be5" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="22">
								<StateVariable Name="AES Input 1 Fader" ID="22" HiQnetStateVariableKey="3fd6b6f8-2874-449e-8930-29d68052a841" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="AES Input 2 Fader" ID="23" HiQnetStateVariableKey="9b1472aa-2b80-4a64-ac63-dcb49abf9652" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="24">
								<StateVariable Name="Cobranet Input 1 Fader" ID="24" HiQnetStateVariableKey="7dab0676-5fe7-4fd2-9327-0f174c1de5ca" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="25">
								<StateVariable Name="Cobranet Input 2 Fader" ID="25" HiQnetStateVariableKey="5f96efc1-268c-471a-829b-aa9dd44674df" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="26">
								<StateVariable Name="Analog Input 1 Depth Of Cut" ID="26" HiQnetStateVariableKey="bb20f6a2-99c3-476a-82aa-de1b93430133" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="27">
								<StateVariable Name="Analog Input 2 Depth Of Cut" ID="27" HiQnetStateVariableKey="6ebd2ccd-e028-4f33-a5e3-357d38d21aa2" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="28">
								<StateVariable Name="AES Input 1 Depth Of Cut" ID="28" HiQnetStateVariableKey="d9297c03-0733-43c3-850e-31ae5223b84d" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="29">
								<StateVariable Name="AES Input 2 Depth Of Cut" ID="29" HiQnetStateVariableKey="4a76cd36-1e1e-4f6f-a2e8-9466c7259800" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Cobranet Input 1 Depth Of Cut" ID="30" HiQnetStateVariableKey="d1e8adb9-d16a-4667-b029-595600386d11" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Cobranet Input 2 Depth Of Cut" ID="31" HiQnetStateVariableKey="be8783dd-be61-410e-918c-2ef3c4a5379a" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Analog Input 1 Attack" ID="32" HiQnetStateVariableKey="5324b235-6005-4e4d-834f-e9905fbff8d1" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Analog Input 2 Attack" ID="33" HiQnetStateVariableKey="91706b67-7b4d-4d50-814d-9621366aae2d" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="34">
								<StateVariable Name="AES Input 1 Attack" ID="34" HiQnetStateVariableKey="684af2e4-9ad5-44bd-9f76-013155313b8d" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="35">
								<StateVariable Name="AES Input 2 Attack" ID="35" HiQnetStateVariableKey="cd41202b-27a6-4fc4-af54-8de40d5dcc0a" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="36">
								<StateVariable Name="Cobranet Input 1 Attack" ID="36" HiQnetStateVariableKey="dc9af268-db3d-4f89-aae0-b47055869203" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="37">
								<StateVariable Name="Cobranet Input 2 Attack" ID="37" HiQnetStateVariableKey="642fffd8-61ce-44e6-90b0-a454ad72540a" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="38">
								<StateVariable Name="Analog Input 1 Release" ID="38" HiQnetStateVariableKey="c56e25ee-3c2a-4257-9e6a-42e9bab18a64" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="39">
								<StateVariable Name="Analog Input 2 Release" ID="39" HiQnetStateVariableKey="5bbcbbef-7091-45a4-b503-82efd5ac76f9" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="40">
								<StateVariable Name="AES Input 1 Release" ID="40" HiQnetStateVariableKey="ddc2638c-9355-4807-a33a-c8ca8a6bec27" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="41">
								<StateVariable Name="AES Input 2 Release" ID="41" HiQnetStateVariableKey="9aba2a0e-e11e-4d55-ad94-7460cdacb063" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="42">
								<StateVariable Name="Cobranet Input 1 Release" ID="42" HiQnetStateVariableKey="875c52ea-3253-47be-a9dc-d8aceb30bf09" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="43">
								<StateVariable Name="Cobranet Input 2 Release" ID="43" HiQnetStateVariableKey="98d752ff-f6cd-42a2-a7e2-b91639b74bd9" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="44">
								<StateVariable Name="Analog Input 1 Gain Meter" ID="44" HiQnetStateVariableKey="573814e4-f7a9-4f56-a818-d7bca430bf7c" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="45">
								<StateVariable Name="Analog Input 2 Gain Meter" ID="45" HiQnetStateVariableKey="3f69f770-b2e2-4eac-afb2-39b5a29ce170" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="46">
								<StateVariable Name="AES Input 1 Gain Meter" ID="46" HiQnetStateVariableKey="1f866bba-f3a4-432c-ad86-45c6e3894cfe" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="47">
								<StateVariable Name="AES Input 2 Gain Meter" ID="47" HiQnetStateVariableKey="483d0225-f87e-4d05-a3db-39c3ce0dd801" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="48">
								<StateVariable Name="Cobranet Input 1 Gain Meter" ID="48" HiQnetStateVariableKey="f21c8365-2d6c-4c25-b94a-59d0769e858a" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="49">
								<StateVariable Name="Cobranet Input 2 Gain Meter" ID="49" HiQnetStateVariableKey="c515de02-0165-4e97-a49b-1981cd23e7e5" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="788" SV_ID="50">
								<StateVariable Name="Priority Input Status" ID="50" HiQnetStateVariableKey="7c22c3a3-580c-4aea-84d4-bb736f50a0a4" ClassID="788" Version="1" DefaultValue="3">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="800" SV_ID="51">
								<StateVariable Name="Sum To Mono Detector Mode" ID="51" HiQnetStateVariableKey="da3250b5-bb94-4798-9e7f-e614ef06b960" ClassID="800" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="12" OBJ_ADDR="330754">
						<Object Name="Ch 2 Input Router" Address="330754" ClassID="12" Version="1" HiQnetObjectKey="4530ae10-2464-4afb-9074-043b6b412b6d">
							<STATE_VARIABLE SV_CLASSID="734" SV_ID="0">
								<StateVariable Name="Mode" ID="0" HiQnetStateVariableKey="516a3d1a-2ad3-45b1-9efa-71dd74d8ec7a" ClassID="734" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>3</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="735" SV_ID="1">
								<StateVariable Name="Analog Source" ID="1" HiQnetStateVariableKey="7218ebf2-37e8-4caf-a065-b084729708d0" ClassID="735" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="736" SV_ID="2">
								<StateVariable Name="Digital Source" ID="2" HiQnetStateVariableKey="20597c6c-ae84-4e2b-9d7a-fc4f4b76257a" ClassID="736" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="748" SV_ID="3">
								<StateVariable Name="AES Source" ID="3" HiQnetStateVariableKey="2581e486-b0df-4414-b0cd-030aeae7c7db" ClassID="748" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="749" SV_ID="4">
								<StateVariable Name="CobraNet Source" ID="4" HiQnetStateVariableKey="82db7d5d-d9c4-46aa-abcb-f675e1469978" ClassID="749" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Analog Signal Detector Threshold" ID="5" HiQnetStateVariableKey="9197c5e6-7960-49b6-b5c9-481e912af77b" ClassID="546" Version="1" DefaultValue="140">
									<Min>80</Min>
									<Max>200</Max>
									<Value>140</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Analog Signal Detector Hold Time" ID="6" HiQnetStateVariableKey="8a458df3-a651-4300-82c0-0492a4e57751" ClassID="733" Version="1" DefaultValue="10">
									<Min>0</Min>
									<Max>60</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="7">
								<StateVariable Name="Analog Signal Detector Status" ID="7" HiQnetStateVariableKey="2f22a6e2-b3e7-4ce0-b485-ad160a7ef0af" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Digital Source Status" ID="8" HiQnetStateVariableKey="569a35ce-1229-4af4-808b-d8f37a18c213" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Mute" ID="9" HiQnetStateVariableKey="c0488e3e-e578-4d2f-9f66-7e685de09137" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="10">
								<StateVariable Name="Fader" ID="10" HiQnetStateVariableKey="93785291-9190-421a-ade3-606a2f07f87c" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Invert" ID="11" HiQnetStateVariableKey="63c93d41-563f-4108-8250-f426d7c059ef" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="12">
								<StateVariable Name="Peak Level Meter" ID="12" HiQnetStateVariableKey="b7b14d04-0f29-464a-8ba9-c9e5dada181e" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="13">
								<StateVariable Name="RMS Level Meter" ID="13" HiQnetStateVariableKey="9f4fe69a-1d6b-4aad-a3e9-3871986b3a7d" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="14">
								<StateVariable Name="Clip Indicator" ID="14" HiQnetStateVariableKey="05fb248b-9b87-45bf-83bd-2c70ceb15e3a" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="15">
								<StateVariable Name="Signal Generator Fader" ID="15" HiQnetStateVariableKey="7f03abda-425d-43ab-b508-869e45a706d2" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="16">
								<StateVariable Name="Signal Generator Mute" ID="16" HiQnetStateVariableKey="d1334dbd-1541-4f20-a9ea-f58e8419ce09" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="17">
								<StateVariable Name="Low Priority Input" ID="17" HiQnetStateVariableKey="c7d44186-eef6-423e-9c07-7617ee208063" ClassID="787" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>9</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="18">
								<StateVariable Name="Medium Priority Input" ID="18" HiQnetStateVariableKey="0d395ef0-559d-4620-b20d-9490882be058" ClassID="787" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>9</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="787" SV_ID="19">
								<StateVariable Name="High Priority Input" ID="19" HiQnetStateVariableKey="a174c49e-986a-4020-b725-4e24c72b5d80" ClassID="787" Version="1" DefaultValue="5">
									<Min>0</Min>
									<Max>9</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="20">
								<StateVariable Name="Analog Input 1 Fader" ID="20" HiQnetStateVariableKey="3236747f-823f-4a95-b62e-770162a93d24" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="21">
								<StateVariable Name="Analog Input 2 Fader" ID="21" HiQnetStateVariableKey="cc441351-6161-47bd-9754-ddaf2c43ad95" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="22">
								<StateVariable Name="AES Input 1 Fader" ID="22" HiQnetStateVariableKey="2e30bc1c-31e9-4498-a98f-1dfb323fa0a8" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="AES Input 2 Fader" ID="23" HiQnetStateVariableKey="a35f999a-ba8f-4b5d-93c0-9bce74d447b1" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="24">
								<StateVariable Name="Cobranet Input 1 Fader" ID="24" HiQnetStateVariableKey="f681a1bb-6b27-4912-aa8d-be750d1d3510" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="25">
								<StateVariable Name="Cobranet Input 2 Fader" ID="25" HiQnetStateVariableKey="866561d4-900b-4fb6-86ca-75efe325f26d" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="26">
								<StateVariable Name="Analog Input 1 Depth Of Cut" ID="26" HiQnetStateVariableKey="fc384b43-8cdf-4d2b-a77a-d1e791ccc3f5" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="27">
								<StateVariable Name="Analog Input 2 Depth Of Cut" ID="27" HiQnetStateVariableKey="42e001eb-fc19-4690-9eb6-423aaa70cc12" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="28">
								<StateVariable Name="AES Input 1 Depth Of Cut" ID="28" HiQnetStateVariableKey="f774f7fe-3eda-4ee8-9617-9bdd7eb0b68a" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="29">
								<StateVariable Name="AES Input 2 Depth Of Cut" ID="29" HiQnetStateVariableKey="43be36e1-c982-4648-a218-2ace01f30f93" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="30">
								<StateVariable Name="Cobranet Input 1 Depth Of Cut" ID="30" HiQnetStateVariableKey="cc486ef9-3365-4fb1-920c-9ab699498808" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="31">
								<StateVariable Name="Cobranet Input 2 Depth Of Cut" ID="31" HiQnetStateVariableKey="2adfc5e7-debf-4957-acd5-746f2c75f852" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>200</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="32">
								<StateVariable Name="Analog Input 1 Attack" ID="32" HiQnetStateVariableKey="ad432d9a-0be6-477a-8270-6a44db85a3f5" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="33">
								<StateVariable Name="Analog Input 2 Attack" ID="33" HiQnetStateVariableKey="d9cf3971-3e7f-4b48-bfcc-e8f4eef01d20" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="34">
								<StateVariable Name="AES Input 1 Attack" ID="34" HiQnetStateVariableKey="f8a12a77-3bd2-4616-85d4-a0991962b966" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="35">
								<StateVariable Name="AES Input 2 Attack" ID="35" HiQnetStateVariableKey="229f7c78-6931-4457-843a-589c6705cb5e" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="36">
								<StateVariable Name="Cobranet Input 1 Attack" ID="36" HiQnetStateVariableKey="d8ab63d1-6542-469f-868c-6c6fdaeb07e9" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="37">
								<StateVariable Name="Cobranet Input 2 Attack" ID="37" HiQnetStateVariableKey="f089ef1d-1e36-46b8-8552-9e72d28934e2" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="38">
								<StateVariable Name="Analog Input 1 Release" ID="38" HiQnetStateVariableKey="e1dde193-c438-4e47-8136-988d1416a5fa" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="39">
								<StateVariable Name="Analog Input 2 Release" ID="39" HiQnetStateVariableKey="5d6dd43f-8ea9-4ba6-af49-ff4316e01958" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="40">
								<StateVariable Name="AES Input 1 Release" ID="40" HiQnetStateVariableKey="dc034f32-4c38-43e1-951d-6d65fc4b2211" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="41">
								<StateVariable Name="AES Input 2 Release" ID="41" HiQnetStateVariableKey="92330d81-babf-4b78-a478-99ae2948db28" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="42">
								<StateVariable Name="Cobranet Input 1 Release" ID="42" HiQnetStateVariableKey="984bccf0-5764-4ef0-80b1-2a4071162972" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="43">
								<StateVariable Name="Cobranet Input 2 Release" ID="43" HiQnetStateVariableKey="9821927d-7da2-45f3-856f-85f104f68dd6" ClassID="733" Version="1" DefaultValue="0.1">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="44">
								<StateVariable Name="Analog Input 1 Gain Meter" ID="44" HiQnetStateVariableKey="dfb4b20d-51e0-49fb-880b-5569ce62bc6c" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="45">
								<StateVariable Name="Analog Input 2 Gain Meter" ID="45" HiQnetStateVariableKey="14a48ce3-49b5-48f2-8dc1-c90b487f6348" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="46">
								<StateVariable Name="AES Input 1 Gain Meter" ID="46" HiQnetStateVariableKey="9e599b73-7391-4301-aca6-a1d58fbe6e75" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="47">
								<StateVariable Name="AES Input 2 Gain Meter" ID="47" HiQnetStateVariableKey="bc2f33cb-4cb6-4667-95c8-877ac3f717c6" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="48">
								<StateVariable Name="Cobranet Input 1 Gain Meter" ID="48" HiQnetStateVariableKey="2b6898ed-c4b5-4964-a443-dfba140e0145" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="49">
								<StateVariable Name="Cobranet Input 2 Gain Meter" ID="49" HiQnetStateVariableKey="5844520d-a8a0-487e-a20c-2f5216d52e49" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">8A==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="788" SV_ID="50">
								<StateVariable Name="Priority Input Status" ID="50" HiQnetStateVariableKey="a0b4124e-abfb-4be2-af4f-bd5388d0f986" ClassID="788" Version="1" DefaultValue="3">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="800" SV_ID="51">
								<StateVariable Name="Sum To Mono Detector Mode" ID="51" HiQnetStateVariableKey="86b32fe0-cacf-45f9-9b64-090f7bfcb315" ClassID="800" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="13" OBJ_ADDR="396545">
						<Object Name="Ch 1 Input Compressor" Address="396545" ClassID="13" Version="1" HiQnetObjectKey="0bb22b21-2d9f-41d7-bd7f-dbf38c57cf2d">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="ab117e55-5f4f-4d44-a16f-7837d10effe0" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" HiQnetStateVariableKey="0885157a-3735-4064-a631-829abe7f54f5" ClassID="546" Version="1" DefaultValue="200">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" HiQnetStateVariableKey="fd4997b5-ce40-410a-bd7c-5555dcd68fa9" ClassID="733" Version="1" DefaultValue="4">
									<Min>2</Min>
									<Max>32</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" HiQnetStateVariableKey="f5ceb8a3-0ae1-4680-ba0f-224674bbd3ef" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>0.001</Min>
									<Max>0.1</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" HiQnetStateVariableKey="7e94db08-9e55-4419-a1ec-260622cfa85a" ClassID="733" Version="1" DefaultValue="1">
									<Min>0.01</Min>
									<Max>10</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Soft Knee Width" ID="5" HiQnetStateVariableKey="f0ec4450-7cf3-4322-8d60-8dbfbedf0c4e" ClassID="546" Version="1" DefaultValue="212">
									<Min>200</Min>
									<Max>224</Max>
									<Value>212</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="6">
								<StateVariable Name="Hysteresis" ID="6" HiQnetStateVariableKey="2e37489c-7747-4449-b4e2-80a5ebcce778" ClassID="546" Version="1" DefaultValue="206">
									<Data2 Len="1">yA==</Data2>
									<Data3 Len="1">4A==</Data3>
									<Data1 Len="1">zg==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Make Up Gain" ID="7" HiQnetStateVariableKey="76123da7-a605-4cee-90c3-7f52f1d4d41d" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>20</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="8">
								<StateVariable Name="Signal Status" ID="8" HiQnetStateVariableKey="eef7b8e1-399d-4bf3-81ce-47a26ca665ae" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" HiQnetStateVariableKey="a1749c1a-13f7-4b9c-8643-c534fbf1d00c" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="13" OBJ_ADDR="396546">
						<Object Name="Ch 2 Input Compressor" Address="396546" ClassID="13" Version="1" HiQnetObjectKey="19027206-c6de-4d4b-850c-b4359811b268">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="601aa883-9ce1-42da-8a00-de6b7aa7fde1" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" HiQnetStateVariableKey="b99d853b-ad7a-4e5c-828f-2d8ca47927f9" ClassID="546" Version="1" DefaultValue="200">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" HiQnetStateVariableKey="27d17135-e6ed-46bc-9b3c-d924a05b9532" ClassID="733" Version="1" DefaultValue="4">
									<Min>2</Min>
									<Max>32</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" HiQnetStateVariableKey="8a7da247-ea12-4da1-89f0-16c48b02a156" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>0.001</Min>
									<Max>0.1</Max>
									<Value>0.01</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" HiQnetStateVariableKey="672d7291-6d0d-4526-b669-b8ecd4a28eb1" ClassID="733" Version="1" DefaultValue="1">
									<Min>0.01</Min>
									<Max>10</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Soft Knee Width" ID="5" HiQnetStateVariableKey="511d6891-5ff0-442c-a08a-46b091d2e085" ClassID="546" Version="1" DefaultValue="212">
									<Min>200</Min>
									<Max>224</Max>
									<Value>212</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="6">
								<StateVariable Name="Hysteresis" ID="6" HiQnetStateVariableKey="98c113af-b8f8-44f4-87cf-7ca849f73f8d" ClassID="546" Version="1" DefaultValue="206">
									<Data2 Len="1">yA==</Data2>
									<Data3 Len="1">4A==</Data3>
									<Data1 Len="1">zg==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Make Up Gain" ID="7" HiQnetStateVariableKey="2cd0c05e-12e0-4346-b7cf-9c02f8018fa4" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>20</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="8">
								<StateVariable Name="Signal Status" ID="8" HiQnetStateVariableKey="6ff878d9-6ed5-42a6-8cd8-b80c35cd379f" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" HiQnetStateVariableKey="81e2d657-1d39-408e-903e-0fc842a99883" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="14" OBJ_ADDR="462337">
						<Object Name="Ch 1 TLC Compressor" Address="462337" ClassID="14" Version="1" HiQnetObjectKey="fe45f770-326b-465c-88b7-2adec75c6612">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="29be012e-fec2-471a-9332-1153f77e7997" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" HiQnetStateVariableKey="556fd04f-5338-422a-8ca0-f58cb832439c" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" HiQnetStateVariableKey="2b7608a3-2166-4ae6-89de-c979426b19cf" ClassID="733" Version="1" DefaultValue="100">
									<Data2 Len="4">AAAAQA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" HiQnetStateVariableKey="cc8cef6a-67b4-4dc5-8089-ecfc20a7bf1f" ClassID="733" Version="1" DefaultValue="0.01">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" HiQnetStateVariableKey="6d93e671-b215-428b-af9c-298ad0c4b540" ClassID="733" Version="1" DefaultValue="1">
									<Data2 Len="4">CtcjPA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Soft Knee Width" ID="5" HiQnetStateVariableKey="167946dc-4636-4617-9d38-3848c943fed6" ClassID="546" Version="1" DefaultValue="200">
									<Data2 Len="1">yA==</Data2>
									<Data3 Len="1">4A==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="6">
								<StateVariable Name="Hysteresis" ID="6" HiQnetStateVariableKey="693b7598-306a-46ac-8266-4b54d4ce59b1" ClassID="546" Version="1" DefaultValue="206">
									<Data2 Len="1">yA==</Data2>
									<Data3 Len="1">4A==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Make Up Gain" ID="7" HiQnetStateVariableKey="865b89c8-c177-48a1-919b-d269c0a6a696" ClassID="733" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="8">
								<StateVariable Name="Signal Status" ID="8" HiQnetStateVariableKey="1bfa4bfc-5781-42ea-8c7c-34e3213c9806" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" HiQnetStateVariableKey="56718363-6a84-478e-aa6e-88b333dbfd8b" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="10">
								<StateVariable Name="Detector Time Constant" ID="10" HiQnetStateVariableKey="88034da6-2bdf-462d-9e9f-fb5ab4346d9b" ClassID="733" Version="1" DefaultValue="0.1">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="14" OBJ_ADDR="462338">
						<Object Name="Ch 2 TLC Compressor" Address="462338" ClassID="14" Version="1" HiQnetObjectKey="8d3ba137-692f-42db-a4ad-7cede2b83f5d">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="55a8339b-5c03-4093-b794-669dd2e3bbfe" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" HiQnetStateVariableKey="dc91b5c6-02a9-4bc8-88e3-ee5a710e3479" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Ratio" ID="2" HiQnetStateVariableKey="522debb1-6c95-4b73-9ea9-bfca1b59cadf" ClassID="733" Version="1" DefaultValue="100">
									<Data2 Len="4">AAAAQA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" HiQnetStateVariableKey="54628e9d-391e-4118-ba95-15466f4aec64" ClassID="733" Version="1" DefaultValue="0.01">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" HiQnetStateVariableKey="15590229-23f7-4d8c-8071-dd1ecca14014" ClassID="733" Version="1" DefaultValue="1">
									<Data2 Len="4">CtcjPA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="5">
								<StateVariable Name="Soft Knee Width" ID="5" HiQnetStateVariableKey="4c0c956d-9436-4001-a833-3fc2c667e010" ClassID="546" Version="1" DefaultValue="200">
									<Data2 Len="1">yA==</Data2>
									<Data3 Len="1">4A==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="6">
								<StateVariable Name="Hysteresis" ID="6" HiQnetStateVariableKey="8a695c06-bf35-483d-842b-b7086a172e4a" ClassID="546" Version="1" DefaultValue="206">
									<Data2 Len="1">yA==</Data2>
									<Data3 Len="1">4A==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Make Up Gain" ID="7" HiQnetStateVariableKey="5a540b0e-11ae-424c-ba27-9a9a440cd072" ClassID="733" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="8">
								<StateVariable Name="Signal Status" ID="8" HiQnetStateVariableKey="1a3dfb72-6c93-4337-89c8-1435e21e1bc7" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="9">
								<StateVariable Name="Gain Meter" ID="9" HiQnetStateVariableKey="3b236903-b2c0-46da-8b14-f1e97c2a987e" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="10">
								<StateVariable Name="Detector Time Constant" ID="10" HiQnetStateVariableKey="5ffc87ec-e331-4ff9-974e-ada865586219" ClassID="733" Version="1" DefaultValue="0.1">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="529409">
						<Object Name="Ch1 Input Delay" Address="529409" ClassID="20" Version="1" HiQnetObjectKey="fd63f958-7812-4636-ad1a-d69af612785b">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" HiQnetStateVariableKey="99949862-8aeb-4586-aa36-ebd3408836b6" ClassID="562" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" HiQnetStateVariableKey="f24e4b3f-ee72-47e0-96fc-09d348948455" ClassID="561" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>0.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" HiQnetStateVariableKey="6cb5ed2b-c16c-4fc9-8163-c5aecf7e0122" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" HiQnetStateVariableKey="d7e8b838-5d6f-441e-82f7-7b60e75150ee" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="529410">
						<Object Name="Ch2 Input Delay" Address="529410" ClassID="20" Version="1" HiQnetObjectKey="b76678fb-68c1-4d90-bb91-b68316a9d0ed">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" HiQnetStateVariableKey="226a5353-69da-45d6-90d0-b6b4780925c0" ClassID="562" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" HiQnetStateVariableKey="86bf2117-f817-41fd-982c-ed46f525660f" ClassID="561" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>0.1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" HiQnetStateVariableKey="6d1ffe2e-3d09-4483-8222-964e0ab653ca" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" HiQnetStateVariableKey="db1428ac-83db-4ede-ae05-6c3969fea0f1" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="35" OBJ_ADDR="598785">
						<Object Name="Ch1 Input EQ Filters" Address="598785" ClassID="35" Version="1" HiQnetObjectKey="12778b2c-b6b0-4478-aef7-2493a10c800c">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" HiQnetStateVariableKey="5e575844-c322-4731-8e44-a52602d667a8" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" HiQnetStateVariableKey="e6033ca4-6959-434d-9116-e073deb08f20" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" HiQnetStateVariableKey="505fa357-d230-4c70-80b1-ca33658e97d2" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" HiQnetStateVariableKey="afe80122-f0c7-4b1e-9f28-1c23de4ecc46" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" HiQnetStateVariableKey="aaa9e795-9436-4501-bbb6-f85ce46d7f12" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" HiQnetStateVariableKey="21e022e8-fafb-4897-9793-8bd6ca0fcfaf" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" HiQnetStateVariableKey="bd168918-f12a-48c4-b8f2-d4cac8d44d40" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" HiQnetStateVariableKey="80116d03-b860-4206-8bb9-5d3f78f615ce" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" HiQnetStateVariableKey="41cd89c3-4719-4804-a757-524de73e6087" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" HiQnetStateVariableKey="eca9a06c-213c-48e5-a3bd-e84a087b26c0" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" HiQnetStateVariableKey="0b06ba7d-a333-44d1-b92c-4c36fe08fb15" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" HiQnetStateVariableKey="61c2de9f-6d20-49bf-b01d-1366cd93d49d" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" HiQnetStateVariableKey="d1c58f5f-b7e4-412f-9241-92cb060fa033" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" HiQnetStateVariableKey="66225192-b860-4c58-932e-6438d0268285" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" HiQnetStateVariableKey="abec689f-763d-4082-9952-6639626da0b1" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" HiQnetStateVariableKey="4ac08e23-a449-4444-8127-db8391f7ab51" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" HiQnetStateVariableKey="98e1a5bb-789c-4ebf-bb69-6ca5172cf20b" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" HiQnetStateVariableKey="4e90b7cf-b519-4dd5-98bb-d6fd20e48c59" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" HiQnetStateVariableKey="96b92982-b3fc-4c43-8899-6cd635aaeb4e" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" HiQnetStateVariableKey="1e00c32e-34f2-41ba-91fc-cfc52aaa8272" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" HiQnetStateVariableKey="257158f4-23b4-4fef-b9ee-1a7f839a5c0e" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" HiQnetStateVariableKey="4631ca68-f085-4016-b7f3-bd5c994c2ff7" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" HiQnetStateVariableKey="49570cc6-ae17-43b1-986e-73b61cc0a19b" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" HiQnetStateVariableKey="6c5185d1-62b5-40f7-aeeb-fd98dee54ada" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" HiQnetStateVariableKey="3d6fa333-0d7c-4a11-bd02-1a8ddb82743a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" HiQnetStateVariableKey="93b7df44-6c8f-4762-91ce-bc6c9b7a570c" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" HiQnetStateVariableKey="c3fc7a4b-2f6a-440d-8811-5d730c720642" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" HiQnetStateVariableKey="5caa402f-4844-4789-9758-b6f531938a00" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" HiQnetStateVariableKey="e0fd7f99-4033-4e87-8fb5-7aa9eed081fb" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" HiQnetStateVariableKey="eb216db5-4a16-4f85-9acb-89624f3332fc" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" HiQnetStateVariableKey="8e531682-79c0-4584-b204-e2dcd3223e26" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" HiQnetStateVariableKey="b092b1f3-6f9b-4a74-93f8-38feab8f420b" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" HiQnetStateVariableKey="0a0134cb-2136-4106-bcd5-425d2d48f1cc" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" HiQnetStateVariableKey="d7d43268-028d-4d1e-ae03-e60b3ead5279" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" HiQnetStateVariableKey="709f225f-7a31-4b00-9c15-22bebc97a1c7" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" HiQnetStateVariableKey="cefd3a6b-181c-44a5-aeba-6a818bf46740" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" HiQnetStateVariableKey="8ca80449-dce3-48f4-9582-e47ef3c336f3" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" HiQnetStateVariableKey="ed167d57-2f7b-43ea-8729-033528a75e10" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" HiQnetStateVariableKey="3954b672-50ee-447a-b97b-6c905d2b6b4a" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" HiQnetStateVariableKey="a3b99392-bf1a-40b1-96d2-f51104482441" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" HiQnetStateVariableKey="cd7c5614-fd9c-49b2-bb1e-0d67d3b4ede5" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" HiQnetStateVariableKey="1e137e36-92fc-492d-ae33-3f0988982279" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" HiQnetStateVariableKey="db95faf7-9211-4b5c-8f9c-0d4ffb515eb2" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" HiQnetStateVariableKey="eaaffb6b-acf2-4596-9550-2e54a4938d78" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" HiQnetStateVariableKey="31d569b8-8b6f-4312-b08a-cfd202f6ba5d" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" HiQnetStateVariableKey="1606ba1c-2e18-4b00-b439-6d1f5e3c5d47" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" HiQnetStateVariableKey="81d171cb-b529-44d4-ae1a-007ebe549cea" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" HiQnetStateVariableKey="419c8e0d-47da-476f-8056-dbdc56079e90" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Enable 9" ID="48" HiQnetStateVariableKey="ac22dddb-6052-4396-86f7-3218f803f1e1" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="49">
								<StateVariable Name="Frequency 9" ID="49" HiQnetStateVariableKey="7d96ccdf-f228-4584-a9f0-a3b2e80759d5" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="50">
								<StateVariable Name="Q 9" ID="50" HiQnetStateVariableKey="af9b7816-f7b7-4719-babe-c9b2763dba4a" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="51">
								<StateVariable Name="Slope 9" ID="51" HiQnetStateVariableKey="db2f2b63-f009-489a-9ce1-53a701e64577" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="52">
								<StateVariable Name="Gain 9" ID="52" HiQnetStateVariableKey="cafcbdac-5ba8-450e-b404-4c019892ba3e" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="53">
								<StateVariable Name="Type 9" ID="53" HiQnetStateVariableKey="ca8b3895-0ad4-464a-b311-96afa6810956" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="54">
								<StateVariable Name="Enable 10" ID="54" HiQnetStateVariableKey="8cde9c1f-9d39-4fe6-a913-0183fdbdb627" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="55">
								<StateVariable Name="Frequency 10" ID="55" HiQnetStateVariableKey="9607475a-e0c6-4d6e-be67-2b43db16c282" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="56">
								<StateVariable Name="Q 10" ID="56" HiQnetStateVariableKey="4b0710a5-db00-4477-99b3-b42e5b4db6a9" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="57">
								<StateVariable Name="Slope 10" ID="57" HiQnetStateVariableKey="d65c7453-5ca8-4252-a5a5-8767d93c0182" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="58">
								<StateVariable Name="Gain 10" ID="58" HiQnetStateVariableKey="490b85f0-5b9b-4efb-93a6-3e6eb1f42aef" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="59">
								<StateVariable Name="Type 10" ID="59" HiQnetStateVariableKey="16e65c4b-cee7-476c-a14c-f1a613ea7108" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="60">
								<StateVariable Name="Enable 11" ID="60" HiQnetStateVariableKey="f754fbd8-5324-4467-8005-269435c0fbdd" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="61">
								<StateVariable Name="Frequency 11" ID="61" HiQnetStateVariableKey="e04a8c1a-00fb-4c2c-9f57-a6e4a00ce648" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="62">
								<StateVariable Name="Q 11" ID="62" HiQnetStateVariableKey="0486930b-beb9-41ba-bca8-0d848a91976d" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="63">
								<StateVariable Name="Slope 11" ID="63" HiQnetStateVariableKey="c09be22c-0f27-42eb-863f-1671b943d3b4" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="64">
								<StateVariable Name="Gain 11" ID="64" HiQnetStateVariableKey="79702668-6459-4f79-b70d-bb36755d6602" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="65">
								<StateVariable Name="Type 11" ID="65" HiQnetStateVariableKey="688aec2c-1e18-4e93-8b3e-f8b7aab01d1b" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="66">
								<StateVariable Name="Enable 12" ID="66" HiQnetStateVariableKey="a5bcaef2-39a2-4e93-a3ff-c25360f178bb" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="67">
								<StateVariable Name="Frequency 12" ID="67" HiQnetStateVariableKey="abd1be4e-a516-4716-b590-69c86d871c53" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="68">
								<StateVariable Name="Q 12" ID="68" HiQnetStateVariableKey="73c9012f-2fa1-4638-97e4-783e40a6880c" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="69">
								<StateVariable Name="Slope 12" ID="69" HiQnetStateVariableKey="554c8afd-4581-42c1-beb5-1b00ef9b6498" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="70">
								<StateVariable Name="Gain 12" ID="70" HiQnetStateVariableKey="ee171660-22b8-4cab-8ac3-3d8d10ed6315" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="71">
								<StateVariable Name="Type 12" ID="71" HiQnetStateVariableKey="41d77fe1-dd4b-4c16-8686-5c6a19366fc8" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="72">
								<StateVariable Name="Enable 13" ID="72" HiQnetStateVariableKey="29416e1f-86ed-4c61-8665-47257b6ddb5a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="73">
								<StateVariable Name="Frequency 13" ID="73" HiQnetStateVariableKey="74db656d-5e18-4acf-b06a-c70839d01677" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="74">
								<StateVariable Name="Q 13" ID="74" HiQnetStateVariableKey="6edd6f42-1abb-499a-a182-d9fe5f060094" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="75">
								<StateVariable Name="Slope 13" ID="75" HiQnetStateVariableKey="4a525a29-48d8-41e4-979c-f33f381fbfdd" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="76">
								<StateVariable Name="Gain 13" ID="76" HiQnetStateVariableKey="0051ceb0-1862-4a8d-b1f5-1d9a7bb46393" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="77">
								<StateVariable Name="Type 13" ID="77" HiQnetStateVariableKey="eb69ae0b-66fe-414f-8d03-a1a6c66a4013" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="78">
								<StateVariable Name="Enable 14" ID="78" HiQnetStateVariableKey="764057b0-16c1-4c64-9d34-b3098ca46dd9" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="79">
								<StateVariable Name="Frequency 14" ID="79" HiQnetStateVariableKey="d69534b2-a7a8-40d1-8cd0-1f623aeb3b89" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="80">
								<StateVariable Name="Q 14" ID="80" HiQnetStateVariableKey="eb87d672-b0e8-4dbc-bac1-061f2261cd15" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="81">
								<StateVariable Name="Slope 14" ID="81" HiQnetStateVariableKey="06c87368-2f88-4889-833e-a857d2cb8b27" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="82">
								<StateVariable Name="Gain 14" ID="82" HiQnetStateVariableKey="31d303b6-754f-4c34-a724-430990e1bfe6" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="83">
								<StateVariable Name="Type 14" ID="83" HiQnetStateVariableKey="d640acd8-90f8-4532-a049-4d635eee8670" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="84">
								<StateVariable Name="Enable 15" ID="84" HiQnetStateVariableKey="3fdd20c7-1b26-42c0-875d-48778dd276fe" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="85">
								<StateVariable Name="Frequency 15" ID="85" HiQnetStateVariableKey="8e49ada3-4179-4d85-8e39-1195c7815ded" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="86">
								<StateVariable Name="Q 15" ID="86" HiQnetStateVariableKey="db6a102d-c244-4fa0-a764-2a22b3b9cc21" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="87">
								<StateVariable Name="Slope 15" ID="87" HiQnetStateVariableKey="2b0fe112-b5d8-46eb-9378-4ad324a60f02" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="88">
								<StateVariable Name="Gain 15" ID="88" HiQnetStateVariableKey="8b81abbe-de71-472f-a1d8-e4c5c7e50381" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="89">
								<StateVariable Name="Type 15" ID="89" HiQnetStateVariableKey="2c505287-142c-4dd3-b76c-f7e2cbd5fc23" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="90">
								<StateVariable Name="Enable 16" ID="90" HiQnetStateVariableKey="0fcd938b-9472-4656-ae5c-fab6c5da87d6" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="91">
								<StateVariable Name="Frequency 16" ID="91" HiQnetStateVariableKey="eab7a792-f051-442a-8e77-038d3ddafe63" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="92">
								<StateVariable Name="Q 16" ID="92" HiQnetStateVariableKey="3fafd105-cefd-4bbe-832d-da0a2157ca50" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="93">
								<StateVariable Name="Slope 16" ID="93" HiQnetStateVariableKey="58eebc34-e6d9-46ab-8000-2a564a776c80" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="94">
								<StateVariable Name="Gain 16" ID="94" HiQnetStateVariableKey="acb9916e-e011-4dbf-8579-cdd179b02c25" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="95">
								<StateVariable Name="Type 16" ID="95" HiQnetStateVariableKey="0258dd2c-e623-4e71-87d8-f30979e6b99a" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="96">
								<StateVariable Name="Bypass 1 Thru 8" ID="96" HiQnetStateVariableKey="ddb2d16a-ecf6-4848-8d84-18e13f4e10a4" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="97">
								<StateVariable Name="Bypass 9 Thru 16" ID="97" HiQnetStateVariableKey="c7aec5a2-b9b8-41db-bf68-e85b75a80c15" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="98">
								<StateVariable Name="Array Volume Control" ID="98" HiQnetStateVariableKey="f21d30c4-5d0d-4973-bae7-a837f9149153" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="35" OBJ_ADDR="598786">
						<Object Name="Ch2 Input EQ Filters" Address="598786" ClassID="35" Version="1" HiQnetObjectKey="f543cbbd-36c2-413d-b78b-960bda8e87c9">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" HiQnetStateVariableKey="b76e9c55-7765-47c9-b897-70ecf866860d" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" HiQnetStateVariableKey="af8dfe39-1e5b-4f74-989c-724a364b12d5" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" HiQnetStateVariableKey="1b49f055-d857-4f17-b2b7-7219218f6017" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" HiQnetStateVariableKey="eb736140-521f-4d52-9d43-15194e91dfa1" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" HiQnetStateVariableKey="619dde40-f207-4dc8-b01a-17876a152de0" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" HiQnetStateVariableKey="456ffc83-de59-494b-ac37-22801cbfdfc8" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" HiQnetStateVariableKey="1b57e52e-031b-4546-953a-650d4e359f2a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" HiQnetStateVariableKey="ccca676c-f8da-48b2-9e89-94b6d41dc4e3" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" HiQnetStateVariableKey="4ac912b4-97ef-4f31-914c-9d8742b3cf78" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" HiQnetStateVariableKey="ecdc8c23-904a-46c4-9fd2-df053985b7d5" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" HiQnetStateVariableKey="ddd29ce0-26eb-4e26-aa88-064dcf7e9035" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" HiQnetStateVariableKey="e138ce13-31df-4a00-8c63-9b4e356e3e19" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" HiQnetStateVariableKey="9a10cd9f-87d0-462d-b189-5307c9a024a4" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" HiQnetStateVariableKey="1799f94c-60f6-4ff9-82c0-ea2245863cc3" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" HiQnetStateVariableKey="915da551-20f3-43ea-8db8-c082bf9a243d" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" HiQnetStateVariableKey="66362220-98dc-43e6-86dc-75892b717e59" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" HiQnetStateVariableKey="310abe2e-452c-4db7-809d-a7d30df90d35" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" HiQnetStateVariableKey="2d4ba0b0-5bee-4c15-8a0f-19cd48f180ca" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" HiQnetStateVariableKey="fc751ae4-cf54-4dc4-8002-dac242f2af52" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" HiQnetStateVariableKey="d2e0e178-6266-458e-9c53-b272d9a178a0" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" HiQnetStateVariableKey="b165c684-93f9-485d-890f-70ecee73b46e" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" HiQnetStateVariableKey="5311218d-ad2a-4be8-8d10-090c74109510" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" HiQnetStateVariableKey="f8e210ed-6e33-445e-85db-f72ac508bee9" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" HiQnetStateVariableKey="1a489349-9ffd-434e-92fd-2baadd34f0bb" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" HiQnetStateVariableKey="bb6c0625-bd2a-493f-8338-f1bdcd58792f" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" HiQnetStateVariableKey="29bfe545-2bed-4d3d-9663-b63469b61bfc" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" HiQnetStateVariableKey="f359f59c-7828-4c22-8830-6643fa933749" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" HiQnetStateVariableKey="3f20ea28-aa67-422d-a442-616ba6f90bef" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" HiQnetStateVariableKey="a4f3c772-2cb1-4103-8fbd-d3b0a49ebdb8" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" HiQnetStateVariableKey="cb567d3e-03a5-4f5e-becb-12af3e04f183" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" HiQnetStateVariableKey="c768fc19-77cc-443a-aa56-cbaa8e82459a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" HiQnetStateVariableKey="9399d3e3-0653-47f3-b0a2-dc12a348cad5" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" HiQnetStateVariableKey="5d6fcaef-ee51-4e68-a0e5-21fb781088fb" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" HiQnetStateVariableKey="2ed6b2dd-5061-44af-bf85-83d1e1153900" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" HiQnetStateVariableKey="4d80aa69-765c-4159-8013-02019282e50e" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" HiQnetStateVariableKey="e05ca944-fd1e-42a6-ae87-aef0ba5d295a" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" HiQnetStateVariableKey="a31e0227-a759-44b2-b538-51278bd9897c" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" HiQnetStateVariableKey="b1fb84ef-5090-467e-b3e4-96444cc0e253" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" HiQnetStateVariableKey="7b4d2c00-6618-4bd7-b6aa-7e0a1542f2c2" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" HiQnetStateVariableKey="a035a81d-630c-4f84-a539-dfe411ee8239" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" HiQnetStateVariableKey="76e569ef-ba30-4838-99e4-befbdec95736" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" HiQnetStateVariableKey="da23c7d1-06fc-474b-92d6-61db0135d805" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" HiQnetStateVariableKey="0692a413-b1ab-4ad3-bb0d-05d002c077e6" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" HiQnetStateVariableKey="5a0a4978-27e4-43d2-8906-5f23b27bc5be" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" HiQnetStateVariableKey="adc70a62-172a-4d56-931b-1ce46e4bf641" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" HiQnetStateVariableKey="aad138bf-d27a-4e91-87cb-2b7919e11329" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" HiQnetStateVariableKey="11d48e11-9ef1-4c3c-b069-7378c27c4216" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" HiQnetStateVariableKey="9f393366-686d-4d3b-946d-cc6759e6d112" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Enable 9" ID="48" HiQnetStateVariableKey="e5b47e81-400a-4516-ac7c-ce5d849ebf17" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="49">
								<StateVariable Name="Frequency 9" ID="49" HiQnetStateVariableKey="a94b587b-32d6-47d3-8926-1eda1d8934d6" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="50">
								<StateVariable Name="Q 9" ID="50" HiQnetStateVariableKey="a1f931b8-864a-42e9-b80f-7a774c6c6bcd" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="51">
								<StateVariable Name="Slope 9" ID="51" HiQnetStateVariableKey="300f37fa-da46-4215-9e0b-be1df2d38f1c" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="52">
								<StateVariable Name="Gain 9" ID="52" HiQnetStateVariableKey="e33dde6f-d685-4741-b17c-7c1a0b3b770b" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="53">
								<StateVariable Name="Type 9" ID="53" HiQnetStateVariableKey="26b3928d-df7e-4a12-b16f-36c805896d02" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="54">
								<StateVariable Name="Enable 10" ID="54" HiQnetStateVariableKey="45aa68fe-7170-470a-a7af-7fd2ae853777" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="55">
								<StateVariable Name="Frequency 10" ID="55" HiQnetStateVariableKey="defdbe69-689f-43f9-b42c-ed6cc3844db1" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="56">
								<StateVariable Name="Q 10" ID="56" HiQnetStateVariableKey="7e42d332-903e-4d26-8b44-4f50cea73ad1" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="57">
								<StateVariable Name="Slope 10" ID="57" HiQnetStateVariableKey="7b4ba9f6-d7c1-4886-a99a-0a8948ea3ec2" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="58">
								<StateVariable Name="Gain 10" ID="58" HiQnetStateVariableKey="d16eff0e-aaa4-4aaa-bd2a-fab7b5a6578a" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="59">
								<StateVariable Name="Type 10" ID="59" HiQnetStateVariableKey="176a6bb3-22c6-42c0-bd82-bcad7f8783da" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="60">
								<StateVariable Name="Enable 11" ID="60" HiQnetStateVariableKey="f97d7da2-643b-4894-88e1-347969d502d4" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="61">
								<StateVariable Name="Frequency 11" ID="61" HiQnetStateVariableKey="5f5cb45e-7dee-42df-8718-2b469370cc8c" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="62">
								<StateVariable Name="Q 11" ID="62" HiQnetStateVariableKey="81e3360d-f82e-4bb6-a971-fd543fe9fd16" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="63">
								<StateVariable Name="Slope 11" ID="63" HiQnetStateVariableKey="2e693802-a9f1-412d-95f0-21f68514de0b" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="64">
								<StateVariable Name="Gain 11" ID="64" HiQnetStateVariableKey="989aa04c-5345-42b1-a9fd-e1b9536c45e2" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="65">
								<StateVariable Name="Type 11" ID="65" HiQnetStateVariableKey="3f3196f7-49a9-4263-a41a-f8ba6b2f87f2" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="66">
								<StateVariable Name="Enable 12" ID="66" HiQnetStateVariableKey="db06ee45-d4df-4c0e-a6d0-18f1abe343cc" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="67">
								<StateVariable Name="Frequency 12" ID="67" HiQnetStateVariableKey="becf3b03-2cdf-4b7d-bfc2-bcb348104c21" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="68">
								<StateVariable Name="Q 12" ID="68" HiQnetStateVariableKey="ce6c3861-3f34-45b6-9277-83e2e5b45a73" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="69">
								<StateVariable Name="Slope 12" ID="69" HiQnetStateVariableKey="541b1dbf-d047-4f8f-9f08-f609922aef29" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="70">
								<StateVariable Name="Gain 12" ID="70" HiQnetStateVariableKey="19d2d984-4624-4858-8283-9a2025dde725" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="71">
								<StateVariable Name="Type 12" ID="71" HiQnetStateVariableKey="1313a1a1-250b-4dfe-ba0a-0b9b2d3d136f" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="72">
								<StateVariable Name="Enable 13" ID="72" HiQnetStateVariableKey="b9592ead-ae86-4b2d-91d5-70844df0c7a8" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="73">
								<StateVariable Name="Frequency 13" ID="73" HiQnetStateVariableKey="646094db-322c-4d4c-9878-b99dd1530084" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="74">
								<StateVariable Name="Q 13" ID="74" HiQnetStateVariableKey="d8ceb7b9-1b05-44fc-910f-2d7b05060fac" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="75">
								<StateVariable Name="Slope 13" ID="75" HiQnetStateVariableKey="bfafa1de-c12d-4245-8547-e1dbf465d519" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="76">
								<StateVariable Name="Gain 13" ID="76" HiQnetStateVariableKey="c0a9a506-d8e8-41cf-b5f9-d830b0c760b0" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="77">
								<StateVariable Name="Type 13" ID="77" HiQnetStateVariableKey="e55f25b1-a5af-4646-a529-0b98a538424c" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="78">
								<StateVariable Name="Enable 14" ID="78" HiQnetStateVariableKey="1dd4f470-cdc8-41c1-b17a-a25442e68a80" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="79">
								<StateVariable Name="Frequency 14" ID="79" HiQnetStateVariableKey="dbfcd05f-ff56-4f8d-8c39-93467d8b2254" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="80">
								<StateVariable Name="Q 14" ID="80" HiQnetStateVariableKey="18cb45d5-7a41-4f36-b925-567813cbba76" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="81">
								<StateVariable Name="Slope 14" ID="81" HiQnetStateVariableKey="01cbb14a-3a59-4d9f-bded-33745b4830b2" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="82">
								<StateVariable Name="Gain 14" ID="82" HiQnetStateVariableKey="6c55d778-e483-42ba-8907-2f5cda2797bb" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="83">
								<StateVariable Name="Type 14" ID="83" HiQnetStateVariableKey="13979486-3086-42cc-8e2c-4818f9e96457" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="84">
								<StateVariable Name="Enable 15" ID="84" HiQnetStateVariableKey="17c01b63-6111-43de-9c7e-2e8386f08cd6" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="85">
								<StateVariable Name="Frequency 15" ID="85" HiQnetStateVariableKey="b0277644-02ad-495e-b6fc-08f5ef65369a" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="86">
								<StateVariable Name="Q 15" ID="86" HiQnetStateVariableKey="863878d8-f6ef-4b41-a491-e7e3fd1db44f" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="87">
								<StateVariable Name="Slope 15" ID="87" HiQnetStateVariableKey="f164a645-ca7b-4fb7-ab80-a4b6c17c1dbb" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="88">
								<StateVariable Name="Gain 15" ID="88" HiQnetStateVariableKey="c6240bb8-12c0-40c7-90f0-ea22114c5b97" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="89">
								<StateVariable Name="Type 15" ID="89" HiQnetStateVariableKey="4d783a03-db5f-4072-b8aa-a53febfe4f03" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="90">
								<StateVariable Name="Enable 16" ID="90" HiQnetStateVariableKey="cf92b5c6-6553-482c-87d7-019489c873d7" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="91">
								<StateVariable Name="Frequency 16" ID="91" HiQnetStateVariableKey="d5b41ced-d19c-4334-ab92-efa8e409cc4e" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="92">
								<StateVariable Name="Q 16" ID="92" HiQnetStateVariableKey="5b8b48cc-47e5-4472-a003-a7f4c9de481e" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="93">
								<StateVariable Name="Slope 16" ID="93" HiQnetStateVariableKey="cc2b3114-294f-41e1-89e4-d10e9649b502" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="94">
								<StateVariable Name="Gain 16" ID="94" HiQnetStateVariableKey="79910b5e-4c67-4dee-ad6e-bdf7e743948d" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="95">
								<StateVariable Name="Type 16" ID="95" HiQnetStateVariableKey="0c936fac-bf25-47ee-b393-0d6ed5427c18" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="96">
								<StateVariable Name="Bypass 1 Thru 8" ID="96" HiQnetStateVariableKey="eaf85421-fceb-4f52-aa31-ac46357db2d3" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="97">
								<StateVariable Name="Bypass 9 Thru 16" ID="97" HiQnetStateVariableKey="e18b5bc3-d3ab-496b-9e9a-1171fed42e96" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="98">
								<StateVariable Name="Array Volume Control" ID="98" HiQnetStateVariableKey="242d5432-c433-48af-bc34-35dc64cc491a" ClassID="546" Version="1" DefaultValue="200">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="36" OBJ_ADDR="664577">
						<Object Name="Ch1 IIR Crossover Filters" Address="664577" ClassID="36" Version="1" HiQnetObjectKey="b2637f41-ed8f-42dd-aee2-a064f43dc3d0">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Highpass Enable" ID="0" HiQnetStateVariableKey="00944153-2940-451f-b159-20262495be43" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Highpass Frequency" ID="1" HiQnetStateVariableKey="dadfe8b2-dfba-4001-93e1-d1089968f948" ClassID="587" Version="1" DefaultValue="20">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AABwQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="667" SV_ID="2">
								<StateVariable Name="Highpass Type" ID="2" HiQnetStateVariableKey="27004717-7431-4f5b-8650-68d6a945f7e9" ClassID="667" Version="1" DefaultValue="15">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="3">
								<StateVariable Name="Highpass Q" ID="3" HiQnetStateVariableKey="1374555d-42f8-4a99-b026-4d13cbf675cd" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="4">
								<StateVariable Name="Highpass Slope" ID="4" HiQnetStateVariableKey="e971f5d0-63f3-4b72-a877-e0f2be08a89d" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Lowpass Enable" ID="5" HiQnetStateVariableKey="339e0f0f-dd61-49df-9d8c-6d53a2e112d0" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Lowpass Frequency" ID="6" HiQnetStateVariableKey="0ef35474-f7da-4f0d-84e7-7d4f447d8373" ClassID="587" Version="1" DefaultValue="20000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AECcRg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="666" SV_ID="7">
								<StateVariable Name="Lowpass Type" ID="7" HiQnetStateVariableKey="50f72833-e8c1-4278-9dd8-040060813022" ClassID="666" Version="1" DefaultValue="15">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Lowpass Q" ID="8" HiQnetStateVariableKey="8ace01ea-881b-4869-9574-442c32269c59" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Lowpass Slope" ID="9" HiQnetStateVariableKey="b8f87c89-699a-4da8-bbd1-ed4222b6b9d2" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="36" OBJ_ADDR="664578">
						<Object Name="Ch2 IIR Crossover Filters" Address="664578" ClassID="36" Version="1" HiQnetObjectKey="ed29d9bd-467b-442e-8353-d606870300b4">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Highpass Enable" ID="0" HiQnetStateVariableKey="edf7b158-4493-42fa-be25-3a4c3d629741" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Highpass Frequency" ID="1" HiQnetStateVariableKey="9e234d68-b18d-4fcd-a8f6-9c289fcaf504" ClassID="587" Version="1" DefaultValue="20">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AABwQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="667" SV_ID="2">
								<StateVariable Name="Highpass Type" ID="2" HiQnetStateVariableKey="97b08e90-b56a-499c-9fd4-cad64039caa7" ClassID="667" Version="1" DefaultValue="15">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="3">
								<StateVariable Name="Highpass Q" ID="3" HiQnetStateVariableKey="0fd00b68-0760-46c3-9750-8d37379ecbab" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="4">
								<StateVariable Name="Highpass Slope" ID="4" HiQnetStateVariableKey="5247ab0e-9650-4575-8d57-8107a1bbcf70" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Lowpass Enable" ID="5" HiQnetStateVariableKey="1c8ff703-514c-442d-923e-cb47c27a00f3" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Lowpass Frequency" ID="6" HiQnetStateVariableKey="b697bbf3-f0d1-4174-a143-22cafdec906d" ClassID="587" Version="1" DefaultValue="20000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AECcRg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="666" SV_ID="7">
								<StateVariable Name="Lowpass Type" ID="7" HiQnetStateVariableKey="05fd94e5-9cb2-4559-8e17-3df646aa7fcd" ClassID="666" Version="1" DefaultValue="15">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">EQ==</Data3>
									<Data1 Len="1">Dw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Lowpass Q" ID="8" HiQnetStateVariableKey="ae3ed92a-1fc7-490b-9edb-7820f066f65d" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Lowpass Slope" ID="9" HiQnetStateVariableKey="ad18079a-ee2d-4b28-a53d-3d8530093fa3" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="37" OBJ_ADDR="730369">
						<Object Name="Ch1 FIR Filter" Address="730369" ClassID="37" Version="1" HiQnetObjectKey="aedea480-2f54-4129-996f-3bf66c67f101">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="c3506846-2837-45f5-8f92-0ce6dddd2fa6" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency" ID="1" HiQnetStateVariableKey="bd6e017c-c69b-4758-a281-ff9a0dc406b5" ClassID="587" Version="1" DefaultValue="2000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AIA7Rg==</Data3>
									<Data1 Len="4">AAD6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="752" SV_ID="2">
								<StateVariable Name="Mode" ID="2" HiQnetStateVariableKey="e7d0a097-53f6-4f9a-83bb-7623804bc277" ClassID="752" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="747" SV_ID="3">
								<StateVariable Name="Coeffs" ID="3" HiQnetStateVariableKey="8e7394c7-6a78-4b6d-a356-d11526d518ad" ClassID="747" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">AEA=</Data3>
									<Data1 Len="1800">AAAAAbO4eAa4OviDuCXzIjfw/Y44kcWvt7YlmrklIzu4xQ1pOTTawTl3Or+5KsaUug8lirlkll46Dt58OgxEIbotF6u61aiYuljOnTqAyDk6qHSOukhDnLs4B1G7FrSTuQoccDn6wLu6uvYuu0TVorq9bX0682mjOzJgtLmuYTW7ewqSu2xd8LjCVWk7H50POtHVerlNV+A5yDTMOyrSljs0zDi5ITTduxoJDbmlWdQ7f1YiO6BMpjqgbg27FL2EukYpETuBZlU7uHPQOwVYDLsGpWy6ud3FOx9sSDtpm5I5cCnJuyY0sLmrNtM7b2FeOyVp57uMvGK8GDeru9rbs7otkFG40TY+u8yrSLwvDMe76hNWuo52Gbs9b4K8VOU9vKH9srxtjr27dhReuuN7+bxAlee8smSxvKaxDrw4wiG74/HevCkQNLxDkmm74a/tu7StuLyYVPC9EiNWvQBZVjqSkqE9Ay1bPM5FDLx3Wk29KOCCvImS3j0OxNo9WvU6PIiRMLzJaw+7RkQ2PZwbFD3/zXw9hLzuvZoIcL4yD/u+DIuTO3g8yj3+EbI+A8E/PRy4h71Ctta9Z74Su4X+pD0zZ949OrXaPHWf/7wrtCm8Sk+fOoREeDx1dQM8wL0OPNAtSDyV6Ms7ZyHgvAvLBbvM1Hk8GLwQPMLD9TzNz5I8iNU0PDMTMjxSuqM8e489PDTq4zt0Bns7aNzMPFfwRzzDgCA819asPK9K3DyH+3Q8ezopPGC45jwO0cc7lnZMO/rVOjyH/tY8t6hIPJrzlzwnF9E7sJhUO/s6Xjw/VhE8Pd0lPAiEfzvmxKg8G+CTPEsK4DxOKhM8OKr8PDRs/zw16Io8EDx9O5sIzDt4PEo8E0/fPIU3QDyT7QI8RyHpO5NJuDsU6tQ7wETlPBrvOzwPE3E7tdNUO4z+djvDSTo7/lfoPALl+zwIqNM8Lt+lPFoh8DxRHlc8C3VDO41gxjtznqs7wTW8O+x39zvJX0Q7nVWkO7E1Qzvklw474Y0xO6AXYDtyJpM7qv4DO/2bxjwDvWE7t/60O1btQjtj9OI7rtlAO8wlIjuwp0c7lTbMO6daXTvGDCI7tqqBO4BrjDtQAx87kOldO8rSWjvSYb87qlcXO5JNZzuryro7zkVWO8SKHDuZS787htcBO6ODEjvCPEE7srd6O4XGqDtsJr47ltUwO7nyODuv1LQ7hxgzO2sDKjuNiKo7qBo1O52rtDt3uJM7XLdsO395ADuMgCw7cGRJOy4UZDsik3A7VFTJO3ZyVTtTkYo7Fh5OOwtDVjs5Iu47Wu43O0L1vDsWlxU7E5l3OzblmDtDGVo7GhD0OtDgrzrNnoM7CxvkOxiFpTrqrrg6mzkYOqiJKTr58Z07D3i2OuvC7Tqu8C86u7W5OvTp7Dr7Jus6tl9iOm1fXDqCY8E6tbX2Orm3aTp/1IM6JwR+OliynDqglXU6oWIMOlJ1LzoBLpc6LS0MOoFkFTp5jIM6FKx3ObBMCjoKebo6U8WhOj3e0zm0RNU5ElvROahSCjoSJnI58lrROQrIxrb3V9g5SPVqOdYWnTmmqvU4Ia91uHvs6DjpOn05gai+OMSmOblMoZW5k/9HuPopLzWP11W5DVAbucOlFLngwu25luiauVzJNbm3E0q6DLllugwfQLnCrO+5m7C/ueDBRrocOQq6Gm7Yuesl+7nN79C6BMv7uiXlsboe6M65/QMIuepnT7oPi6y6JqgEuhltVrn0uJG55YlQugf1jboWRu+6BbfeudY/5rnRUy65+vUuugkmI7n1zsq5z45GudRZhrn3r8W6AEZLudxrvbm37M25vWbhudpreLneCPu5v9rtuaklC7m2zNO50HFfuc3mCrmxipi5otmBubOjQLnGnJO5uvD0uZwRR7mQooa5onGUubCxM7mfj5i5gBAauW7N3rmJ0Mu5lN8PuYDIcLlE8PW5PK/xuWoj+bmB6wG5WayEuRZqBbkFsby5LoSMuUsE67kmc9m4xZBNuJX0orjg1Y65FF8buPIPvLhC6oC25ONhuAltC7ilPQe4mW/ytuVOwThg0po4Q6kXttjaLLfLUkc4EpeZOPQi+DkKRoE4lKE5N69rGziAeH85JaMPOVCUYDkOZ5M4YDJLOIzmsTkzoik5ejtiOUAuczikXI84i1U4OTNNVjmIBaY5YZhAOMksyzh/KpY5I2dYOYN6WzliGKU4x9IwODnbbzjx6GI5S2NhOSr4ADiA2A83qWAPOKH+fDkLqvw40DTCN5+mRLZAU8k4Tp3rOLgspjha7hq3I0LCt5G9GDfyKtk4a/VjN9nfTredbx23rjUCN2XqqTgI//Q3XHMDt3VgebeEGpM2l5C8N4Sctja21bK3KP19tzrUVDWaDhw3IySx</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="4">
								<StateVariable Name="FFT Length" ID="4" HiQnetStateVariableKey="b1580e4a-0a02-4a05-b6f0-686af11f538a" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Latency" ID="5" HiQnetStateVariableKey="afbb13e7-de3a-4c4b-8bb0-fb29e10cb291" ClassID="535" Version="1" DefaultValue="-1E+37">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="Utilization" ID="6" HiQnetStateVariableKey="395f9b08-0eee-4d18-8b38-383f58f01dec" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="754" SV_ID="7">
								<StateVariable Name="Latency48KHz" ID="7" HiQnetStateVariableKey="6d3722b1-e86a-4c37-b8ef-d5623771127d" ClassID="754" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="755" SV_ID="8">
								<StateVariable Name="Latency96KHz" ID="8" HiQnetStateVariableKey="991cec30-dc4a-4727-bf74-b38da86ac0b4" ClassID="755" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">Ag==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="751" SV_ID="9">
								<StateVariable Name="Type" ID="9" HiQnetStateVariableKey="797257f2-8f65-4ff2-95aa-4c7beff82bd5" ClassID="751" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">Aw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="37" OBJ_ADDR="730370">
						<Object Name="Ch2 FIR Filter" Address="730370" ClassID="37" Version="1" HiQnetObjectKey="b9a653da-5a64-43d3-8090-0bd118ee7b29">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="8d50ae91-2bd2-4f59-85a7-d2117aaf763f" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency" ID="1" HiQnetStateVariableKey="70fe1376-9fd7-44dd-b70d-f3e937635818" ClassID="587" Version="1" DefaultValue="2000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AIA7Rg==</Data3>
									<Data1 Len="4">AAD6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="752" SV_ID="2">
								<StateVariable Name="Mode" ID="2" HiQnetStateVariableKey="76529f03-0890-4953-a21b-538374173f0e" ClassID="752" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="747" SV_ID="3">
								<StateVariable Name="Coeffs" ID="3" HiQnetStateVariableKey="96fa46e3-fdac-48c6-b6a4-aeccc782f762" ClassID="747" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">AEA=</Data3>
									<Data1 Len="1800">AAAAAbO4eAa4OviDuCXzIjfw/Y44kcWvt7YlmrklIzu4xQ1pOTTawTl3Or+5KsaUug8lirlkll46Dt58OgxEIbotF6u61aiYuljOnTqAyDk6qHSOukhDnLs4B1G7FrSTuQoccDn6wLu6uvYuu0TVorq9bX0682mjOzJgtLmuYTW7ewqSu2xd8LjCVWk7H50POtHVerlNV+A5yDTMOyrSljs0zDi5ITTduxoJDbmlWdQ7f1YiO6BMpjqgbg27FL2EukYpETuBZlU7uHPQOwVYDLsGpWy6ud3FOx9sSDtpm5I5cCnJuyY0sLmrNtM7b2FeOyVp57uMvGK8GDeru9rbs7otkFG40TY+u8yrSLwvDMe76hNWuo52Gbs9b4K8VOU9vKH9srxtjr27dhReuuN7+bxAlee8smSxvKaxDrw4wiG74/HevCkQNLxDkmm74a/tu7StuLyYVPC9EiNWvQBZVjqSkqE9Ay1bPM5FDLx3Wk29KOCCvImS3j0OxNo9WvU6PIiRMLzJaw+7RkQ2PZwbFD3/zXw9hLzuvZoIcL4yD/u+DIuTO3g8yj3+EbI+A8E/PRy4h71Ctta9Z74Su4X+pD0zZ949OrXaPHWf/7wrtCm8Sk+fOoREeDx1dQM8wL0OPNAtSDyV6Ms7ZyHgvAvLBbvM1Hk8GLwQPMLD9TzNz5I8iNU0PDMTMjxSuqM8e489PDTq4zt0Bns7aNzMPFfwRzzDgCA819asPK9K3DyH+3Q8ezopPGC45jwO0cc7lnZMO/rVOjyH/tY8t6hIPJrzlzwnF9E7sJhUO/s6Xjw/VhE8Pd0lPAiEfzvmxKg8G+CTPEsK4DxOKhM8OKr8PDRs/zw16Io8EDx9O5sIzDt4PEo8E0/fPIU3QDyT7QI8RyHpO5NJuDsU6tQ7wETlPBrvOzwPE3E7tdNUO4z+djvDSTo7/lfoPALl+zwIqNM8Lt+lPFoh8DxRHlc8C3VDO41gxjtznqs7wTW8O+x39zvJX0Q7nVWkO7E1Qzvklw474Y0xO6AXYDtyJpM7qv4DO/2bxjwDvWE7t/60O1btQjtj9OI7rtlAO8wlIjuwp0c7lTbMO6daXTvGDCI7tqqBO4BrjDtQAx87kOldO8rSWjvSYb87qlcXO5JNZzuryro7zkVWO8SKHDuZS787htcBO6ODEjvCPEE7srd6O4XGqDtsJr47ltUwO7nyODuv1LQ7hxgzO2sDKjuNiKo7qBo1O52rtDt3uJM7XLdsO395ADuMgCw7cGRJOy4UZDsik3A7VFTJO3ZyVTtTkYo7Fh5OOwtDVjs5Iu47Wu43O0L1vDsWlxU7E5l3OzblmDtDGVo7GhD0OtDgrzrNnoM7CxvkOxiFpTrqrrg6mzkYOqiJKTr58Z07D3i2OuvC7Tqu8C86u7W5OvTp7Dr7Jus6tl9iOm1fXDqCY8E6tbX2Orm3aTp/1IM6JwR+OliynDqglXU6oWIMOlJ1LzoBLpc6LS0MOoFkFTp5jIM6FKx3ObBMCjoKebo6U8WhOj3e0zm0RNU5ElvROahSCjoSJnI58lrROQrIxrb3V9g5SPVqOdYWnTmmqvU4Ia91uHvs6DjpOn05gai+OMSmOblMoZW5k/9HuPopLzWP11W5DVAbucOlFLngwu25luiauVzJNbm3E0q6DLllugwfQLnCrO+5m7C/ueDBRrocOQq6Gm7Yuesl+7nN79C6BMv7uiXlsboe6M65/QMIuepnT7oPi6y6JqgEuhltVrn0uJG55YlQugf1jboWRu+6BbfeudY/5rnRUy65+vUuugkmI7n1zsq5z45GudRZhrn3r8W6AEZLudxrvbm37M25vWbhudpreLneCPu5v9rtuaklC7m2zNO50HFfuc3mCrmxipi5otmBubOjQLnGnJO5uvD0uZwRR7mQooa5onGUubCxM7mfj5i5gBAauW7N3rmJ0Mu5lN8PuYDIcLlE8PW5PK/xuWoj+bmB6wG5WayEuRZqBbkFsby5LoSMuUsE67kmc9m4xZBNuJX0orjg1Y65FF8buPIPvLhC6oC25ONhuAltC7ilPQe4mW/ytuVOwThg0po4Q6kXttjaLLfLUkc4EpeZOPQi+DkKRoE4lKE5N69rGziAeH85JaMPOVCUYDkOZ5M4YDJLOIzmsTkzoik5ejtiOUAuczikXI84i1U4OTNNVjmIBaY5YZhAOMksyzh/KpY5I2dYOYN6WzliGKU4x9IwODnbbzjx6GI5S2NhOSr4ADiA2A83qWAPOKH+fDkLqvw40DTCN5+mRLZAU8k4Tp3rOLgspjha7hq3I0LCt5G9GDfyKtk4a/VjN9nfTredbx23rjUCN2XqqTgI//Q3XHMDt3VgebeEGpM2l5C8N4Sctja21bK3KP19tzrUVDWaDhw3IySx</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="4">
								<StateVariable Name="FFT Length" ID="4" HiQnetStateVariableKey="8ff480c2-31e8-438e-a366-2c9fcfbf4a8a" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Latency" ID="5" HiQnetStateVariableKey="9893bd2e-e089-4fe3-bdc7-ed4e2daba639" ClassID="535" Version="1" DefaultValue="-1E+37">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="Utilization" ID="6" HiQnetStateVariableKey="7db9d9e8-356b-4c56-94cc-638799896d06" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="754" SV_ID="7">
								<StateVariable Name="Latency48KHz" ID="7" HiQnetStateVariableKey="aef09aed-abc1-4f3e-9f9d-680f34dca48d" ClassID="754" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="755" SV_ID="8">
								<StateVariable Name="Latency96KHz" ID="8" HiQnetStateVariableKey="c8a4ed2e-a58f-46f8-90bc-27ea808eca61" ClassID="755" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">BQ==</Data3>
									<Data1 Len="1">Ag==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="751" SV_ID="9">
								<StateVariable Name="Type" ID="9" HiQnetStateVariableKey="c646d7ac-c483-4e3d-a15f-ad650dd809ed" ClassID="751" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">Aw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="34" OBJ_ADDR="795137">
						<Object Name="Ch1 Speaker EQ Filters" Address="795137" ClassID="34" Version="1" HiQnetObjectKey="149c3110-5b09-43ac-9c89-9bdbfc68761c">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" HiQnetStateVariableKey="04fe81ae-8d1b-4f74-acf0-531421dcc81a" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" HiQnetStateVariableKey="344b2697-78db-432c-99cc-c8bf6c12fc11" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AACcQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" HiQnetStateVariableKey="e538bb8f-171d-4503-a142-b3df761353ec" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AAAgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" HiQnetStateVariableKey="78c1f82e-bde4-4c0c-9be2-188e42070608" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" HiQnetStateVariableKey="398dc212-1385-40d6-919b-745da01c51dc" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" HiQnetStateVariableKey="b06499af-931b-45cb-9e09-2f514b744346" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" HiQnetStateVariableKey="304b702b-8eef-4024-aee0-dffa77116aaa" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" HiQnetStateVariableKey="85a6ebc5-d9ae-48a3-99fa-a8d44c819a47" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAA+Qw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" HiQnetStateVariableKey="812838a0-5425-4209-9ecf-3de72570df82" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AAAAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" HiQnetStateVariableKey="e26f7369-e4b2-4b17-be97-a42cbbc276ca" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" HiQnetStateVariableKey="e6565998-6afd-45f4-995d-5b634b9f9fda" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAwA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" HiQnetStateVariableKey="e381cc32-55aa-49d3-9c01-9914c9af1ecf" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" HiQnetStateVariableKey="52a7c920-19f0-4e38-b7af-3ada41cc395a" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" HiQnetStateVariableKey="27ac792d-5f6f-4658-b709-558958e28d87" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AACgQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" HiQnetStateVariableKey="aba52915-658d-4c8a-9989-99eb54ecb9d7" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" HiQnetStateVariableKey="8102727c-0219-48fd-82f4-029e5cad2bfa" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" HiQnetStateVariableKey="5b0df5d3-1c59-4a06-ba8f-62bec2bf0165" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACQQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" HiQnetStateVariableKey="13a4160b-7963-42b7-b488-b960ffa4ce16" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" HiQnetStateVariableKey="22eae889-61b5-4c5a-8b7b-9afe08de184d" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" HiQnetStateVariableKey="78f0dd86-ebc5-4573-8c90-4f508d322e51" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AADIQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" HiQnetStateVariableKey="18bc0358-6067-47c2-bb9e-523fe181f579" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" HiQnetStateVariableKey="4108416c-8085-4464-b96e-fb1b90062ac2" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" HiQnetStateVariableKey="c3825335-e134-4f6f-8816-8f2d7064403b" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAIwQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" HiQnetStateVariableKey="204fd0f8-f1cb-43fc-8e08-00289397376b" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" HiQnetStateVariableKey="d5a32d2b-552b-42ce-9602-3341e68b7ded" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" HiQnetStateVariableKey="af76da4e-1324-4ef0-9e82-311ff1f79b2c" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAWRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" HiQnetStateVariableKey="17711bff-f1be-4bbe-962b-1e383db82677" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">zcxMQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" HiQnetStateVariableKey="a9d5b445-0dcf-4a17-a759-4e7dc8176a1e" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" HiQnetStateVariableKey="55ca4097-f8dd-4d89-8ef7-bba0dec604e2" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACQQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" HiQnetStateVariableKey="85f0b0aa-65e8-4583-b205-05f07957fd7c" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" HiQnetStateVariableKey="0df76b31-8f4c-46c3-86c7-b1a982c1e515" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" HiQnetStateVariableKey="0bf2b6e8-0e90-4d1b-bfb3-388ccca01208" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAvRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" HiQnetStateVariableKey="4b5d3118-28d0-4684-84a6-fe49f36b89c4" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" HiQnetStateVariableKey="fcfdec3f-4e96-4de5-acfd-a2f41e4520ea" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" HiQnetStateVariableKey="879cd670-fafb-4f77-b576-104827aa2db0" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACAwA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" HiQnetStateVariableKey="0f6feb8d-04f0-4e59-a532-3bdd8576f286" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" HiQnetStateVariableKey="8e57bdd4-0d70-437e-a670-01e8f960ed18" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" HiQnetStateVariableKey="4d8d8754-65f3-4db0-8a41-0e889096a9bf" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" HiQnetStateVariableKey="5fffa852-ebd8-42bf-8bbb-45d04bf62949" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" HiQnetStateVariableKey="12198bee-53f9-4f00-a665-4695cee90cfa" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" HiQnetStateVariableKey="8c1c0586-4451-447b-9029-e66fa9cdb378" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" HiQnetStateVariableKey="3d0f9eea-119f-44a7-ab8c-151cff567dea" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" HiQnetStateVariableKey="43c64fbd-da5c-4e3f-9f65-7fe1722dfe3a" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" HiQnetStateVariableKey="4d07fa27-bc89-4667-badb-403708c58f36" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" HiQnetStateVariableKey="28e8010d-4f75-4dff-bfa9-f258fad0f36f" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" HiQnetStateVariableKey="bc30d561-f739-4a95-b2c7-288402d51c42" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" HiQnetStateVariableKey="b3829980-e5b4-4692-b073-ffe7e5e7e7f2" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" HiQnetStateVariableKey="fd6fd490-f85a-4256-b6de-848b3c5f76b9" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Bypass" ID="48" HiQnetStateVariableKey="1af737fa-7c54-4ec6-83e5-db4a9d1cc726" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="49">
								<StateVariable Name="Enable 9" ID="49" HiQnetStateVariableKey="10992ec6-dc97-479a-892d-811acb42daa4" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="50">
								<StateVariable Name="Frequency 9" ID="50" HiQnetStateVariableKey="0f5cc357-66eb-440c-b54d-7987fac3f4ca" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="51">
								<StateVariable Name="Q 9" ID="51" HiQnetStateVariableKey="dd1962d8-d8a8-447e-aa84-9391c051845a" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="52">
								<StateVariable Name="Slope 9" ID="52" HiQnetStateVariableKey="9e303da6-e0d4-4078-a446-ccdce5dbe124" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="53">
								<StateVariable Name="Gain 9" ID="53" HiQnetStateVariableKey="f9bc4291-5d3c-4709-a37f-ad1c7caa005e" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="54">
								<StateVariable Name="Type 9" ID="54" HiQnetStateVariableKey="f5b50c22-c88d-41c0-9388-a7a986064274" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="55">
								<StateVariable Name="Enable 10" ID="55" HiQnetStateVariableKey="a118bc8f-1a05-4e3c-9ab8-c4690e9e6370" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="56">
								<StateVariable Name="Frequency 10" ID="56" HiQnetStateVariableKey="eb74cc5c-cb80-46d3-aa42-43741896a381" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="57">
								<StateVariable Name="Q 10" ID="57" HiQnetStateVariableKey="d41b2e07-5e11-4582-bb34-baa66771c68b" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="58">
								<StateVariable Name="Slope 10" ID="58" HiQnetStateVariableKey="35ccb788-9d35-47f5-9a56-9add2deed25f" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="59">
								<StateVariable Name="Gain 10" ID="59" HiQnetStateVariableKey="f249e84a-7326-4c7b-b1fd-57b5a2f56a23" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="60">
								<StateVariable Name="Type 10" ID="60" HiQnetStateVariableKey="d9b51f59-3ff0-467a-b511-377f49029b60" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="61">
								<StateVariable Name="Enable 11" ID="61" HiQnetStateVariableKey="0bf1643f-ce03-46d0-a3e3-b3bfa365201f" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="62">
								<StateVariable Name="Frequency 11" ID="62" HiQnetStateVariableKey="322b8970-f650-414d-a8fa-9610f00c4984" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="63">
								<StateVariable Name="Q 11" ID="63" HiQnetStateVariableKey="61fec626-0f03-474c-99f4-3d533a96ff89" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="64">
								<StateVariable Name="Slope 11" ID="64" HiQnetStateVariableKey="c3e2de96-1b95-49cf-962c-5dcef9533f3e" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="65">
								<StateVariable Name="Gain 11" ID="65" HiQnetStateVariableKey="8c5637d5-cc25-4cd2-a26e-2bed762801e2" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="66">
								<StateVariable Name="Type 11" ID="66" HiQnetStateVariableKey="77f762e9-3935-4cda-ab72-fe43ff5ca07e" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="67">
								<StateVariable Name="Enable 12" ID="67" HiQnetStateVariableKey="40d2bb41-2920-4853-9237-6a65e5c68d9a" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="68">
								<StateVariable Name="Frequency 12" ID="68" HiQnetStateVariableKey="d2270a1a-9422-4f62-97d6-77486b8b12f6" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="69">
								<StateVariable Name="Q 12" ID="69" HiQnetStateVariableKey="a21c6d16-6ce2-4900-a82f-a1a3ff7b438c" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="70">
								<StateVariable Name="Slope 12" ID="70" HiQnetStateVariableKey="30a2bbf6-f307-4cf4-8250-5a19ea771b5f" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="71">
								<StateVariable Name="Gain 12" ID="71" HiQnetStateVariableKey="fe145fd1-4f90-47a6-9d7f-ca8676b0693b" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="72">
								<StateVariable Name="Type 12" ID="72" HiQnetStateVariableKey="a452978b-7d12-4e5e-b4bb-58816620a5a7" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="34" OBJ_ADDR="795138">
						<Object Name="Ch2 Speaker EQ Filters" Address="795138" ClassID="34" Version="1" HiQnetObjectKey="acc69b29-a9cc-40dd-ae81-e69a8bdcc4f3">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" HiQnetStateVariableKey="520bebc5-63fe-415c-99be-32fee8149dd7" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" HiQnetStateVariableKey="ba607790-e97d-46ab-9ec9-abd2436f9501" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AACcQg==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" HiQnetStateVariableKey="bdc35e4c-8143-4497-a550-3a91a5be8088" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AAAgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" HiQnetStateVariableKey="30951ed7-acd7-4d7b-a707-2279520b5b05" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" HiQnetStateVariableKey="a113b223-1c83-4034-ba03-4f4d8f2f2872" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" HiQnetStateVariableKey="a8e46f17-4b3f-4f48-ad62-ac7320e0f46c" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" HiQnetStateVariableKey="4916cff3-075d-4f03-8cc6-795d25ce6ed0" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" HiQnetStateVariableKey="185cfd1d-0974-4da7-8635-68fd83415a12" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAA+Qw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" HiQnetStateVariableKey="36d79b7c-f1aa-48c0-b956-40c3ab1388b3" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AAAAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" HiQnetStateVariableKey="fd501f51-00bf-431c-961a-30dcd3627e74" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" HiQnetStateVariableKey="9cbb35e7-05ae-4a09-b949-c5f70bcd8a77" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAwA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" HiQnetStateVariableKey="399a3cd0-2d27-4cdd-a020-a13f40a67591" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" HiQnetStateVariableKey="31ba13bf-fdce-4c2f-afc4-a946557fd548" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" HiQnetStateVariableKey="42b38f52-ebe7-48fc-8869-35d849de8207" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AACgQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" HiQnetStateVariableKey="a82006c1-4121-482c-a109-5fea482fe28b" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" HiQnetStateVariableKey="e1f94943-69a7-49a2-8e04-304fee22ad62" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" HiQnetStateVariableKey="3953029c-d160-4109-9e01-a4809d179cde" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACQQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" HiQnetStateVariableKey="5958665b-dd42-426d-9470-151cf06d211f" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" HiQnetStateVariableKey="8d4ff5b3-bf9e-4736-8e73-91430fa4426e" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" HiQnetStateVariableKey="f80f3279-7faa-4737-92f6-0d703fe8760a" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AADIQw==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" HiQnetStateVariableKey="d837a96c-af0b-4d59-ac9c-d8a9b33afbab" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" HiQnetStateVariableKey="a510bcd5-3f38-483a-8190-9ba067529e72" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" HiQnetStateVariableKey="5d1e0d6a-278f-4064-a90b-a23eaebb9c78" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAIwQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" HiQnetStateVariableKey="58253a32-1612-4a1b-89e5-ab7b6edffa07" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Enable 5" ID="24" HiQnetStateVariableKey="e33fa143-7ee8-4acf-8ba3-a954bf027860" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="25">
								<StateVariable Name="Frequency 5" ID="25" HiQnetStateVariableKey="fae3b4fe-f38e-437b-bd53-bddae08da9f3" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAWRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="26">
								<StateVariable Name="Q 5" ID="26" HiQnetStateVariableKey="050666f9-c391-49b7-9e71-01a8df5d56a0" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">zcxMQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="27">
								<StateVariable Name="Slope 5" ID="27" HiQnetStateVariableKey="e7c43c09-67e5-45e5-a5ab-a5182a6f9b8f" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="28">
								<StateVariable Name="Gain 5" ID="28" HiQnetStateVariableKey="9f1b1fd3-bdd8-490a-a8c2-136000a8b96b" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACQQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="29">
								<StateVariable Name="Type 5" ID="29" HiQnetStateVariableKey="34a3768f-199b-4a29-97cf-4de14c78f7c3" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Enable 6" ID="30" HiQnetStateVariableKey="6ff04baf-7cbd-48a9-b420-9fe77c59f941" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="31">
								<StateVariable Name="Frequency 6" ID="31" HiQnetStateVariableKey="4ed6bd82-43c3-428d-8dfc-16f5ad0c1a7a" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAAvRA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="32">
								<StateVariable Name="Q 6" ID="32" HiQnetStateVariableKey="649b166f-5809-4c05-873e-d4925e9a67a4" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACgQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="33">
								<StateVariable Name="Slope 6" ID="33" HiQnetStateVariableKey="43316392-999e-4ee6-bd0a-0e4287a72aee" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="34">
								<StateVariable Name="Gain 6" ID="34" HiQnetStateVariableKey="e5bdfa4b-778e-4675-89b5-c0c6069f2bb1" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AACAwA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="35">
								<StateVariable Name="Type 6" ID="35" HiQnetStateVariableKey="be47522a-8096-416c-b782-bddde1679e63" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="36">
								<StateVariable Name="Enable 7" ID="36" HiQnetStateVariableKey="db74e42c-e61d-4d07-a0eb-f31e37af804e" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="37">
								<StateVariable Name="Frequency 7" ID="37" HiQnetStateVariableKey="8cf51f71-4849-463c-b4f7-f4d2d9710400" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="38">
								<StateVariable Name="Q 7" ID="38" HiQnetStateVariableKey="c13aa547-8045-41e5-9a6b-07f7264556fc" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="39">
								<StateVariable Name="Slope 7" ID="39" HiQnetStateVariableKey="ea88597c-a96a-4ba1-9c02-cd6f62fb6724" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="40">
								<StateVariable Name="Gain 7" ID="40" HiQnetStateVariableKey="31dc99eb-4715-4b2b-88ba-aa499c0e4a75" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="41">
								<StateVariable Name="Type 7" ID="41" HiQnetStateVariableKey="67489577-52b3-4220-a2c4-d74af76e0c08" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="42">
								<StateVariable Name="Enable 8" ID="42" HiQnetStateVariableKey="b89119ff-edfc-47c1-924e-fd9901a484b6" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="43">
								<StateVariable Name="Frequency 8" ID="43" HiQnetStateVariableKey="c6b87ef1-2e1d-4a3f-be9b-89c163397363" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="44">
								<StateVariable Name="Q 8" ID="44" HiQnetStateVariableKey="518efcb4-eb64-4773-af3e-9c93217b9616" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="45">
								<StateVariable Name="Slope 8" ID="45" HiQnetStateVariableKey="4a26a644-60e6-4f3e-bfd7-37534bf9db6d" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="46">
								<StateVariable Name="Gain 8" ID="46" HiQnetStateVariableKey="8defc783-73f7-4684-b68c-3c7ba9778547" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="47">
								<StateVariable Name="Type 8" ID="47" HiQnetStateVariableKey="2539292b-cbab-4dee-b042-b8bf3adac426" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="48">
								<StateVariable Name="Bypass" ID="48" HiQnetStateVariableKey="e93b6c42-219a-4504-8836-528385eebddc" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="49">
								<StateVariable Name="Enable 9" ID="49" HiQnetStateVariableKey="2b62ad6f-41f3-43ad-ab24-b6b54f921f56" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="50">
								<StateVariable Name="Frequency 9" ID="50" HiQnetStateVariableKey="9cb18c1e-b336-441f-8734-fb3e9161ffe9" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="51">
								<StateVariable Name="Q 9" ID="51" HiQnetStateVariableKey="90e2f9ee-7238-432e-993b-d8a348f4358e" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="52">
								<StateVariable Name="Slope 9" ID="52" HiQnetStateVariableKey="6548d2b7-208a-4ffa-9b88-0c73a90eaa78" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="53">
								<StateVariable Name="Gain 9" ID="53" HiQnetStateVariableKey="ed29c9b8-7803-4836-8079-6f489b391832" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="54">
								<StateVariable Name="Type 9" ID="54" HiQnetStateVariableKey="477e1c04-ae2c-493f-8f47-35fc0785ee04" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="55">
								<StateVariable Name="Enable 10" ID="55" HiQnetStateVariableKey="8c557456-2944-4c55-92a5-b313fbd5b0ab" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="56">
								<StateVariable Name="Frequency 10" ID="56" HiQnetStateVariableKey="dd865022-42c6-489d-92a5-9de336d2d15b" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="57">
								<StateVariable Name="Q 10" ID="57" HiQnetStateVariableKey="8974cfa3-20db-4804-9cd2-6bd7eb2cadb4" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="58">
								<StateVariable Name="Slope 10" ID="58" HiQnetStateVariableKey="65a8626c-2aff-4d04-8052-f926765fd5e7" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="59">
								<StateVariable Name="Gain 10" ID="59" HiQnetStateVariableKey="9fa81a15-b74d-4714-be68-ade956883dfc" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="60">
								<StateVariable Name="Type 10" ID="60" HiQnetStateVariableKey="2deff39c-fbdc-4f06-83b5-9eae5d08833e" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="61">
								<StateVariable Name="Enable 11" ID="61" HiQnetStateVariableKey="deae6450-1774-4a0b-9dd6-f12ab5060735" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="62">
								<StateVariable Name="Frequency 11" ID="62" HiQnetStateVariableKey="dec888cc-eb33-4396-82c6-622eea3d52f0" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="63">
								<StateVariable Name="Q 11" ID="63" HiQnetStateVariableKey="d684fa98-d98e-4353-8a50-0f2577d58ca8" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="64">
								<StateVariable Name="Slope 11" ID="64" HiQnetStateVariableKey="b4251038-8ba7-4f71-90db-3cac0c4e609c" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="65">
								<StateVariable Name="Gain 11" ID="65" HiQnetStateVariableKey="cbfd7c32-ae43-46c0-b588-3baba287eeb9" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="66">
								<StateVariable Name="Type 11" ID="66" HiQnetStateVariableKey="d922ca87-fa9b-414d-8057-4e42c9d08940" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="67">
								<StateVariable Name="Enable 12" ID="67" HiQnetStateVariableKey="6b6effcf-43a2-45c6-aa70-48e37889ec09" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="68">
								<StateVariable Name="Frequency 12" ID="68" HiQnetStateVariableKey="39aa042c-637f-43bf-b36f-f821ad6b915d" ClassID="587" Version="1" DefaultValue="1000">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">AECcRg==</Data3>
									<Data1 Len="4">AAB6RA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="69">
								<StateVariable Name="Q 12" ID="69" HiQnetStateVariableKey="8a39ddeb-d2d0-4a39-a43d-ec1e6703f742" ClassID="588" Version="1" DefaultValue="4">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAMQg==</Data3>
									<Data1 Len="4">AACAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="70">
								<StateVariable Name="Slope 12" ID="70" HiQnetStateVariableKey="f271cf99-d8c0-4273-ac64-8f1111336587" ClassID="668" Version="1" DefaultValue="6">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AABAQQ==</Data3>
									<Data1 Len="4">AADAQA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="71">
								<StateVariable Name="Gain 12" ID="71" HiQnetStateVariableKey="79bd796c-5985-48e1-93dc-c54e1a563c28" ClassID="589" Version="1" DefaultValue="0">
									<Data2 Len="4">AADAwQ==</Data2>
									<Data3 Len="4">AADAQQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="72">
								<StateVariable Name="Type 12" ID="72" HiQnetStateVariableKey="3cec44c2-c98f-4374-9e0f-78998f8c7588" ClassID="665" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Cg==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="857089">
						<Object Name="Ch1 Speaker Delay" Address="857089" ClassID="20" Version="1" HiQnetObjectKey="f7f0c840-35de-4a19-a530-fcf1a6a1d1a4">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" HiQnetStateVariableKey="66beeb58-7543-4c19-a843-5a6af18e4249" ClassID="562" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAQA==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" HiQnetStateVariableKey="64516d29-6c61-4b67-9e08-1cceae96d226" ClassID="561" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" HiQnetStateVariableKey="04e8f40a-c543-4f54-b7d2-1daa8f15788f" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" HiQnetStateVariableKey="a1260393-6c0b-43ff-a2ce-00f9aa93d03a" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="20" OBJ_ADDR="857090">
						<Object Name="Ch2 Speaker Delay" Address="857090" ClassID="20" Version="1" HiQnetObjectKey="f8923b6e-b2f7-401f-a9b9-57c10331491d">
							<STATE_VARIABLE SV_CLASSID="562" SV_ID="0">
								<StateVariable Name="Coarse" ID="0" HiQnetStateVariableKey="214d6cb5-6b86-4ef0-9101-d050ec9d4378" ClassID="562" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAQA==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="1">
								<StateVariable Name="Fine" ID="1" HiQnetStateVariableKey="64e3fd6d-b748-4648-9e4d-53e1690cfcd9" ClassID="561" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Coarse Bypass" ID="2" HiQnetStateVariableKey="88ff5ecc-7104-4a20-aee8-6aa66d6f6169" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Fine Bypass" ID="3" HiQnetStateVariableKey="0351e78e-f0ac-4342-8baa-db14cdc10930" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="15" OBJ_ADDR="921345">
						<Object Name="Ch 1 IOC Limiter" Address="921345" ClassID="15" Version="1" HiQnetObjectKey="8b23741a-98a8-4012-b6d2-9313d80819eb">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="0b73af04-e24b-48f0-a2b5-bdfaeeaa6377" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Attack" ID="1" HiQnetStateVariableKey="5e02927b-0539-4b88-be70-f5ad6fc8f888" ClassID="733" Version="1" DefaultValue="0.02">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Release" ID="2" HiQnetStateVariableKey="febd353b-9032-4e27-8e38-77e0a0891f1b" ClassID="733" Version="1" DefaultValue="0.6">
									<Data2 Len="4">CtcjPA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Threshold" ID="3" HiQnetStateVariableKey="7043ddf4-93d3-4a20-a395-632214208e2b" ClassID="733" Version="1" DefaultValue="0.001">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Hold" ID="4" HiQnetStateVariableKey="5644f28e-b473-432a-ae54-81ca8ba0bb4f" ClassID="733" Version="1" DefaultValue="0.001">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="5">
								<StateVariable Name="Status" ID="5" HiQnetStateVariableKey="f5249588-fb18-408a-bc25-0da05ce1a6ae" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Gain Meter" ID="6" HiQnetStateVariableKey="326b5364-5bc2-407f-8f57-b5a713256c9b" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="15" OBJ_ADDR="921346">
						<Object Name="Ch 2 IOC Limiter" Address="921346" ClassID="15" Version="1" HiQnetObjectKey="6e372e08-4cc2-4a74-81cd-a18559158d78">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="d77ae289-28b0-428c-98fb-1136156b5de9" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Attack" ID="1" HiQnetStateVariableKey="e2057d08-0e3a-4d42-8e4f-abdbc63d0f1a" ClassID="733" Version="1" DefaultValue="0.02">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Release" ID="2" HiQnetStateVariableKey="f463b6cf-3016-4372-8c9f-cfcc657b9cef" ClassID="733" Version="1" DefaultValue="0.6">
									<Data2 Len="4">CtcjPA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Threshold" ID="3" HiQnetStateVariableKey="8a890e43-8bf0-4015-899d-6e6ce837d528" ClassID="733" Version="1" DefaultValue="0.001">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Hold" ID="4" HiQnetStateVariableKey="f87c75aa-30a7-404a-9119-8f3f38ff27ca" ClassID="733" Version="1" DefaultValue="0.001">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">zczMPQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="5">
								<StateVariable Name="Status" ID="5" HiQnetStateVariableKey="dd3f5551-a306-473e-9302-5f1aaefaa2c3" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Gain Meter" ID="6" HiQnetStateVariableKey="fb052c87-454d-4bcf-8993-c6112d6c525f" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="16" OBJ_ADDR="987137">
						<Object Name="Ch 1 Limiter Suite" Address="987137" ClassID="16" Version="1" HiQnetObjectKey="b39408e1-4f31-45cd-92a6-164026ae4b64">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="788c3cfe-f553-4995-9f2c-1a72c617080e" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="757" SV_ID="1">
								<StateVariable Name="Mode" ID="1" HiQnetStateVariableKey="a491fa39-54cd-41b6-90c3-5356918987d6" ClassID="757" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="16" OBJ_ADDR="987138">
						<Object Name="Ch 2 Limiter Suite" Address="987138" ClassID="16" Version="1" HiQnetObjectKey="1e145888-0529-4fc8-be7e-d1a87aa48f36">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="be43ba7e-2cf6-43e3-9ef2-dd8654d47d71" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="757" SV_ID="1">
								<StateVariable Name="Mode" ID="1" HiQnetStateVariableKey="76747df3-b8bf-4e3c-905d-3ff5829de684" ClassID="757" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="17" OBJ_ADDR="1052929">
						<Object Name="Ch 1 Peak Limiter" Address="1052929" ClassID="17" Version="1" HiQnetObjectKey="36079b46-babf-4f83-b177-571e65215210">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="66d70db0-add0-44e4-a694-12dac4106290" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" HiQnetStateVariableKey="7ca2ff56-75d8-4da2-9159-76f75c02846d" ClassID="806" Version="1" DefaultValue="100">
									<Min>1</Min>
									<Max>201.2</Max>
									<Value>165</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="2">
								<StateVariable Name="Lookahead Delay" ID="2" HiQnetStateVariableKey="4087919a-5b02-459e-bb26-66a76055e326" ClassID="561" Version="1" DefaultValue="0.0005">
									<Min>0</Min>
									<Max>0.01</Max>
									<Value>0.0005</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Release" ID="3" HiQnetStateVariableKey="480b5c51-58c9-4b97-b275-b86547851fc1" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>0.0001</Min>
									<Max>10</Max>
									<Value>0.2</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Gain Meter" ID="4" HiQnetStateVariableKey="d81274c2-469c-46ff-89fc-1c0b18fc50ed" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Sidechain EQ Filters Enable 1" ID="5" HiQnetStateVariableKey="56cb8717-a126-4c88-b7ce-b3bb41033314" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Sidechain EQ Filters Frequency 1" ID="6" HiQnetStateVariableKey="ccb5580d-d9e7-4676-948d-a9cba768adae" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="7">
								<StateVariable Name="Sidechain EQ Filters Q 1" ID="7" HiQnetStateVariableKey="cbf63f0e-2c7c-478a-bec9-2b944254ba40" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="8">
								<StateVariable Name="Sidechain EQ Filters Slope 1" ID="8" HiQnetStateVariableKey="f068019d-0a87-4560-b882-94a54aa3531f" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="9">
								<StateVariable Name="Sidechain EQ Filters Gain 1" ID="9" HiQnetStateVariableKey="1a02a8ef-7470-45c9-b611-8b94ae58baa0" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="10">
								<StateVariable Name="Sidechain EQ Filters Type 1" ID="10" HiQnetStateVariableKey="25cb5b01-ca4f-4e30-95f7-72dab8a2a903" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Sidechain EQ Filters Enable 2" ID="11" HiQnetStateVariableKey="496cb708-4dad-4c62-8a66-e2127e4a616b" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="12">
								<StateVariable Name="Sidechain EQ Filters Frequency 2" ID="12" HiQnetStateVariableKey="a7d36269-dde5-4103-8311-2698d3b91f08" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="13">
								<StateVariable Name="Sidechain EQ Filters Q 2" ID="13" HiQnetStateVariableKey="08dca203-f957-429b-a7b9-8f1670bca0b5" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="14">
								<StateVariable Name="Sidechain EQ Filters Slope 2" ID="14" HiQnetStateVariableKey="35b5f602-63d4-4603-a4da-1eee8076de65" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Sidechain EQ Filters Gain 2" ID="15" HiQnetStateVariableKey="0ba3b1e6-db47-4fb8-9a63-2a294a948505" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="16">
								<StateVariable Name="Sidechain EQ Filters Type 2" ID="16" HiQnetStateVariableKey="7bb502cd-9030-48d5-82c6-418f176a0c9f" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Sidechain EQ Filters Enable 3" ID="17" HiQnetStateVariableKey="18643d28-64e9-4baf-88ed-1e6e3e3e5dee" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="18">
								<StateVariable Name="Sidechain EQ Filters Frequency 3" ID="18" HiQnetStateVariableKey="fb506abe-6a3a-4b0f-8de1-1a064426bedf" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="19">
								<StateVariable Name="Sidechain EQ Filters Q 3" ID="19" HiQnetStateVariableKey="a05fb570-2e85-4205-bc8a-60f048114700" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="20">
								<StateVariable Name="Sidechain EQ Filters Slope 3" ID="20" HiQnetStateVariableKey="5bade740-9c26-41d3-af95-dba6a69e6a2b" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="21">
								<StateVariable Name="Sidechain EQ Filters Gain 3" ID="21" HiQnetStateVariableKey="91f9464b-3cc0-4b3e-8d27-765fac0b0128" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="22">
								<StateVariable Name="Sidechain EQ Filters Type 3" ID="22" HiQnetStateVariableKey="54f63dbe-b293-4d66-9e43-2cfd24dae761" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="23">
								<StateVariable Name="Sidechain EQ Filters Bypass" ID="23" HiQnetStateVariableKey="5dc87f5f-d877-4bd3-ba2f-1d1687a1521a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="17" OBJ_ADDR="1052930">
						<Object Name="Ch 2 Peak Limiter" Address="1052930" ClassID="17" Version="1" HiQnetObjectKey="7bfb6aa1-7b5b-4b90-80e4-87be7489e7be">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="67627d81-bf65-450e-bea4-12104aba7bd4" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="1">
								<StateVariable Name="Threshold" ID="1" HiQnetStateVariableKey="1a9e5ee7-5c7e-4b17-a549-83634813fee6" ClassID="806" Version="1" DefaultValue="100">
									<Min>1</Min>
									<Max>201.2</Max>
									<Value>165</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="561" SV_ID="2">
								<StateVariable Name="Lookahead Delay" ID="2" HiQnetStateVariableKey="a12bada0-5544-4e19-818d-46df8b74ed16" ClassID="561" Version="1" DefaultValue="0.0005">
									<Min>0</Min>
									<Max>0.01</Max>
									<Value>0.0005</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Release" ID="3" HiQnetStateVariableKey="ff2b0deb-0621-4b07-a70a-858429f02b40" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>0.0001</Min>
									<Max>10</Max>
									<Value>0.2</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Gain Meter" ID="4" HiQnetStateVariableKey="d9f2a1a7-548a-4024-be18-90e90abb3257" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="5">
								<StateVariable Name="Sidechain EQ Filters Enable 1" ID="5" HiQnetStateVariableKey="6e098511-552b-45b5-b0c5-6415cd2c7422" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="6">
								<StateVariable Name="Sidechain EQ Filters Frequency 1" ID="6" HiQnetStateVariableKey="4c7e6b84-8a5a-4b63-ab75-03923535a063" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="7">
								<StateVariable Name="Sidechain EQ Filters Q 1" ID="7" HiQnetStateVariableKey="b6f83a3a-b78d-4481-9260-b8282bcf2eed" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="8">
								<StateVariable Name="Sidechain EQ Filters Slope 1" ID="8" HiQnetStateVariableKey="6a96dea2-fa3e-4cf9-82df-47592d9c83ec" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="9">
								<StateVariable Name="Sidechain EQ Filters Gain 1" ID="9" HiQnetStateVariableKey="1b24d333-f247-418c-8d37-e5481c89001c" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="10">
								<StateVariable Name="Sidechain EQ Filters Type 1" ID="10" HiQnetStateVariableKey="d16943b2-fd27-4d83-821c-f778bd023d4d" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Sidechain EQ Filters Enable 2" ID="11" HiQnetStateVariableKey="d5e0f164-8110-419c-9a88-7293efeecdc2" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="12">
								<StateVariable Name="Sidechain EQ Filters Frequency 2" ID="12" HiQnetStateVariableKey="94a24190-c96c-4072-974c-482fcc868361" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="13">
								<StateVariable Name="Sidechain EQ Filters Q 2" ID="13" HiQnetStateVariableKey="4fb82b5a-7286-40e7-81ac-022d64187f59" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="14">
								<StateVariable Name="Sidechain EQ Filters Slope 2" ID="14" HiQnetStateVariableKey="150a5c45-c702-4640-8857-cdf88f995591" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Sidechain EQ Filters Gain 2" ID="15" HiQnetStateVariableKey="a913b1f7-6149-4f51-8331-d24b41a34780" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="16">
								<StateVariable Name="Sidechain EQ Filters Type 2" ID="16" HiQnetStateVariableKey="3ce8fcc2-5c5f-4673-853e-f800b9ad0b8e" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Sidechain EQ Filters Enable 3" ID="17" HiQnetStateVariableKey="e4fb9340-18b3-4e79-8c98-97c489e0af50" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="18">
								<StateVariable Name="Sidechain EQ Filters Frequency 3" ID="18" HiQnetStateVariableKey="dc3a2839-730e-4f4b-8fb8-c2be92163c0a" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="19">
								<StateVariable Name="Sidechain EQ Filters Q 3" ID="19" HiQnetStateVariableKey="60d29221-ad4e-4fc1-9b9d-2eaa575d5942" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="20">
								<StateVariable Name="Sidechain EQ Filters Slope 3" ID="20" HiQnetStateVariableKey="854fa77c-248d-47a6-b8bf-fe033339c653" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="21">
								<StateVariable Name="Sidechain EQ Filters Gain 3" ID="21" HiQnetStateVariableKey="7799555b-73d9-4ef8-9c62-5791dbba5196" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="22">
								<StateVariable Name="Sidechain EQ Filters Type 3" ID="22" HiQnetStateVariableKey="7f713c60-9e51-4b00-b223-9fbe1896bd16" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="23">
								<StateVariable Name="Sidechain EQ Filters Bypass" ID="23" HiQnetStateVariableKey="784675fe-a7ac-4d7e-9205-9ca3a92016f9" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="18" OBJ_ADDR="1118721">
						<Object Name="Ch 1 RMS Limiter" Address="1118721" ClassID="18" Version="1" HiQnetObjectKey="c7b87e7f-f93b-4a1c-89c1-63439fb2f161">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="80e5cdd9-a312-49dd-aaf9-4a394df43025" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Detector Time Constant" ID="1" HiQnetStateVariableKey="a915e2b2-9dd5-4169-a056-46d8dfe8cdb1" ClassID="733" Version="1" DefaultValue="0.001">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.004</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" HiQnetStateVariableKey="7760095a-e8ed-466c-80c3-726244b8ece2" ClassID="806" Version="1" DefaultValue="100">
									<Min>1</Min>
									<Max>400</Max>
									<Value>65</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" HiQnetStateVariableKey="db06ace6-4e57-44e0-ab27-cb58a3eefe60" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.3</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" HiQnetStateVariableKey="47367be9-8598-48b4-82af-89af5e750f06" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.6063</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="Gain Meter" ID="5" HiQnetStateVariableKey="92a9f5c3-068a-4ef9-9dae-f1319d9808f9" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="18" OBJ_ADDR="1118722">
						<Object Name="Ch 2 RMS Limiter" Address="1118722" ClassID="18" Version="1" HiQnetObjectKey="48335503-fbad-4494-ba75-800263a4b4fb">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="2414366b-590e-4439-9586-194e50bbaaa7" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Detector Time Constant" ID="1" HiQnetStateVariableKey="c716c2dd-8ddf-4dd9-908b-bf9fbec24217" ClassID="733" Version="1" DefaultValue="0.001">
									<Min>0.001</Min>
									<Max>1</Max>
									<Value>0.004</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" HiQnetStateVariableKey="fb559f4c-be26-430b-a783-cce1e2023d9b" ClassID="806" Version="1" DefaultValue="100">
									<Min>1</Min>
									<Max>400</Max>
									<Value>65</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Attack" ID="3" HiQnetStateVariableKey="1fb10d5e-c72a-470a-83db-175f32b4c983" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.3</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Release" ID="4" HiQnetStateVariableKey="5e615756-2ef3-423a-8b4c-5ee779f04b32" ClassID="733" Version="1" DefaultValue="0.01">
									<Min>1E-05</Min>
									<Max>10</Max>
									<Value>0.6063</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="Gain Meter" ID="5" HiQnetStateVariableKey="9d705bb2-ae6f-42a0-98b7-7562ad69133b" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="19" OBJ_ADDR="1184513">
						<Object Name="Ch 1 Speaker Thermal Limiter" Address="1184513" ClassID="19" Version="1" HiQnetObjectKey="ec2eefa4-bf49-4803-a0ce-4af81b0674a3">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="e110e99b-da66-428d-8f6b-a02c99debe74" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Time Constant" ID="1" HiQnetStateVariableKey="b8103994-6464-4188-a82f-0c5a023b2a5d" ClassID="733" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>600</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" HiQnetStateVariableKey="81970240-6283-4ca6-8597-d65d0de81f2f" ClassID="806" Version="1" DefaultValue="100">
									<Min>1</Min>
									<Max>500</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Proportional K" ID="3" HiQnetStateVariableKey="14931fa2-7bc9-4c1f-8223-a1959d8d914e" ClassID="733" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.85</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Integral K" ID="4" HiQnetStateVariableKey="6f827466-e758-4881-953d-573c2268a3f1" ClassID="733" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.17</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Thermal Voltage" ID="5" HiQnetStateVariableKey="ee7282af-3691-427c-8817-04b98fe66875" ClassID="535" Version="1" DefaultValue="100">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="RMS Limiter Threshold Adjust" ID="6" HiQnetStateVariableKey="13391a9f-b40c-4b4c-9ab9-32a8249541e2" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="7">
								<StateVariable Name="RMS Limiter Threshold Adjust dB" ID="7" HiQnetStateVariableKey="8d96ed71-9ca1-4831-914b-613801dd01fc" ClassID="535" Version="1" DefaultValue="-40">
									<Data2 Len="4">AAAgwg==</Data2>
									<Data3 Len="4">AAAAAA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="8">
								<StateVariable Name="Gain Meter" ID="8" HiQnetStateVariableKey="e4157a61-f38b-4e3e-bcaa-802c7d6778cf" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="19" OBJ_ADDR="1184514">
						<Object Name="Ch 2 Speaker Thermal Limiter" Address="1184514" ClassID="19" Version="1" HiQnetObjectKey="c971ac36-2ea1-4f0f-b1ad-f055d7fc76b5">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="0cdaa4e8-6582-4ac6-8c58-66ac17e2c652" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Time Constant" ID="1" HiQnetStateVariableKey="d203a6d1-82c4-4a1b-9fd8-3b7a7f9618e1" ClassID="733" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>600</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="806" SV_ID="2">
								<StateVariable Name="Threshold" ID="2" HiQnetStateVariableKey="02e032a4-ef4b-457b-a919-06f4f7381c87" ClassID="806" Version="1" DefaultValue="100">
									<Min>1</Min>
									<Max>500</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Proportional K" ID="3" HiQnetStateVariableKey="ca40c49a-76b5-4aad-a505-e61c77bc3ec6" ClassID="733" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.85</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Integral K" ID="4" HiQnetStateVariableKey="61cab121-c985-4995-bb50-c5cdf6681222" ClassID="733" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0.17</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Thermal Voltage" ID="5" HiQnetStateVariableKey="0a969c92-f188-4d8d-af80-b5af3de12ab8" ClassID="535" Version="1" DefaultValue="100">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="RMS Limiter Threshold Adjust" ID="6" HiQnetStateVariableKey="74ae15f5-7027-42cb-811b-5a386ac1073a" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="7">
								<StateVariable Name="RMS Limiter Threshold Adjust dB" ID="7" HiQnetStateVariableKey="91cfd76e-d434-4d4d-bf52-72e51345bf31" ClassID="535" Version="1" DefaultValue="-40">
									<Data2 Len="4">AAAgwg==</Data2>
									<Data3 Len="4">AAAAAA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="8">
								<StateVariable Name="Gain Meter" ID="8" HiQnetStateVariableKey="faab9425-dfe9-4ccb-b722-08b0399b63fb" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="21" OBJ_ADDR="1250561">
						<Object Name="Ch 1 Processing Output" Address="1250561" ClassID="21" Version="1" HiQnetObjectKey="c41cee79-e1f6-479c-809a-ae62870d4fd1">
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="0">
								<StateVariable Name="Fader" ID="0" HiQnetStateVariableKey="9f5195cc-748b-4057-b2e5-e014bf453b46" ClassID="546" Version="1" DefaultValue="120">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="1">
								<StateVariable Name="Invert" ID="1" HiQnetStateVariableKey="8f726a60-2725-4027-b39a-e7c78e287056" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Mute Enable" ID="2" HiQnetStateVariableKey="7e15a7d2-25fc-46d2-84d1-a7efb2183e85" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Attenuator Limit" ID="3" HiQnetStateVariableKey="c1e70cf1-ff39-4593-9a73-40f65cf94da3" ClassID="546" Version="1" DefaultValue="200">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Peak Level Meter" ID="4" HiQnetStateVariableKey="72a9f102-bf7a-4079-a062-afddd55da755" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="RMS Level Meter" ID="5" HiQnetStateVariableKey="c5445549-948c-446b-9187-70e1b99dd47a" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Clip Indicator" ID="6" HiQnetStateVariableKey="6ace00e8-4100-4b71-aa07-4e2c47a16a99" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Gain Meter" ID="7" HiQnetStateVariableKey="398b7bec-1ac2-4421-b95c-701caaf3de31" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="8">
								<StateVariable Name="Unused" ID="8" HiQnetStateVariableKey="040e28d3-d46d-4953-93ab-f0aa05a8b8c4" ClassID="733" Version="1" DefaultValue="0">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="9">
								<StateVariable Name="Clip Counter" ID="9" HiQnetStateVariableKey="56e1d1e1-0c5c-47f8-b34e-38b432bb124e" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Report Clip Errors" ID="10" HiQnetStateVariableKey="61a85797-66f4-4b7a-b827-3922298ed024" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="11">
								<StateVariable Name="Clip Error Threshold" ID="11" HiQnetStateVariableKey="389f2fef-9c0f-4e75-8ec1-efa9fc432ef3" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="12">
								<StateVariable Name="Clip Error Time" ID="12" HiQnetStateVariableKey="6e062d33-8c01-4570-a92c-79af900cc8ad" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="13">
								<StateVariable Name="Clip Error Log" ID="13" HiQnetStateVariableKey="2272eb3c-ff48-45b1-bd20-f146a5737540" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="14">
								<StateVariable Name="Clip Error Last" ID="14" HiQnetStateVariableKey="b3d7ffb6-5d51-4f22-a74f-e8e58fbe5f62" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Band Gain" ID="15" HiQnetStateVariableKey="eed7ed2c-b3af-43c2-a4b2-d43652e57fa3" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>12</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="16">
								<StateVariable Name="Highpass Family" ID="16" HiQnetStateVariableKey="16024320-b203-45f5-883a-e7177c6966c9" ClassID="753" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="17">
								<StateVariable Name="Lowpass Family" ID="17" HiQnetStateVariableKey="3c249041-6172-4b5f-93ac-deed41974f8b" ClassID="753" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="21" OBJ_ADDR="1250562">
						<Object Name="Ch 2 Processing Output" Address="1250562" ClassID="21" Version="1" HiQnetObjectKey="782217fa-bfc9-4f7f-a747-8ab5fa042389">
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="0">
								<StateVariable Name="Fader" ID="0" HiQnetStateVariableKey="1b823186-f091-477c-8342-a12f7f66e6be" ClassID="546" Version="1" DefaultValue="120">
									<Min>0</Min>
									<Max>240</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="1">
								<StateVariable Name="Invert" ID="1" HiQnetStateVariableKey="be5cdb65-fa4b-4d61-9aa5-a56d50c6a394" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Mute Enable" ID="2" HiQnetStateVariableKey="a9422aa9-d66e-404b-9097-1607f6b95206" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="3">
								<StateVariable Name="Attenuator Limit" ID="3" HiQnetStateVariableKey="f7329d8d-9733-44ac-887d-30533d7b62d9" ClassID="546" Version="1" DefaultValue="200">
									<Min>40</Min>
									<Max>200</Max>
									<Value>200</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="4">
								<StateVariable Name="Peak Level Meter" ID="4" HiQnetStateVariableKey="0000c138-4a6f-4c73-8bb9-19d58ebfa549" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="5">
								<StateVariable Name="RMS Level Meter" ID="5" HiQnetStateVariableKey="7c5f84dc-e1a0-49cf-b0b5-47e7785d535d" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Clip Indicator" ID="6" HiQnetStateVariableKey="ce062d6c-0a33-4644-ae27-7de7dd56e7d4" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="7">
								<StateVariable Name="Gain Meter" ID="7" HiQnetStateVariableKey="98d6910a-aad3-42ad-8b1f-a3b881d7713c" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="8">
								<StateVariable Name="Unused" ID="8" HiQnetStateVariableKey="9f61598d-343f-4548-a01e-9e40863804c6" ClassID="733" Version="1" DefaultValue="0">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<Data1 Len="4">AAAAAA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="9">
								<StateVariable Name="Clip Counter" ID="9" HiQnetStateVariableKey="f23455ca-f142-46ee-afb8-2f753afaebe0" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="10">
								<StateVariable Name="Report Clip Errors" ID="10" HiQnetStateVariableKey="f13095fd-bc1b-4027-908f-86ea0396100a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="11">
								<StateVariable Name="Clip Error Threshold" ID="11" HiQnetStateVariableKey="8d1c9a44-a108-4249-b120-e3e37f15f962" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="12">
								<StateVariable Name="Clip Error Time" ID="12" HiQnetStateVariableKey="9cb595e4-46b7-4f9c-b7ca-64e46942a8be" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="13">
								<StateVariable Name="Clip Error Log" ID="13" HiQnetStateVariableKey="2139c57a-3c2d-4ed8-84b6-baae3afd465a" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="14">
								<StateVariable Name="Clip Error Last" ID="14" HiQnetStateVariableKey="dea6cf30-cc96-41a8-b02f-7cfdd01ae33a" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="15">
								<StateVariable Name="Band Gain" ID="15" HiQnetStateVariableKey="85412227-e0db-4eff-9351-8aa6245a99fa" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>12</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="16">
								<StateVariable Name="Highpass Family" ID="16" HiQnetStateVariableKey="900c779a-4e30-4c49-ae5b-6ecd2dcbf286" ClassID="753" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="753" SV_ID="17">
								<StateVariable Name="Lowpass Family" ID="17" HiQnetStateVariableKey="694add2c-5e3a-4df6-86e5-0e29c1f1c9ed" ClassID="753" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="22" OBJ_ADDR="1316353">
						<Object Name="Ch 1 Amp Output" Address="1316353" ClassID="22" Version="1" HiQnetObjectKey="88647766-c512-4fa2-b8e0-6259fb5ac95e">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Current Peak Level Meter" ID="0" HiQnetStateVariableKey="6224520a-ada0-4c13-abc2-89fd212f118d" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Current RMS Level Meter" ID="1" HiQnetStateVariableKey="c8df0f07-8668-4479-aaa3-b3e9ae1bd512" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="2">
								<StateVariable Name="Voltage Peak Level Meter" ID="2" HiQnetStateVariableKey="9b0615e4-13e1-4101-9829-db1ffb136b71" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="3">
								<StateVariable Name="Voltage RMS Level Meter" ID="3" HiQnetStateVariableKey="a2673e0e-0c04-4afa-8acf-c5e0ed5f9fbc" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Enable" ID="4" HiQnetStateVariableKey="1b15e6ae-8277-41b0-92d9-8682e2ed78e1" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Temperature" ID="5" HiQnetStateVariableKey="3149269d-4f08-4694-a5bf-5ff95a945146" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Sleeping" ID="6" HiQnetStateVariableKey="d1297871-bd61-45f3-96af-7b7cf3c0c2fb" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="7">
								<StateVariable Name="Clip Counter" ID="7" HiQnetStateVariableKey="5a0a2ba2-c87b-435b-a6bf-7c816b2ecf4c" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="8">
								<StateVariable Name="Temperature Deg C" ID="8" HiQnetStateVariableKey="744b960d-5b4c-44b9-a991-df6d205a318b" ClassID="535" Version="1" DefaultValue="20">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Report Thermal Errors" ID="9" HiQnetStateVariableKey="0e1f2559-e3f8-4e00-9dcf-38d61a096e44" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="10">
								<StateVariable Name="Thermal Error Threshold" ID="10" HiQnetStateVariableKey="c5d13653-1d8c-4dee-af56-7d57f23c3e5a" ClassID="616" Version="1" DefaultValue="70">
									<Min>0</Min>
									<Max>100</Max>
									<Value>70</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="11">
								<StateVariable Name="Thermal Error Log" ID="11" HiQnetStateVariableKey="84c09dac-787e-4f24-ab6c-3c74e6b48bf8" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="12">
								<StateVariable Name="Thermal Error Last" ID="12" HiQnetStateVariableKey="18fd8831-a937-47e5-be06-d72de5769833" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="13">
								<StateVariable Name="Report Clip Errors" ID="13" HiQnetStateVariableKey="390ad018-6755-4f20-8fce-82801845e199" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="14">
								<StateVariable Name="Clip Error Threshold" ID="14" HiQnetStateVariableKey="133268da-e2c5-422e-8f6a-81f2d752e1aa" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Clip Error Time" ID="15" HiQnetStateVariableKey="9fd49fa4-ee5e-42dd-abe0-ff1ead559dab" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="16">
								<StateVariable Name="Clip Error Log" ID="16" HiQnetStateVariableKey="2088cf54-924e-47fe-9425-507eca00935a" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="17">
								<StateVariable Name="Clip Error Last" ID="17" HiQnetStateVariableKey="c4f6afb9-bbcb-41bb-9a0a-27037355c3e6" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="18">
								<StateVariable Name="RMS Amp Meter" ID="18" HiQnetStateVariableKey="7806f742-a8b6-4ab5-92be-d6183e62963d" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="19">
								<StateVariable Name="RMS Volt Meter" ID="19" HiQnetStateVariableKey="eadb3d45-ac49-4dfa-b480-ff17fbd18142" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="20">
								<StateVariable Name="Peak Amp Meter" ID="20" HiQnetStateVariableKey="30995cfc-7070-4339-8099-857482de1de7" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="21">
								<StateVariable Name="Peak Volt Meter" ID="21" HiQnetStateVariableKey="a92f6932-bb87-461c-ac08-6fa4232f69a6" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="22">
								<StateVariable Name="Auto Standby Turn Off Delay" ID="22" HiQnetStateVariableKey="989c0870-5819-4e7d-8bd7-e8ab833ed23e" ClassID="616" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="Auto Standby Threshold" ID="23" HiQnetStateVariableKey="d9d09a6a-2348-422f-8e34-9b80b6703851" ClassID="546" Version="1" DefaultValue="40">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="22" OBJ_ADDR="1316354">
						<Object Name="Ch 2 Amp Output" Address="1316354" ClassID="22" Version="1" HiQnetObjectKey="3c7cfb4a-10ca-409e-98f7-8af1bdafb20d">
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="0">
								<StateVariable Name="Current Peak Level Meter" ID="0" HiQnetStateVariableKey="234e2508-0279-4c92-b9c6-151111fa95a8" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="1">
								<StateVariable Name="Current RMS Level Meter" ID="1" HiQnetStateVariableKey="87dc87c1-f717-47fd-b688-414815882c6e" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="2">
								<StateVariable Name="Voltage Peak Level Meter" ID="2" HiQnetStateVariableKey="70fcd1f6-d900-4ce5-bcc2-8dd0c4e1704e" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="3">
								<StateVariable Name="Voltage RMS Level Meter" ID="3" HiQnetStateVariableKey="9f30c379-73eb-42b2-84e7-e9540817dd71" ClassID="646" Version="1" DefaultValue="40">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Enable" ID="4" HiQnetStateVariableKey="3fd27256-02b5-4ad4-b147-e61047853ce9" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Temperature" ID="5" HiQnetStateVariableKey="dc31c7a0-08b2-4643-9e49-258d1d2386f1" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="6">
								<StateVariable Name="Sleeping" ID="6" HiQnetStateVariableKey="10c7bbd5-f624-499c-8802-6c58ebf000dd" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="7">
								<StateVariable Name="Clip Counter" ID="7" HiQnetStateVariableKey="9070f4ec-029e-4678-a80c-97bad2f9135b" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="8">
								<StateVariable Name="Temperature Deg C" ID="8" HiQnetStateVariableKey="f7edd532-4051-467b-ab92-b736cee4d4fb" ClassID="535" Version="1" DefaultValue="20">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="9">
								<StateVariable Name="Report Thermal Errors" ID="9" HiQnetStateVariableKey="599b34fc-2566-470c-9d91-1449b27f0220" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="10">
								<StateVariable Name="Thermal Error Threshold" ID="10" HiQnetStateVariableKey="93ec759d-5876-40a8-ba35-4cd1aa85fd04" ClassID="616" Version="1" DefaultValue="70">
									<Min>0</Min>
									<Max>100</Max>
									<Value>70</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="11">
								<StateVariable Name="Thermal Error Log" ID="11" HiQnetStateVariableKey="0f227081-6f73-4a9d-b201-55364c0cb48b" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="12">
								<StateVariable Name="Thermal Error Last" ID="12" HiQnetStateVariableKey="1c028c75-a938-4f64-bf26-8f28a21e064e" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="13">
								<StateVariable Name="Report Clip Errors" ID="13" HiQnetStateVariableKey="9d5e61b5-ca61-4aa4-9b66-924cc0ebfd77" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="14">
								<StateVariable Name="Clip Error Threshold" ID="14" HiQnetStateVariableKey="6a009d27-5d9d-4a25-9303-4dcba61b7be7" ClassID="616" Version="1" DefaultValue="10">
									<Min>1</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="15">
								<StateVariable Name="Clip Error Time" ID="15" HiQnetStateVariableKey="b35c6b55-5ae2-43bf-a677-bf66461f5a8d" ClassID="616" Version="1" DefaultValue="5">
									<Min>1</Min>
									<Max>10</Max>
									<Value>5</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="16">
								<StateVariable Name="Clip Error Log" ID="16" HiQnetStateVariableKey="d9dc1990-ab47-41a6-a918-41311075d2f0" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="17">
								<StateVariable Name="Clip Error Last" ID="17" HiQnetStateVariableKey="3c812f1e-e91f-4372-ab7c-1dd969e81329" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="18">
								<StateVariable Name="RMS Amp Meter" ID="18" HiQnetStateVariableKey="39ae3d9b-7e7c-4ad3-9fdb-0698ca5ee48a" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="19">
								<StateVariable Name="RMS Volt Meter" ID="19" HiQnetStateVariableKey="aacb6e86-42a1-455f-b77a-68aa142cbe4c" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="20">
								<StateVariable Name="Peak Amp Meter" ID="20" HiQnetStateVariableKey="aef02072-1323-4f4c-9bdc-08bc1fc82470" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="21">
								<StateVariable Name="Peak Volt Meter" ID="21" HiQnetStateVariableKey="4be68d6e-86dc-46bf-96c4-c565953a157e" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAD6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="22">
								<StateVariable Name="Auto Standby Turn Off Delay" ID="22" HiQnetStateVariableKey="c5af5357-dbb1-411b-b907-e91d9386807a" ClassID="616" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>240</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="23">
								<StateVariable Name="Auto Standby Threshold" ID="23" HiQnetStateVariableKey="eab1a0f6-a3c2-4ecf-b836-b28a6d3cffa5" ClassID="546" Version="1" DefaultValue="40">
									<Min>40</Min>
									<Max>200</Max>
									<Value>40</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="25" OBJ_ADDR="1382657">
						<Object Name="Ch 1 Load Supervision" Address="1382657" ClassID="25" Version="1" HiQnetObjectKey="dea070b6-5a73-49bb-a306-90f6fe6a9bed">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="6f861c13-98b4-4ac2-b88c-6e1f790cf0fe" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Low Limit" ID="1" HiQnetStateVariableKey="3779ca13-1db7-4e24-86b0-d8a397999819" ClassID="733" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>250</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="High Limit" ID="2" HiQnetStateVariableKey="b7df36da-d4fa-4d23-b1c0-e929e63a340f" ClassID="733" Version="1" DefaultValue="50">
									<Min>0</Min>
									<Max>250</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="3">
								<StateVariable Name="Testing" ID="3" HiQnetStateVariableKey="8a04cec2-e11c-4af7-a4dd-d0820f029ed0" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="585" SV_ID="4">
								<StateVariable Name="Status" ID="4" HiQnetStateVariableKey="d0fc8198-a933-4142-8e72-ae0b6ff5813b" ClassID="585" Version="1" DefaultValue="3">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="Nominal Load Impedance" ID="5" HiQnetStateVariableKey="f14c6ce4-d1ed-43bc-9cf6-ae06b45970ba" ClassID="733" Version="1" DefaultValue="8">
									<Min>1</Min>
									<Max>250</Max>
									<Value>8</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="Average Impedance" ID="6" HiQnetStateVariableKey="f777b904-2c96-45df-8dc8-62a74b93891b" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAB6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Report Errors" ID="7" HiQnetStateVariableKey="ee07af76-73d9-4d40-ae72-598d68af4572" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="8">
								<StateVariable Name="Low Limit Error Log" ID="8" HiQnetStateVariableKey="f9a37ce7-580a-4768-8364-b88a6145ec0b" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="9">
								<StateVariable Name="Low Limit Error Last" ID="9" HiQnetStateVariableKey="29c5d4ba-27de-48ed-be8c-a3ad36f1464f" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="10">
								<StateVariable Name="High Limit Error Log" ID="10" HiQnetStateVariableKey="c7ae73b6-8deb-4772-b274-ab4eeefbbe91" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="11">
								<StateVariable Name="High Limit Error Last" ID="11" HiQnetStateVariableKey="0e0b7959-1d6b-4770-b51d-d809baa007d6" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="25" OBJ_ADDR="1382658">
						<Object Name="Ch 2 Load Supervision" Address="1382658" ClassID="25" Version="1" HiQnetObjectKey="dadcf31f-81a3-4ab5-8f5b-8036580ec785">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="3ade1816-9733-44b1-8697-2be81fe44d00" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Low Limit" ID="1" HiQnetStateVariableKey="602162b9-b734-4de7-96a4-aed88462cb54" ClassID="733" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>250</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="High Limit" ID="2" HiQnetStateVariableKey="28a4d1b7-301e-4265-8869-87d1fcc1ae50" ClassID="733" Version="1" DefaultValue="50">
									<Min>0</Min>
									<Max>250</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="3">
								<StateVariable Name="Testing" ID="3" HiQnetStateVariableKey="5ccf4945-bb03-462d-95d0-5ce915f92a2f" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="585" SV_ID="4">
								<StateVariable Name="Status" ID="4" HiQnetStateVariableKey="9ef5e418-1cba-4284-937c-0ebf5e62cea1" ClassID="585" Version="1" DefaultValue="3">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="Nominal Load Impedance" ID="5" HiQnetStateVariableKey="d4ad4d41-0119-42ab-a6ad-47b0b2d3dcf0" ClassID="733" Version="1" DefaultValue="8">
									<Min>1</Min>
									<Max>250</Max>
									<Value>8</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="6">
								<StateVariable Name="Average Impedance" ID="6" HiQnetStateVariableKey="c4dafa92-84be-44f6-b2fa-2b03ccda3eb7" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAB6Qw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Report Errors" ID="7" HiQnetStateVariableKey="20ac607f-6693-4f92-ac4e-98583a41bded" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="8">
								<StateVariable Name="Low Limit Error Log" ID="8" HiQnetStateVariableKey="d4494c5f-90b8-4d29-888a-13db6ce815bc" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="9">
								<StateVariable Name="Low Limit Error Last" ID="9" HiQnetStateVariableKey="b3f49be1-7c75-4561-92d5-7d61e65f31cb" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="10">
								<StateVariable Name="High Limit Error Log" ID="10" HiQnetStateVariableKey="d0f303a6-f3ad-4deb-a6fc-ecfc2f5ddd8b" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="11">
								<StateVariable Name="High Limit Error Last" ID="11" HiQnetStateVariableKey="4b342f3e-a039-49b7-91da-4c51e6e32fff" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="26" OBJ_ADDR="1448449">
						<Object Name="Ch 1 Sweep Load Monitoring" Address="1448449" ClassID="26" Version="1" HiQnetObjectKey="906b295a-a5ea-4467-8ceb-adba2e1d5ef6">
							<STATE_VARIABLE SV_CLASSID="622" SV_ID="0">
								<StateVariable Name="Acquire Mode" ID="0" HiQnetStateVariableKey="ce9cce85-2008-4d1c-ad6e-237c05f13749" ClassID="622" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>5</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Start Freq" ID="1" HiQnetStateVariableKey="e61c2792-58b7-4625-9a12-eb8074be4e9b" ClassID="587" Version="1" DefaultValue="20">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="2">
								<StateVariable Name="Stop Freq" ID="2" HiQnetStateVariableKey="dd730c04-fade-47db-8186-d2d215412b1f" ClassID="587" Version="1" DefaultValue="20000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="3">
								<StateVariable Name="Impedance Reference" ID="3" HiQnetStateVariableKey="8927f102-1c61-4f40-be0f-2b92c8104ffa" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="4">
								<StateVariable Name="Impedance Response" ID="4" HiQnetStateVariableKey="4fb8ff47-c151-45df-bee7-2bee45e35662" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="5">
								<StateVariable Name="Frequency Reference" ID="5" HiQnetStateVariableKey="49a81174-663c-4fc5-9cd2-12868ba01da4" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="6">
								<StateVariable Name="Frequency Response" ID="6" HiQnetStateVariableKey="41aa3bbd-8f29-49ab-877a-a97b30aaee61" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="7">
								<StateVariable Name="Impedance PassFail" ID="7" HiQnetStateVariableKey="ed50e71d-0947-435d-931a-63823e4c4a7f" ClassID="625" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="8">
								<StateVariable Name="Freq Resp PassFail" ID="8" HiQnetStateVariableKey="4cd6df95-59d7-4dc2-808c-ac73c1945463" ClassID="625" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="649" SV_ID="9">
								<StateVariable Name="Curve Notes" ID="9" HiQnetStateVariableKey="9a350e6f-7af8-47bb-8c16-2a9589e0e0fe" ClassID="649" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>514</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="10">
								<StateVariable Name="Slm Error Log" ID="10" HiQnetStateVariableKey="073ea13f-16c8-4937-9356-a79936b18f34" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="11">
								<StateVariable Name="Slm Error Last" ID="11" HiQnetStateVariableKey="fab8036a-61ef-424c-9796-ac05594a8a03" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="26" OBJ_ADDR="1448450">
						<Object Name="Ch 2 Sweep Load Monitoring" Address="1448450" ClassID="26" Version="1" HiQnetObjectKey="54f20ed7-3752-4f03-835b-a78af622d52c">
							<STATE_VARIABLE SV_CLASSID="622" SV_ID="0">
								<StateVariable Name="Acquire Mode" ID="0" HiQnetStateVariableKey="2c02dad4-7203-4a75-90ae-ab2566dc4175" ClassID="622" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>5</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Start Freq" ID="1" HiQnetStateVariableKey="fe4d3299-b769-46aa-b1f0-8c791f2d511c" ClassID="587" Version="1" DefaultValue="20">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="2">
								<StateVariable Name="Stop Freq" ID="2" HiQnetStateVariableKey="f6d06b2b-ee23-416f-a7fe-60e524596d4f" ClassID="587" Version="1" DefaultValue="20000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="3">
								<StateVariable Name="Impedance Reference" ID="3" HiQnetStateVariableKey="97c1739e-f56d-43a0-b61c-f18f545659e8" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="4">
								<StateVariable Name="Impedance Response" ID="4" HiQnetStateVariableKey="054e842b-c0e1-4c7e-ba13-77b30c1c3efb" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="5">
								<StateVariable Name="Frequency Reference" ID="5" HiQnetStateVariableKey="d2209556-073d-40ec-a0ed-3bc9ddef2dd0" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="648" SV_ID="6">
								<StateVariable Name="Frequency Response" ID="6" HiQnetStateVariableKey="02e0a0db-e101-4a81-aea3-a32d60364524" ClassID="648" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>2280</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="7">
								<StateVariable Name="Impedance PassFail" ID="7" HiQnetStateVariableKey="e4416af8-2e07-4a24-b5db-0d69216eec03" ClassID="625" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="625" SV_ID="8">
								<StateVariable Name="Freq Resp PassFail" ID="8" HiQnetStateVariableKey="e6b35265-42ca-43a8-a887-7c3e6e24bb72" ClassID="625" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="649" SV_ID="9">
								<StateVariable Name="Curve Notes" ID="9" HiQnetStateVariableKey="9714eea0-75ae-4953-840c-5fd807fdd5ad" ClassID="649" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>514</Max>
									<Block Len="0"></Block>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="10">
								<StateVariable Name="Slm Error Log" ID="10" HiQnetStateVariableKey="1c1dc86c-b9db-4521-841a-16b1cd67aa38" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="11">
								<StateVariable Name="Slm Error Last" ID="11" HiQnetStateVariableKey="de85bae2-c307-46c4-abfe-a8376e67d6da" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="27" OBJ_ADDR="1448704">
						<Object Name="Common Sweep Load Monitoring" Address="1448704" ClassID="27" Version="1" HiQnetObjectKey="7b53a7af-cb31-41b7-bd2a-80b0aa982654">
							<STATE_VARIABLE SV_CLASSID="623" SV_ID="0">
								<StateVariable Name="Sweep Resolution" ID="0" HiQnetStateVariableKey="92be1ad5-d7ef-410d-8c5f-1c776018246d" ClassID="623" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>6</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Sweep Start Freq" ID="1" HiQnetStateVariableKey="152f0498-fe5c-4cd3-8833-0f64324f5761" ClassID="587" Version="1" DefaultValue="20">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="2">
								<StateVariable Name="Sweep Stop Freq" ID="2" HiQnetStateVariableKey="744e8944-e1ac-4c94-82de-7a749397858a" ClassID="587" Version="1" DefaultValue="20000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>20000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="3">
								<StateVariable Name="Test in progress" ID="3" HiQnetStateVariableKey="b2404e13-f88b-4631-8560-81c3c5fcc916" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Report Slm Errors" ID="4" HiQnetStateVariableKey="dc462be6-56d4-4a6f-8cab-3035b71bd3f5" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="550" SV_ID="5">
								<StateVariable Name="Impedance Test Tolerance" ID="5" HiQnetStateVariableKey="6c76c7e9-5025-4ab3-9e6c-7aa155d2e500" ClassID="550" Version="1" DefaultValue="10">
									<Min>10</Min>
									<Max>100</Max>
									<Value>10</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="624" SV_ID="6">
								<StateVariable Name="Frequency Response Test Tolerance" ID="6" HiQnetStateVariableKey="9250a878-8aad-4039-a015-34ff4194e44d" ClassID="624" Version="1" DefaultValue="3">
									<Min>3</Min>
									<Max>25</Max>
									<Value>3</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Start Sweep" ID="7" HiQnetStateVariableKey="65cd22d9-be98-4946-b4a8-8e688cae6d89" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="8">
								<StateVariable Name="Abort Sweep" ID="8" HiQnetStateVariableKey="56cee950-c2d0-4392-b0a6-4d50251662a6" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="11" OBJ_ADDR="1510144">
						<Object Name="Signal Generator" Address="1510144" ClassID="11" Version="1" HiQnetObjectKey="4381913a-b2f0-411d-9081-5449b2d605ed">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="ac34cbd7-96a1-405b-a575-0ce03a8496c9" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="737" SV_ID="1">
								<StateVariable Name="Mode" ID="1" HiQnetStateVariableKey="f5eaedf6-3b53-4863-acf1-4bb73c2eec18" ClassID="737" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="546" SV_ID="2">
								<StateVariable Name="Master Gain" ID="2" HiQnetStateVariableKey="e2a81c51-9d06-4661-a886-2ae0f94fdbba" ClassID="546" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>240</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="3">
								<StateVariable Name="Frequency" ID="3" HiQnetStateVariableKey="6b23a045-590a-4ac9-8017-5383aec41616" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="33" OBJ_ADDR="1581312">
						<Object Name="Signal Generator EQ Filters" Address="1581312" ClassID="33" Version="1" HiQnetObjectKey="94fb56d3-9d22-4b96-992b-6ee86fc9b4cd">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable 1" ID="0" HiQnetStateVariableKey="c1f1bf28-a6a6-412d-98d3-0710adaf9bff" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="1">
								<StateVariable Name="Frequency 1" ID="1" HiQnetStateVariableKey="8a399495-488a-4112-9746-a41d0e73254c" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="2">
								<StateVariable Name="Q 1" ID="2" HiQnetStateVariableKey="b3dda868-f41a-41c1-b0d8-02a1fcb8a469" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="3">
								<StateVariable Name="Slope 1" ID="3" HiQnetStateVariableKey="a2e35c09-18eb-4e81-9a51-7b1627079ae7" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="4">
								<StateVariable Name="Gain 1" ID="4" HiQnetStateVariableKey="f5cd6665-975e-4a4f-b39c-eae25706c9bf" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="5">
								<StateVariable Name="Type 1" ID="5" HiQnetStateVariableKey="4a47590b-4c1b-4b61-9d9b-aaf61d6047fe" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Enable 2" ID="6" HiQnetStateVariableKey="62bb77c8-9ea5-4d40-8eaf-54f87fd2a056" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="7">
								<StateVariable Name="Frequency 2" ID="7" HiQnetStateVariableKey="f8e88680-fac4-4883-b05d-21aafccd8e21" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="8">
								<StateVariable Name="Q 2" ID="8" HiQnetStateVariableKey="bacc6829-040d-4612-9f63-774f0f45e16c" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="9">
								<StateVariable Name="Slope 2" ID="9" HiQnetStateVariableKey="1069fd3a-0b55-48c2-a9fc-e68ae2ad7a4b" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="10">
								<StateVariable Name="Gain 2" ID="10" HiQnetStateVariableKey="88c17249-2e91-466e-bcd4-3a73d49506ab" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="11">
								<StateVariable Name="Type 2" ID="11" HiQnetStateVariableKey="640934ad-d306-4247-84cc-932499dd6f21" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Enable 3" ID="12" HiQnetStateVariableKey="b35c716a-f013-4fff-bcf3-e27333400ef5" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="13">
								<StateVariable Name="Frequency 3" ID="13" HiQnetStateVariableKey="c200deee-bd39-4a01-a8de-9f8ea4e0f9ce" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="14">
								<StateVariable Name="Q 3" ID="14" HiQnetStateVariableKey="84ebd3e8-4caf-4680-ab02-638a855fd2e0" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="15">
								<StateVariable Name="Slope 3" ID="15" HiQnetStateVariableKey="bc05d55c-902f-4b26-8132-ea48c470b015" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="16">
								<StateVariable Name="Gain 3" ID="16" HiQnetStateVariableKey="560a4331-761b-4bf0-9b93-97bb82d22bb9" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="17">
								<StateVariable Name="Type 3" ID="17" HiQnetStateVariableKey="445a264a-90f0-44a6-833f-134f7ab04c1b" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Enable 4" ID="18" HiQnetStateVariableKey="04ec50a6-c7ae-452e-a6d6-67699a426297" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="587" SV_ID="19">
								<StateVariable Name="Frequency 4" ID="19" HiQnetStateVariableKey="3932119e-2d91-4565-a946-42fa148e8bf8" ClassID="587" Version="1" DefaultValue="1000">
									<Min>20</Min>
									<Max>20000</Max>
									<Value>1000</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="588" SV_ID="20">
								<StateVariable Name="Q 4" ID="20" HiQnetStateVariableKey="9fb6f7f9-d049-492c-b5e4-7bed2c204b5e" ClassID="588" Version="1" DefaultValue="4">
									<Min>0.1</Min>
									<Max>35</Max>
									<Value>4</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="668" SV_ID="21">
								<StateVariable Name="Slope 4" ID="21" HiQnetStateVariableKey="269b93f4-0385-4815-ba51-cbc25db9e62e" ClassID="668" Version="1" DefaultValue="6">
									<Min>0.1</Min>
									<Max>12</Max>
									<Value>6</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="589" SV_ID="22">
								<StateVariable Name="Gain 4" ID="22" HiQnetStateVariableKey="6dfe109c-23e3-45be-9ffa-da5bb2eef824" ClassID="589" Version="1" DefaultValue="0">
									<Min>-24</Min>
									<Max>24</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="665" SV_ID="23">
								<StateVariable Name="Type 4" ID="23" HiQnetStateVariableKey="8689f08d-bf28-42d7-9131-c1f4d2ece244" ClassID="665" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>10</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="31" OBJ_ADDR="1646336">
						<Object Name="Error Reporting" Address="1646336" ClassID="31" Version="1" HiQnetObjectKey="76c972ab-124f-4b0d-a854-615dce61c2bc">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Report Line Voltage Errors" ID="0" HiQnetStateVariableKey="5d52f4a0-aeb3-46b0-84d8-87019383b649" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Low Line Voltage Error Threshold" ID="1" HiQnetStateVariableKey="90c6c5cc-71b1-493e-82fe-f5db2f93f707" ClassID="733" Version="1" DefaultValue="90">
									<Min>85</Min>
									<Max>277</Max>
									<Value>90</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="High Line Voltage Error Threshold" ID="2" HiQnetStateVariableKey="a9307d3a-71ab-4286-bbd0-b6f0ffcd25fb" ClassID="733" Version="1" DefaultValue="265">
									<Min>85</Min>
									<Max>277</Max>
									<Value>265</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="3">
								<StateVariable Name="Low Line Voltage  Limit Error Log" ID="3" HiQnetStateVariableKey="c443c1eb-1af5-43cb-9f2e-400d2764e762" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Low Line Voltage  Limit Error Last" ID="4" HiQnetStateVariableKey="3ab9ab51-f329-4888-a0d7-25ec73b933e4" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="5">
								<StateVariable Name="High Line Voltage Limit Error Log" ID="5" HiQnetStateVariableKey="138388ef-4415-4d47-956a-23ca717535c4" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="High Line Voltage  Limit Error Last" ID="6" HiQnetStateVariableKey="f14e9d35-5b64-42bb-99ed-ef567bb05bed" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="7">
								<StateVariable Name="Report Power Supply Thermal Errors" ID="7" HiQnetStateVariableKey="a2f406b8-9b70-467c-a402-b43cf72d0b64" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="8">
								<StateVariable Name="Power Supply Thermal Error Threshold" ID="8" HiQnetStateVariableKey="ccddb00a-1ebc-4a41-9fce-fe13f08adbbd" ClassID="616" Version="1" DefaultValue="70">
									<Min>0</Min>
									<Max>100</Max>
									<Value>70</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="9">
								<StateVariable Name="Power Supply Thermal Error Log" ID="9" HiQnetStateVariableKey="f95a6e68-812c-46be-a19c-700860d1eddb" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="10">
								<StateVariable Name="Power Supply Thermal Error Last" ID="10" HiQnetStateVariableKey="be8886b9-ea88-495b-9ee6-dfa09dc2690e" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="11">
								<StateVariable Name="Report Fan Errors" ID="11" HiQnetStateVariableKey="d2eeb933-40e5-40d9-841c-2bcb510a5a42" ClassID="512" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="12">
								<StateVariable Name="Fan Error Log" ID="12" HiQnetStateVariableKey="9fb17900-1471-4f44-b3ca-83f44f327405" ClassID="609" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="13">
								<StateVariable Name="Fan Error Last" ID="13" HiQnetStateVariableKey="338c59f1-1906-45f7-b5a2-2197a2d86061" ClassID="733" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1E+37</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="14">
								<StateVariable Name="Erase All Error Logs" ID="14" HiQnetStateVariableKey="8c5343b2-7672-4f55-8eba-230fad74a226" ClassID="616" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="15">
								<StateVariable Name="Amp Output Clip Log Display Control" ID="15" HiQnetStateVariableKey="da6402d6-6d7b-4832-96ae-af1eca787c81" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="16">
								<StateVariable Name="Analog Input Clip Log Display Control" ID="16" HiQnetStateVariableKey="c7f933c2-1ba2-435f-878b-456cb10a1872" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Amp Output Thermal Log Display Control" ID="17" HiQnetStateVariableKey="53e3fd99-486d-4eeb-ad7b-77f926a53be9" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="18">
								<StateVariable Name="Load Supervision Low Log Display Control" ID="18" HiQnetStateVariableKey="901ed858-0fc3-487e-9844-c51a438ca9c8" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Load Supervision High Log Display Control" ID="19" HiQnetStateVariableKey="652358b2-7ca2-4004-887b-22887fb4b466" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="20">
								<StateVariable Name="Slm Log Display Control" ID="20" HiQnetStateVariableKey="9fd5e97c-62bc-446a-abad-1e8eadf0152c" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="21">
								<StateVariable Name="Line Voltage Log Display Control" ID="21" HiQnetStateVariableKey="bd3205fe-b6e9-42ae-ac50-984caf6dc48d" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="22">
								<StateVariable Name="Fan Log Display Control" ID="22" HiQnetStateVariableKey="59a52c6b-f227-4898-b508-db0aa1defbb9" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="23">
								<StateVariable Name="Clear All Log Display Control" ID="23" HiQnetStateVariableKey="8b354434-9c9c-451a-968c-3b06eead433e" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="24">
								<StateVariable Name="Report Source Change via Network" ID="24" HiQnetStateVariableKey="4a01c2e5-1c90-460d-b706-1af88626c730" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="0" OBJ_ADDR="1703936">
						<Object Name="Amp Global" Address="1703936" ClassID="0" Version="1" HiQnetObjectKey="2edcee0b-3693-48e8-bfed-bf9e83f0bce8">
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="0">
								<StateVariable Name="Model" ID="0" HiQnetStateVariableKey="1fba0f2c-9afc-4c5b-8517-77fd2ab9d164" ClassID="616" Version="1" DefaultValue="2">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="740" SV_ID="1">
								<StateVariable Name="Mode" ID="1" HiQnetStateVariableKey="ea772ee3-01dc-44e9-bd65-82372a65a33a" ClassID="740" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">NQA=</DataF>
									<DataF2 Len="2">NQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="2">
								<StateVariable Name="Compressor Tie" ID="2" HiQnetStateVariableKey="52a19d8d-6aaf-4fa0-8611-cb1a67bf895a" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="3">
								<StateVariable Name="Limiter Tie" ID="3" HiQnetStateVariableKey="f48ada8e-9c9a-4663-a4ce-d69500a8a247" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="4">
								<StateVariable Name="Attenuator Link" ID="4" HiQnetStateVariableKey="a09c03b8-1716-459d-8d1f-5590545508aa" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="FF Voltage Scale Factor" ID="5" HiQnetStateVariableKey="7b853f04-351a-4658-bfb3-9863f666fb05" ClassID="733" Version="1" DefaultValue="201.2">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="FB Voltage Scale Factor" ID="6" HiQnetStateVariableKey="fb8c6ae7-4297-4ea5-8076-205e960fc6d4" ClassID="733" Version="1" DefaultValue="167.3">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="FB Current Scale Factor" ID="7" HiQnetStateVariableKey="498226e1-3229-4ead-a565-4e98cda3a59b" ClassID="733" Version="1" DefaultValue="75">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="8">
								<StateVariable Name="Prop VCC Scale Factor" ID="8" HiQnetStateVariableKey="63e946bb-13c7-46d5-8e44-5573796ddc6a" ClassID="733" Version="1" DefaultValue="160">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="515" SV_ID="9">
								<StateVariable Name="Front Panel Lockout" ID="9" HiQnetStateVariableKey="e0aa2138-a1a7-4d69-ae25-bcd731306de8" ClassID="515" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="10">
								<StateVariable Name="Sample Rate" ID="10" HiQnetStateVariableKey="d4fc5d2a-d1b2-42e7-82df-a1282d3bb581" ClassID="616" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="11">
								<StateVariable Name="Hardware Revision" ID="11" HiQnetStateVariableKey="d8de77ea-522d-4e59-88a7-7062e11ba0f6" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">/w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="12">
								<StateVariable Name="Display Led Type" ID="12" HiQnetStateVariableKey="81d532d5-ee01-48c1-9137-61b65642e2ce" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="743" SV_ID="13">
								<StateVariable Name="Display Bar Meter Type" ID="13" HiQnetStateVariableKey="3758cbd2-8b0f-45a5-a0dd-08f151319e66" ClassID="743" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Aw==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="14">
								<StateVariable Name="Display Diagnostic Mode Enable" ID="14" HiQnetStateVariableKey="8cdc5e13-b23b-413c-8a23-6adf83f72f3b" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="15">
								<StateVariable Name="Amp Gain" ID="15" HiQnetStateVariableKey="9fd2532e-3cff-49d8-b9e2-c8754e9d7cb3" ClassID="733" Version="1" DefaultValue="23.95">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="16">
								<StateVariable Name="Voltage At 8 Ohm Max Rated Power" ID="16" HiQnetStateVariableKey="be961a62-b56a-426d-b162-5691fe0cc8fc" ClassID="733" Version="1" DefaultValue="100">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="17">
								<StateVariable Name="Locate" ID="17" HiQnetStateVariableKey="95f6b4c5-3ffb-47ae-8ad0-d03983cced40" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="689" SV_ID="18">
								<StateVariable Name="Front Panel Blackout" ID="18" HiQnetStateVariableKey="b9e60650-eede-4604-8698-892df32ac453" ClassID="689" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>3</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="19">
								<StateVariable Name="Usb Lockout" ID="19" HiQnetStateVariableKey="f81b3e09-50ab-4d0e-8bcb-f42789f98610" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="20">
								<StateVariable Name="DSP Bypass" ID="20" HiQnetStateVariableKey="08748d03-5cfe-4ad3-881d-dd8406496a4b" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="746" SV_ID="21">
								<StateVariable Name="Fixed Gain Mode" ID="21" HiQnetStateVariableKey="04e0bacc-5cb7-48ed-891d-2b854fdb9197" ClassID="746" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>2</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="22">
								<StateVariable Name="InternalPassword" ID="22" HiQnetStateVariableKey="6efd5d2d-111d-43ed-b1c2-516dbfcb39f0" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">EgA=</Data3>
									<Data1 Len="16">YQB1ADYAYgBhAHQAZAB4AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="23">
								<StateVariable Name="Usb Overcurrent" ID="23" HiQnetStateVariableKey="9afe2717-f4a1-41ba-8e25-da57418a7e96" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="24">
								<StateVariable Name="Usb Device Detected" ID="24" HiQnetStateVariableKey="1c3d7150-3e2e-4283-b03b-3da9d4210dfe" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="756" SV_ID="25">
								<StateVariable Name="Disable Protocol" ID="25" HiQnetStateVariableKey="f781aa00-8aca-4e5a-a3f2-513cef085cf6" ClassID="756" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="26">
								<StateVariable Name="Hiqnet Address Display Control" ID="26" HiQnetStateVariableKey="f934f2a8-082e-4d12-b66a-ce131c46d67b" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="27">
								<StateVariable Name="DHCP Display Control" ID="27" HiQnetStateVariableKey="7c651c76-9046-4e7f-921a-c0e219a9457e" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="28">
								<StateVariable Name="IP Address Display Control" ID="28" HiQnetStateVariableKey="23391ecf-1430-4a8e-a243-41b2dab1938a" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="29">
								<StateVariable Name="Subnet Mask Display Control" ID="29" HiQnetStateVariableKey="06d374f0-39b8-4ab3-a84a-d51d9873825f" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="30">
								<StateVariable Name="Preset Recall Display Control" ID="30" HiQnetStateVariableKey="ca31441f-7d8e-4c30-8c63-083dbe7f2c71" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="31">
								<StateVariable Name="Delay FIR Coeff Calculation" ID="31" HiQnetStateVariableKey="db92a76c-7aa0-4289-86d9-a174c561b3e5" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<Data1 Len="1">AQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="32">
								<StateVariable Name="Front Panel Display Home Screen" ID="32" HiQnetStateVariableKey="c9c27df3-ca92-4d74-9a66-61f28ba7248d" ClassID="512" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="794" SV_ID="33">
								<StateVariable Name="VRACKPrimaryInput" ID="33" HiQnetStateVariableKey="2d9c1871-42e1-499e-beec-9444320b3fca" ClassID="794" Version="1" DefaultValue="9">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Dw==</Data3>
									<Data1 Len="1">CQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="794" SV_ID="34">
								<StateVariable Name="VRACKSecondaryInput" ID="34" HiQnetStateVariableKey="8baf240f-d915-4c18-9931-5779eec47090" ClassID="794" Version="1" DefaultValue="2">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Dw==</Data3>
									<Data1 Len="1">Ag==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="795" SV_ID="35">
								<StateVariable Name="VRACKOutputConfig" ID="35" HiQnetStateVariableKey="5a3379ec-ef7b-494b-a848-ba5d951c47a7" ClassID="795" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">DA==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="36">
								<StateVariable Name="Restore All SVs To Default" ID="36" HiQnetStateVariableKey="bd2e6dc6-9fc8-4e64-8150-a1dd8e2d84a5" ClassID="616" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="1" OBJ_ADDR="1704192">
						<Object Name="Amp Info" Address="1704192" ClassID="1" Version="1" HiQnetObjectKey="1ac4866e-4100-4465-82b7-6a1ee87ca248">
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="0">
								<StateVariable Name="User Label 1" ID="0" HiQnetStateVariableKey="c201ac6c-ab66-41ce-bf88-0fa150172561" ClassID="517" Version="1" DefaultValue="Channel 1">
									<Min>0</Min>
									<Max>64</Max>
									<Value>M20 FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="1">
								<StateVariable Name="User Label 2" ID="1" HiQnetStateVariableKey="ad5cf405-104d-4dc3-b337-881df11321b9" ClassID="517" Version="1" DefaultValue="Channel 2">
									<Min>0</Min>
									<Max>64</Max>
									<Value>M20 FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="2">
								<StateVariable Name="Date Code" ID="2" HiQnetStateVariableKey="792334e8-3195-4325-bc74-b09e0dce2e54" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="3">
								<StateVariable Name="Manufacturer" ID="3" HiQnetStateVariableKey="69641b43-af28-4ce5-bb25-352d4fa13345" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="4">
								<StateVariable Name="Model" ID="4" HiQnetStateVariableKey="368289ea-a362-4805-aaf8-43318c50758e" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="5">
								<StateVariable Name="Serial Number" ID="5" HiQnetStateVariableKey="48b23f89-0d19-4bbd-8bcb-fa37f348f17b" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="6">
								<StateVariable Name="Data LED" ID="6" HiQnetStateVariableKey="3399521f-34c2-4204-8011-9ea3b472363b" ClassID="512" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>1</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="7">
								<StateVariable Name="Firmware Version Timestamp" ID="7" HiQnetStateVariableKey="c0621d54-6a86-429b-bea5-e4a2b2393103" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="8">
								<StateVariable Name="Firmware Version Number" ID="8" HiQnetStateVariableKey="d038259a-26fd-4ff8-b57d-f360da170199" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="9">
								<StateVariable Name="Venue Table" ID="9" HiQnetStateVariableKey="4b90665e-8f72-4974-94f2-d7d23a11374c" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">+v8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="10">
								<StateVariable Name="Node Attributes" ID="10" HiQnetStateVariableKey="c0593c6f-4a33-4052-b420-d06b41c95074" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">+v8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="11">
								<StateVariable Name="Work Group" ID="11" HiQnetStateVariableKey="1307115a-286f-485b-991d-71cdd09d3266" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">AAI=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="12">
								<StateVariable Name="Operating Time" ID="12" HiQnetStateVariableKey="a754b0fe-54b4-4f56-bf33-0d9560e5859c" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="13">
								<StateVariable Name="Display Firmware Version String" ID="13" HiQnetStateVariableKey="a8351cfb-ee1a-4b7f-962f-df79a00d93cc" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="14">
								<StateVariable Name="Firmware Version String" ID="14" HiQnetStateVariableKey="24739580-355d-4709-a94a-b4da574d60ac" ClassID="517" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="2" OBJ_ADDR="1704448">
						<Object Name="Miscellaneous" Address="1704448" ClassID="2" Version="1" HiQnetObjectKey="3d77b869-1cba-4de0-9eeb-ef31d9a2be9c">
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="0">
								<StateVariable Name="DSP Crunch CPU Utilization" ID="0" HiQnetStateVariableKey="9bf42178-4f2d-4050-b866-119ecff57d9d" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="1">
								<StateVariable Name="DSP Process CPU Utilization" ID="1" HiQnetStateVariableKey="1599a4ed-5f83-4f8b-8276-6de22d38accb" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="2">
								<StateVariable Name="DSP Workload" ID="2" HiQnetStateVariableKey="d1840b70-9e5d-4f56-a8e1-e8dc99d129ce" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="533" SV_ID="3">
								<StateVariable Name="DSP Warped Workload" ID="3" HiQnetStateVariableKey="4a16a7ad-c9b3-4678-93e9-3edbb8e1fba3" ClassID="533" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">ZA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="3" OBJ_ADDR="1704704">
						<Object Name="CobraNet General" Address="1704704" ClassID="3" Version="1" HiQnetObjectKey="5c278173-3371-4b3d-9a4e-d045ad257afe">
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="0">
								<StateVariable Name="System Name" ID="0" HiQnetStateVariableKey="017e49b7-72ab-464b-87de-f81cf3715c87" ClassID="517" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>64</Max>
									<Value>System Name</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="758" SV_ID="1">
								<StateVariable Name="System Description" ID="1" HiQnetStateVariableKey="420736fb-304e-4b82-8fc5-57e192a60a44" ClassID="758" Version="1" DefaultValue="Itech-CN CobraNet version 2.11.6">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">gAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="2">
								<StateVariable Name="System Location" ID="2" HiQnetStateVariableKey="8374dfa7-5b9b-4f3e-be18-f7feb184748c" ClassID="517" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>64</Max>
									<Value>System Location</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="3">
								<StateVariable Name="System Contact" ID="3" HiQnetStateVariableKey="ac8832c6-f352-44f5-ac8d-0b5775b36f98" ClassID="517" Version="1" DefaultValue="">
									<Min>0</Min>
									<Max>64</Max>
									<Value>System Contact</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="4">
								<StateVariable Name="Firmware Protocol Version" ID="4" HiQnetStateVariableKey="834c14ce-5ba3-4b35-bb92-532a65270181" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="5">
								<StateVariable Name="Firmware Major Version" ID="5" HiQnetStateVariableKey="150faa30-c195-46f4-a418-b932856962a2" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="6">
								<StateVariable Name="Firmware Minor Version" ID="6" HiQnetStateVariableKey="31a4b979-1eec-4c0b-9b9c-63e90afabbce" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="628" SV_ID="7">
								<StateVariable Name="Error Indicators" ID="7" HiQnetStateVariableKey="07998469-be22-4943-910e-a524a8bc866a" ClassID="628" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">DQAHAA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="8">
								<StateVariable Name="Conductor Indicator" ID="8" HiQnetStateVariableKey="ea0f0325-a465-44ae-97de-f877f8b45b86" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="9">
								<StateVariable Name="Conductor Priority" ID="9" HiQnetStateVariableKey="72360801-eb3b-4327-a453-2ce29049cf02" ClassID="616" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>255</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="629" SV_ID="10">
								<StateVariable Name="Ethernet Status" ID="10" HiQnetStateVariableKey="9879bd3b-ac43-4e7a-90b7-a3b88449f92e" ClassID="629" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="11">
								<StateVariable Name="Ethernet Rx Activity" ID="11" HiQnetStateVariableKey="778ca32f-bd83-47a4-9449-b098f1929231" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="12">
								<StateVariable Name="Ethernet Tx Activity" ID="12" HiQnetStateVariableKey="b7c300bb-d186-4544-8112-b140d0a6c00f" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="684" SV_ID="13">
								<StateVariable Name="Static IP Address" ID="13" HiQnetStateVariableKey="e55e95c3-5dbb-4ce8-aeb7-f2475b9fbb47" ClassID="684" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Value>0</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="684" SV_ID="14">
								<StateVariable Name="IP Address" ID="14" HiQnetStateVariableKey="1c87f4f3-9e7f-49fb-8341-06b9b6e8f5f7" ClassID="684" Version="1" DefaultValue="0">
									<Min>0</Min>
									<Max>4294967295</Max>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="654" SV_ID="15">
								<StateVariable Name="MAC Address" ID="15" HiQnetStateVariableKey="f663db61-fd00-4c58-85ee-a26d2f95e965" ClassID="654" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">JAA=</Data3>
									<DataF Len="2">MAA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="656" SV_ID="16">
								<StateVariable Name="Sample Rate" ID="16" HiQnetStateVariableKey="1deaf6b0-818a-4194-993b-c9fca81082fd" ClassID="656" Version="1" DefaultValue="1">
									<Min>0</Min>
									<Max>1</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="655" SV_ID="17">
								<StateVariable Name="Latency" ID="17" HiQnetStateVariableKey="b0937a08-9e4e-4808-80b1-ada4cf812fd1" ClassID="655" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>2</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="630" SV_ID="18">
								<StateVariable Name="SNMP Variable Change" ID="18" HiQnetStateVariableKey="3c5a71bd-e777-479a-b30f-5e8a59f3bc56" ClassID="630" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="19">
								<StateVariable Name="TxA Slot 1 Bit Resolution" ID="19" HiQnetStateVariableKey="68110947-fd5c-41ec-8a4b-e502b0c78b89" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="20">
								<StateVariable Name="TxA Slot 2 Bit Resolution" ID="20" HiQnetStateVariableKey="c131cf4d-8878-4437-8da8-8b9526aea749" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="21">
								<StateVariable Name="TxA Slot 3 Bit Resolution" ID="21" HiQnetStateVariableKey="b836da56-ea1f-4c02-9b92-9523da7b5eac" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="22">
								<StateVariable Name="TxA Slot 4 Bit Resolution" ID="22" HiQnetStateVariableKey="bdbc7901-7e4d-4edc-b88b-67fe2eab065a" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="23">
								<StateVariable Name="TxA Slot 5 Bit Resolution" ID="23" HiQnetStateVariableKey="76ed8d54-32d1-4873-bcf0-763fcfd09ae6" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="24">
								<StateVariable Name="TxA Slot 6 Bit Resolution" ID="24" HiQnetStateVariableKey="01b10d6d-f58b-44ee-83fb-f4a7dbac3360" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="25">
								<StateVariable Name="TxA Slot 7 Bit Resolution" ID="25" HiQnetStateVariableKey="cd6f1eec-f5d6-4d94-9777-1a04e59bf35b" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="26">
								<StateVariable Name="TxA Slot 8 Bit Resolution" ID="26" HiQnetStateVariableKey="562e77b3-ac68-4a93-b2c4-8118b4eb13f0" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="27">
								<StateVariable Name="TxB Slot 1 Bit Resolution" ID="27" HiQnetStateVariableKey="18cfcbed-df6b-4c2f-966c-fdbe7569342a" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="28">
								<StateVariable Name="TxB Slot 2 Bit Resolution" ID="28" HiQnetStateVariableKey="f7adbe2a-1092-4973-a642-b7f658c99723" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="29">
								<StateVariable Name="TxB Slot 3 Bit Resolution" ID="29" HiQnetStateVariableKey="92654ea6-7bdc-4c08-b125-dbc1a1e35961" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="30">
								<StateVariable Name="TxB Slot 4 Bit Resolution" ID="30" HiQnetStateVariableKey="d1e9533b-2eb3-4cac-a49d-937a6217fb52" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="31">
								<StateVariable Name="TxB Slot 5 Bit Resolution" ID="31" HiQnetStateVariableKey="f3948ec3-ab09-4cb0-9c8d-46bce8c2effc" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="32">
								<StateVariable Name="TxB Slot 6 Bit Resolution" ID="32" HiQnetStateVariableKey="0ae98d28-f862-4d7c-9596-02ac2e4475e7" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="33">
								<StateVariable Name="TxB Slot 7 Bit Resolution" ID="33" HiQnetStateVariableKey="e13a9553-6623-450e-aa88-4a5b7cfe5f20" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="34">
								<StateVariable Name="TxB Slot 8 Bit Resolution" ID="34" HiQnetStateVariableKey="bb897f68-8438-421c-8313-85448170cb81" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="35">
								<StateVariable Name="TxC Slot 1 Bit Resolution" ID="35" HiQnetStateVariableKey="8231ba9d-2f83-4443-925e-0a23a46ae3ab" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="36">
								<StateVariable Name="TxC Slot 2 Bit Resolution" ID="36" HiQnetStateVariableKey="94583b43-67b1-47c2-94c9-2d21076dee5a" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="37">
								<StateVariable Name="TxC Slot 3 Bit Resolution" ID="37" HiQnetStateVariableKey="53e67eae-c494-4a73-811e-5c15498ddbb7" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="38">
								<StateVariable Name="TxC Slot 4 Bit Resolution" ID="38" HiQnetStateVariableKey="0ca90918-1493-4f79-8eef-ffbf65d79b19" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="39">
								<StateVariable Name="TxC Slot 5 Bit Resolution" ID="39" HiQnetStateVariableKey="44ca1630-b6f5-4c7d-ac11-db0596fd7f71" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="40">
								<StateVariable Name="TxC Slot 6 Bit Resolution" ID="40" HiQnetStateVariableKey="b25551f0-e07f-4294-9020-64dd90988c4f" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="41">
								<StateVariable Name="TxC Slot 7 Bit Resolution" ID="41" HiQnetStateVariableKey="01b85807-a07a-4742-9d12-2c874444ceb0" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="42">
								<StateVariable Name="TxC Slot 8 Bit Resolution" ID="42" HiQnetStateVariableKey="1c0a9d37-1d1e-4b54-8893-1a2ffbb62455" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="43">
								<StateVariable Name="TxD Slot 1 Bit Resolution" ID="43" HiQnetStateVariableKey="99467050-7b90-4249-9d74-e4f37d0ad08a" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="44">
								<StateVariable Name="TxD Slot 2 Bit Resolution" ID="44" HiQnetStateVariableKey="cfff2222-edf5-446a-95a1-dff85578045d" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="45">
								<StateVariable Name="TxD Slot 3 Bit Resolution" ID="45" HiQnetStateVariableKey="fc54c03b-ae71-487e-9692-e2c4af13e227" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="46">
								<StateVariable Name="TxD Slot 4 Bit Resolution" ID="46" HiQnetStateVariableKey="b1b4c76e-cbd8-4579-b32a-35e706743eb6" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="47">
								<StateVariable Name="TxD Slot 5 Bit Resolution" ID="47" HiQnetStateVariableKey="88ace7bd-6e6b-461e-b188-cf6c4e16df67" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="48">
								<StateVariable Name="TxD Slot 6 Bit Resolution" ID="48" HiQnetStateVariableKey="14f5176c-fe42-4ed2-be65-8dafa10a4146" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="49">
								<StateVariable Name="TxD Slot 7 Bit Resolution" ID="49" HiQnetStateVariableKey="3e814ed7-2a85-4368-ada2-42611209372d" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="626" SV_ID="50">
								<StateVariable Name="TxD Slot 8 Bit Resolution" ID="50" HiQnetStateVariableKey="66519181-4199-40ad-ba35-a72f9400ca50" ClassID="626" Version="1" DefaultValue="2">
									<Min>0</Min>
									<Max>3</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="609" SV_ID="51">
								<StateVariable Name="Mode Rate Control" ID="51" HiQnetStateVariableKey="0e53371a-bc88-4a1b-a7ba-d92ce4b06b72" ClassID="609" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">/////w==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="52">
								<StateVariable Name="TxA Max Packet Size Reached" ID="52" HiQnetStateVariableKey="5dfbc09e-e46f-43d3-9000-6c714da0e65b" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="53">
								<StateVariable Name="TxB Max Packet Size Reached" ID="53" HiQnetStateVariableKey="20a58249-37a2-4293-8899-7884a2eaaf31" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="54">
								<StateVariable Name="TxC Max Packet Size Reached" ID="54" HiQnetStateVariableKey="5e9f9f16-0945-48c5-9b07-a1f122a24753" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="55">
								<StateVariable Name="TxD Max Packet Size Reached" ID="55" HiQnetStateVariableKey="d24e2c46-f093-4469-8127-826bfaf0a1d2" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="4" OBJ_ADDR="1704960">
						<Object Name="Presets" Address="1704960" ClassID="4" Version="1" HiQnetObjectKey="e1b9fd8c-84e3-4735-a25b-bcdd2f0b6868">
							<STATE_VARIABLE SV_CLASSID="747" SV_ID="0">
								<StateVariable Name="Preset Colors" ID="0" HiQnetStateVariableKey="c6034e62-41cb-4e79-bf18-83b4ef82c59e" ClassID="747" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">MgA=</Data3>
									<Data1 Len="50">AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="1">
								<StateVariable Name="Preset Valid" ID="1" HiQnetStateVariableKey="2b92520b-8c4a-4491-aa94-64c05d0b7551" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MQA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="2">
								<StateVariable Name="Current Preset" ID="2" HiQnetStateVariableKey="dc9019ee-93f5-4b26-a001-22866a625e5e" ClassID="616" Version="1" DefaultValue="1">
									<Min>1</Min>
									<Max>50</Max>
									<Value>2</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="635" SV_ID="3">
								<StateVariable Name="Store Preset" ID="3" HiQnetStateVariableKey="e5a6087f-6c19-4fae-bcd1-211c32f1a19e" ClassID="635" Version="1" DefaultValue="2">
									<Data2 Len="1">Ag==</Data2>
									<Data3 Len="1">Mg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="635" SV_ID="4">
								<StateVariable Name="Recall Preset" ID="4" HiQnetStateVariableKey="4643c88f-3fc6-4c88-aaaf-0d9097ca6917" ClassID="635" Version="1" DefaultValue="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">Mg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="5">
								<StateVariable Name="Current Preset Name" ID="5" HiQnetStateVariableKey="00fc9f56-5272-4dd8-a174-7309673aa013" ClassID="517" Version="1" DefaultValue="Default">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20 FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="6">
								<StateVariable Name="Preset 1 Blob" ID="6" HiQnetStateVariableKey="97854479-a1f3-450d-a7df-21fd6015d65e" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="7">
								<StateVariable Name="Preset 1 Name" ID="7" HiQnetStateVariableKey="1d70996a-1cd9-48d6-9f37-4d1c9bc9437c" ClassID="517" Version="1" DefaultValue="Default">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Default</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="8">
								<StateVariable Name="Preset 2 Blob" ID="8" HiQnetStateVariableKey="7f9641c3-9162-4dc9-b7f5-0b342f8b54f0" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4991">[encoded data, 6656 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="9">
								<StateVariable Name="Preset 2 Name" ID="9" HiQnetStateVariableKey="9003b105-a95f-434a-b379-472e57009ce9" ClassID="517" Version="1" DefaultValue="Preset2">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20 FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="10">
								<StateVariable Name="Preset 3 Blob" ID="10" HiQnetStateVariableKey="a3e8d917-f3de-46b5-bfcd-2eb50c67dcb9" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4945">[encoded data, 6596 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="11">
								<StateVariable Name="Preset 3 Name" ID="11" HiQnetStateVariableKey="bdc132cc-8bee-463a-a69e-b11549c89f84" ClassID="517" Version="1" DefaultValue="Preset3">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M22 FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="12">
								<StateVariable Name="Preset 4 Blob" ID="12" HiQnetStateVariableKey="830d42d4-dfa4-4191-a5e0-322f4406896d" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4980">[encoded data, 6640 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="13">
								<StateVariable Name="Preset 4 Name" ID="13" HiQnetStateVariableKey="b587d9fa-067f-40b0-b763-771fd19325f3" ClassID="517" Version="1" DefaultValue="Preset4">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20-M22 FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="14">
								<StateVariable Name="Preset 5 Blob" ID="14" HiQnetStateVariableKey="f7b56fc6-8159-47ae-ba7c-7384618b8be6" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="15">
								<StateVariable Name="Preset 5 Name" ID="15" HiQnetStateVariableKey="e95c9aae-53a8-4cf7-a890-cd435cd9b54e" ClassID="517" Version="1" DefaultValue="Preset5">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset5</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="16">
								<StateVariable Name="Preset 6 Blob" ID="16" HiQnetStateVariableKey="aeb2457a-cddb-4e3d-a331-fa9e3ed29f23" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4951">[encoded data, 6604 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="17">
								<StateVariable Name="Preset 6 Name" ID="17" HiQnetStateVariableKey="04577b1a-5f29-464f-9d6f-7b1f794d6679" ClassID="517" Version="1" DefaultValue="Preset6">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="18">
								<StateVariable Name="Preset 7 Blob" ID="18" HiQnetStateVariableKey="881e8000-e1ff-47c6-abf5-847c2b931762" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4953">[encoded data, 6604 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="19">
								<StateVariable Name="Preset 7 Name" ID="19" HiQnetStateVariableKey="38444ef9-2993-4b7c-9c74-0fa2377ecefa" ClassID="517" Version="1" DefaultValue="Preset7">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M22 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="20">
								<StateVariable Name="Preset 8 Blob" ID="20" HiQnetStateVariableKey="745418b8-47ef-432f-86c8-d9b8228eefc7" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4907">[encoded data, 6544 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="21">
								<StateVariable Name="Preset 8 Name" ID="21" HiQnetStateVariableKey="fd1cab92-a6e7-45f2-a6e2-2d03b2a5d31a" ClassID="517" Version="1" DefaultValue="Preset8">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20-M22 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="22">
								<StateVariable Name="Preset 9 Blob" ID="22" HiQnetStateVariableKey="c74b2be8-bdab-4b0b-9cd3-a75307f1c51b" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="23">
								<StateVariable Name="Preset 9 Name" ID="23" HiQnetStateVariableKey="686167e0-e8e4-41c8-a8b8-726298ec6d64" ClassID="517" Version="1" DefaultValue="Preset9">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset9</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="24">
								<StateVariable Name="Preset 10 Blob" ID="24" HiQnetStateVariableKey="788f7526-506a-443c-a5f2-02c1fcd6c172" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4765">[encoded data, 6356 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="25">
								<StateVariable Name="Preset 10 Name" ID="25" HiQnetStateVariableKey="4df5f18e-bce9-4662-97c3-e6258cdcbe0b" ClassID="517" Version="1" DefaultValue="Preset10">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20 2W FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="26">
								<StateVariable Name="Preset 11 Blob" ID="26" HiQnetStateVariableKey="705f01e9-6b3d-4312-95db-8c3f8f587599" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4771">[encoded data, 6364 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="27">
								<StateVariable Name="Preset 11 Name" ID="27" HiQnetStateVariableKey="e5d46ab0-0de8-4966-876f-abdd82db31d6" ClassID="517" Version="1" DefaultValue="Preset11">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M22 2W FR</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="28">
								<StateVariable Name="Preset 12 Blob" ID="28" HiQnetStateVariableKey="c0d670cb-0b7a-479c-90b3-6bc1e79b31d6" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="29">
								<StateVariable Name="Preset 12 Name" ID="29" HiQnetStateVariableKey="bbdfa0a3-83bb-475d-b181-95c2612cc545" ClassID="517" Version="1" DefaultValue="Preset12">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset12</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="30">
								<StateVariable Name="Preset 13 Blob" ID="30" HiQnetStateVariableKey="cf542eb5-39db-4815-88dd-ff0e180d0041" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4745">[encoded data, 6328 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="31">
								<StateVariable Name="Preset 13 Name" ID="31" HiQnetStateVariableKey="ffce7a22-f828-4679-bf67-bbf73c55609e" ClassID="517" Version="1" DefaultValue="Preset13">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M20 2W 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="32">
								<StateVariable Name="Preset 14 Blob" ID="32" HiQnetStateVariableKey="eb3d7031-390f-4ac8-911f-13656d2362df" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="4775">[encoded data, 6368 characters]</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="33">
								<StateVariable Name="Preset 14 Name" ID="33" HiQnetStateVariableKey="8fe8984e-096f-4df8-b41a-e58c8f3411c4" ClassID="517" Version="1" DefaultValue="Preset14">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX M22 2W 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="34">
								<StateVariable Name="Preset 15 Blob" ID="34" HiQnetStateVariableKey="dc5537ff-e271-43a6-b2f2-57f4869af643" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="35">
								<StateVariable Name="Preset 15 Name" ID="35" HiQnetStateVariableKey="47b71eb6-5684-474c-a7a9-1891be964cbb" ClassID="517" Version="1" DefaultValue="Preset15">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset15</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="36">
								<StateVariable Name="Preset 16 Blob" ID="36" HiQnetStateVariableKey="f89b75ce-51ff-4fb1-ae9e-76a65d1a8435" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="1421">AEwAAQgAAAMGAAAAAAABCAAACQYAAAAAAAEIAAAMAQAAAQgAACMBeAABCAAAJQY8I9cKAAIJAAAfAXgAAgkAACEGPHXCjwAFDAEADwHIAAUMAgABAQAABQwCAAMBAAAFDAIABAEAAAUMAgAPAcgACSMBAAABAQAJIwEABgEBAAkjAQAMAQEACSMBABIBAQAJIwEAGAEBAAkjAQAeAQEACSMBACQBAQAJIwEAKgEBAAkjAQAwAQEACSMBADYBAQAJIwEAPAEBAAkjAQBCAQEACSMBAEgBAQAJIwEATgEBAAkjAQBUAQEACSMBAFoBAQAJIwIAAAEBAAkjAgAGAQEACSMCAAwBAQAJIwIAEgEBAAkjAgAYAQEACSMCAB4BAQAJIwIAJAEBAAkjAgAqAQEACSMCADABAQAJIwIANgEBAAkjAgA8AQEACSMCAEIBAQAJIwIASAEBAAkjAgBOAQEACSMCAFQBAQAJIwIAWgEBAAokAQAAAQEACiQBAAEGQcgAAAAKJAEABQEBAAokAQAGBkKgAAAACiQCAAABAQAKJAIAAQZByAAAAAokAgAFAQEACiQCAAYGQqAAAAAMIgEAAAEBAAwiAQABBkI4AAAADCIBAAIGQAXCjwAMIgEABAbABmZmAAwiAQAGAQEADCIBAAcGQq4AAAAMIgEACAZARHrhAAwiAQAKBj+ZmZoADCIBAAwBAQAMIgEADQZCBAAAAAwiAQAOBkCseuEADCIBABAGP0zMzQAMIgEAEgEBAAwiAQATBkJaeuEADCIBABQGPgUeuAAMIgEAFgZA4AAAAAwiAQAYAQEADCIBABkGRDTAAAAMIgEAGgY+YUeuAAwiAQAcBsAzMzMADCICAAABAQAMIgIAAQZCOAAAAAwiAgACBkAFwo8ADCICAAQGwAZmZgAMIgIABgEBAAwiAgAHBkKuAAAADCICAAgGQER64QAMIgIACgY/mZmaAAwiAgAMAQEADCICAA0GQgQAAAAMIgIADgZArHrhAAwiAgAQBj9MzM0ADCICABIBAQAMIgIAEwZCWnrhAAwiAgAUBj4FHrgADCICABYGQOAAAAAMIgIAGAEBAAwiAgAZBkQ0wAAADCICABoGPmFHrgAMIgIAHAbAMzMzAA0UAQABBjqdSVIADRQCAAEGOp1JUgAPEAEAAAEBAA8QAQABAQIADxACAAABAQAPEAIAAQECABARAQAAAQEAEBEBAAEGQ1uAAAAQEQEAAwY+dcKPABARAQAFAQEAEBEBAAYGQlwAAAAQEQEACQZAoAAAABARAgAAAQEAEBECAAEGQ1t6mQAQEQIAAwY+dcKPABARAgAFAQEAEBECAAYGQlwAAAAQEQIACQZAoAAAABESAQAAAQEAERIBAAEGPLctvQAREgEAAgZC3AAAABESAQADBj64UewAERIBAAQGPziTdQAREgIAAAEBABESAgABBjy3Lb8AERICAAIGQtwAAAAREgIAAwY+uFHsABESAgAEBj84k3gAEhMBAAABAQASEwEAAQZA4AAAABITAQACBkKpzM0AEhMBAAMGP2uFHwASEwEABAY+BR64ABITAgAAAQEAEhMCAAEGQOAAAAASEwIAAgZCqczNABITAgADBj9sLCwAEhMCAAQGPgb0qgATFQEAAAHIABMVAQAPBkGQAAAAExUBABABAQATFQEAEQEBABMVAgAAAcgAExUCAA8GQZAAAAATFQIAEAEBABMVAgARAQEAFRkBAAABAQAVGQIAAAEBABcLAAABAQEAGgAAABUBAQAaAAAAFgkAEgBhAHUANgBiAGEAdABkAHgAAAAaAAAAGQEBABoBAAAACQAQAEYAMQA4AFMAIAA4ADAAAAAaAQAAAQkAEABGADEAOABTACAAOAAwAAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="37">
								<StateVariable Name="Preset 16 Name" ID="37" HiQnetStateVariableKey="5bf54a1f-afde-4398-ba88-a64b07d3b338" ClassID="517" Version="1" DefaultValue="Preset16">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX F18S 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="38">
								<StateVariable Name="Preset 17 Blob" ID="38" HiQnetStateVariableKey="98d91c6e-9206-4ecf-b0b1-1d164fedfb83" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="1463">AEwAAQgAAAMGAAAAAAABCAAACQYAAAAAAAEIAAAMAQAAAQgAACMBeAABCAAAJQY8I9cKAAIJAAAfAXgAAgkAACEGPHXCjwAFDAEADwHIAAUMAgAPAcgACSMBAAABAQAJIwEABgEBAAkjAQAMAQEACSMBABIBAQAJIwEAGAEBAAkjAQAeAQEACSMBACQBAQAJIwEAKgEBAAkjAQAwAQEACSMBADYBAQAJIwEAPAEBAAkjAQBCAQEACSMBAEgBAQAJIwEATgEBAAkjAQBUAQEACSMBAFoBAQAJIwIAAAEBAAkjAgAGAQEACSMCAAwBAQAJIwIAEgEBAAkjAgAYAQEACSMCAB4BAQAJIwIAJAEBAAkjAgAqAQEACSMCADABAQAJIwIANgEBAAkjAgA8AQEACSMCAEIBAQAJIwIASAEBAAkjAgBOAQEACSMCAFQBAQAJIwIAWgEBAAokAQAAAQEACiQBAAEGQfAAAAAKJAEABQEBAAokAQAGBkKgAAAACiQCAAABAQAKJAIAAQZB8AAAAAokAgAFAQEACiQCAAYGQqAAAAALJQEACAECAAslAgAIAQIADCIBAAABAQAMIgEAAQZCDgAAAAwiAQACBkBAAAAADCIBAAQGQSAAAAAMIgEABgEBAAwiAQAHBkIgAAAADCIBAAgGPiPXCgAMIgEACgZAwAAAAAwiAQAMAQEADCIBAA0GQvwAAAAMIgEAEAa/gAAAAAwiAQASAQEADCIBABMGQnAAAAAMIgEAFAZAYAAAAAwiAQAWBkAgAAAADCIBABgBAQAMIgEAGQZDggAAAAwiAQAaBkEgAAAADCIBABwGwcAAAAAMIgIAAAEBAAwiAgABBkIOAAAADCICAAIGQEAAAAAMIgIABAZBIAAAAAwiAgAGAQEADCICAAcGQiAAAAAMIgIACAY+I9cKAAwiAgAKBkDAAAAADCICAAwBAQAMIgIADQZC/AAAAAwiAgAQBr+AAAAADCICABIBAQAMIgIAEwZCcAAAAAwiAgAUBkBgAAAADCICABYGQCAAAAAMIgIAGAEBAAwiAgAZBkOCAAAADCICABoGQSAAAAAMIgIAHAbBwAAAAA8QAQAAAQEADxABAAEBAgAPEAIAAAEBAA8QAgABAQIAEBEBAAABAQAQEQEAAQZDMYAAABARAQADBj5bbbYAEBEBAAUBAQAQEQEABgZCBAAAABARAQAIBkFAAAAAEBEBAAkGQSAAAAAQEQEACgEDABARAQALAQEAEBEBAAwGQloAAAAQEQEADQZBAAAAABARAQAPBkDAAAAAEBECAAABAQAQEQIAAQZDMYAAABARAgADBj5bbbYAEBECAAUBAQAQEQIABgZCBAAAABARAgAIBkFAAAAAEBECAAkGQSAAAAAQEQIACgEDABARAgALAQEAEBECAAwGQloAAAAQEQIADQZBAAAAABARAgAPBkDAAAAAERIBAAABAQAREgEAAQY8x91EABESAQACBkKqAAAAERIBAAMGPqSSSgAREgEABAY/JbyLABESAgAAAQEAERICAAEGPMfdRAAREgIAAgZCqgAAABESAgADBj6kkkoAERICAAQGPyW8iwASEwEAAAEBABITAQABBkEAAAAAEhMBAAIGQo4zMwASEwEABAY9zMzNABITAgAAAQEAEhMCAAEGQQAAAAASEwIAAgZCjjMzABITAgAEBj3MzM0AExUBAAAByAATFQEADwZBEAAAABMVAQAQAQEAExUBABEBAQATFQIAAAHIABMVAgAPBkEQAAAAExUCABABAQATFQIAEQEBABUZAQAAAQEAFRkCAAABAQAXCwAAAQEBABoAAAAVAQEAGgAAABYJABIAYQB1ADYAYgBhAHQAZAB4AAAAGgAAABkBAQAaAQAAAAkADgBTADIANQAgADgAMAAAABoBAAABCQAOAFMAMgA1ACAAOAAwAAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="39">
								<StateVariable Name="Preset 17 Name" ID="39" HiQnetStateVariableKey="b0cf7c3c-9f0b-44bc-ae1a-7f948e552c6e" ClassID="517" Version="1" DefaultValue="Preset17">
									<Min>0</Min>
									<Max>64</Max>
									<Value>VTX S25 80</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="40">
								<StateVariable Name="Preset 18 Blob" ID="40" HiQnetStateVariableKey="103adf6e-0e29-41f1-9d35-66a52e997eda" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="41">
								<StateVariable Name="Preset 18 Name" ID="41" HiQnetStateVariableKey="996a8a6c-8048-40dd-89bd-491bfc357602" ClassID="517" Version="1" DefaultValue="Preset18">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset18</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="42">
								<StateVariable Name="Preset 19 Blob" ID="42" HiQnetStateVariableKey="3b57e71d-1a82-4dad-b187-7af4834119ca" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="43">
								<StateVariable Name="Preset 19 Name" ID="43" HiQnetStateVariableKey="c1f55803-78a0-4db9-8692-fcae9928d5b5" ClassID="517" Version="1" DefaultValue="Preset19">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset19</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="44">
								<StateVariable Name="Preset 20 Blob" ID="44" HiQnetStateVariableKey="51715f7a-c622-4a82-8352-880a3bdea306" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="45">
								<StateVariable Name="Preset 20 Name" ID="45" HiQnetStateVariableKey="bddafc58-6265-40a6-8649-7d4c1329b786" ClassID="517" Version="1" DefaultValue="Preset20">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset20</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="46">
								<StateVariable Name="Preset 21 Blob" ID="46" HiQnetStateVariableKey="356393e0-62dd-43ef-8143-65a2b5803ca2" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="47">
								<StateVariable Name="Preset 21 Name" ID="47" HiQnetStateVariableKey="30684488-0888-424e-a814-90e5d717ca63" ClassID="517" Version="1" DefaultValue="Preset21">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset21</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="48">
								<StateVariable Name="Preset 22 Blob" ID="48" HiQnetStateVariableKey="4abe6c38-5dd3-413f-b0dc-f3e39eb57b9b" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="49">
								<StateVariable Name="Preset 22 Name" ID="49" HiQnetStateVariableKey="d063d7d1-e362-4ff3-9916-6e033ee90799" ClassID="517" Version="1" DefaultValue="Preset22">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset22</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="50">
								<StateVariable Name="Preset 23 Blob" ID="50" HiQnetStateVariableKey="26f919f2-74fe-4106-a590-6197ca230684" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="51">
								<StateVariable Name="Preset 23 Name" ID="51" HiQnetStateVariableKey="58aad308-3a80-48ee-a4aa-ae178ff7d924" ClassID="517" Version="1" DefaultValue="Preset23">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset23</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="52">
								<StateVariable Name="Preset 24 Blob" ID="52" HiQnetStateVariableKey="6c90c42b-110c-4f59-b80f-69f667c610f7" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="53">
								<StateVariable Name="Preset 24 Name" ID="53" HiQnetStateVariableKey="83d93642-1de2-43b1-9082-a742f9785bf1" ClassID="517" Version="1" DefaultValue="Preset24">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset24</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="54">
								<StateVariable Name="Preset 25 Blob" ID="54" HiQnetStateVariableKey="6ef111b0-17d2-4ae5-b630-bc70a83e78f8" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="55">
								<StateVariable Name="Preset 25 Name" ID="55" HiQnetStateVariableKey="540e1c3d-e0b5-4f6b-bd8a-e7e9647bdffd" ClassID="517" Version="1" DefaultValue="Preset25">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset25</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="56">
								<StateVariable Name="Preset 26 Blob" ID="56" HiQnetStateVariableKey="c6d934d4-6564-42dd-be2a-e3c4a2a4dc50" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="57">
								<StateVariable Name="Preset 26 Name" ID="57" HiQnetStateVariableKey="4c5dc245-3c8e-436b-ae90-6d9e7f79e4d8" ClassID="517" Version="1" DefaultValue="Preset26">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset26</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="58">
								<StateVariable Name="Preset 27 Blob" ID="58" HiQnetStateVariableKey="46ea5939-e733-41e7-936e-89ad24ad8524" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="59">
								<StateVariable Name="Preset 27 Name" ID="59" HiQnetStateVariableKey="525f2ea9-eefb-4099-8e00-71bb470e6caf" ClassID="517" Version="1" DefaultValue="Preset27">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset27</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="60">
								<StateVariable Name="Preset 28 Blob" ID="60" HiQnetStateVariableKey="01a349ae-b8cf-4af8-95db-5eee995f7e66" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="61">
								<StateVariable Name="Preset 28 Name" ID="61" HiQnetStateVariableKey="3e3a0bae-6ff6-46ff-87bb-1a9e24a43ccc" ClassID="517" Version="1" DefaultValue="Preset28">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset28</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="62">
								<StateVariable Name="Preset 29 Blob" ID="62" HiQnetStateVariableKey="6e301491-6bc1-4364-a6af-46ebf987f244" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="63">
								<StateVariable Name="Preset 29 Name" ID="63" HiQnetStateVariableKey="490cf6b9-3e4b-4d57-ab6a-fca448149e17" ClassID="517" Version="1" DefaultValue="Preset29">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset29</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="64">
								<StateVariable Name="Preset 30 Blob" ID="64" HiQnetStateVariableKey="014c8bbe-c450-43df-90c9-26d9498aa906" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="65">
								<StateVariable Name="Preset 30 Name" ID="65" HiQnetStateVariableKey="8d9f4fcb-b486-42e3-afc4-2efb8d0e10b5" ClassID="517" Version="1" DefaultValue="Preset30">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset30</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="66">
								<StateVariable Name="Preset 31 Blob" ID="66" HiQnetStateVariableKey="c6f2ff1f-e75c-4197-8fd8-78dbc440ea95" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="67">
								<StateVariable Name="Preset 31 Name" ID="67" HiQnetStateVariableKey="59f8ff3a-6190-4c8c-b0f4-5e2b9f17d72c" ClassID="517" Version="1" DefaultValue="Preset31">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset31</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="68">
								<StateVariable Name="Preset 32 Blob" ID="68" HiQnetStateVariableKey="226976cb-7dc6-4d61-bfcb-dcc0e203dcf2" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="69">
								<StateVariable Name="Preset 32 Name" ID="69" HiQnetStateVariableKey="7186b461-48ea-44a1-97ea-93b06f6d0573" ClassID="517" Version="1" DefaultValue="Preset32">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset32</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="70">
								<StateVariable Name="Preset 33 Blob" ID="70" HiQnetStateVariableKey="84a0f6e6-2cbf-4021-9dea-af578df5dccc" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="71">
								<StateVariable Name="Preset 33 Name" ID="71" HiQnetStateVariableKey="452edfeb-d04e-48d1-94a6-8e047ebe0490" ClassID="517" Version="1" DefaultValue="Preset33">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset33</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="72">
								<StateVariable Name="Preset 34 Blob" ID="72" HiQnetStateVariableKey="a671eb62-bcfa-4086-8f6b-e59d310dbe3e" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="73">
								<StateVariable Name="Preset 34 Name" ID="73" HiQnetStateVariableKey="4ddee852-e7fe-494c-95de-14cd27cd5142" ClassID="517" Version="1" DefaultValue="Preset34">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset34</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="74">
								<StateVariable Name="Preset 35 Blob" ID="74" HiQnetStateVariableKey="663c28c5-aa92-484a-8dda-d20d06cd68ee" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="75">
								<StateVariable Name="Preset 35 Name" ID="75" HiQnetStateVariableKey="21f6d16d-d507-47b0-8304-7f05490877be" ClassID="517" Version="1" DefaultValue="Preset35">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset35</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="76">
								<StateVariable Name="Preset 36 Blob" ID="76" HiQnetStateVariableKey="b7062277-ff88-4b1a-ae3b-e6ea11fe7e5b" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="77">
								<StateVariable Name="Preset 36 Name" ID="77" HiQnetStateVariableKey="3d3c9e9f-d729-4b97-84c2-50978649745f" ClassID="517" Version="1" DefaultValue="Preset36">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset36</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="78">
								<StateVariable Name="Preset 37 Blob" ID="78" HiQnetStateVariableKey="04f406f8-32da-4009-a116-16d6c4307c15" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="79">
								<StateVariable Name="Preset 37 Name" ID="79" HiQnetStateVariableKey="63c8b7bc-1d5f-406b-b920-b60dfc91ffe6" ClassID="517" Version="1" DefaultValue="Preset37">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset37</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="80">
								<StateVariable Name="Preset 38 Blob" ID="80" HiQnetStateVariableKey="3bd79b6e-a993-4b56-a6db-c1898e300300" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="81">
								<StateVariable Name="Preset 38 Name" ID="81" HiQnetStateVariableKey="e5715c01-e78d-4844-8b90-08e041ef4532" ClassID="517" Version="1" DefaultValue="Preset38">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset38</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="82">
								<StateVariable Name="Preset 39 Blob" ID="82" HiQnetStateVariableKey="7ccbc47f-9101-4c4f-9d09-45d133aa359c" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="83">
								<StateVariable Name="Preset 39 Name" ID="83" HiQnetStateVariableKey="56f8b6a5-8436-49cf-9da3-6d2078cb370c" ClassID="517" Version="1" DefaultValue="Preset39">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset39</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="84">
								<StateVariable Name="Preset 40 Blob" ID="84" HiQnetStateVariableKey="98534e0f-4b2e-40b9-a180-38d237edf352" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="85">
								<StateVariable Name="Preset 40 Name" ID="85" HiQnetStateVariableKey="8255ba5b-6cf0-4f01-a81b-983081eba46f" ClassID="517" Version="1" DefaultValue="Preset40">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset40</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="86">
								<StateVariable Name="Preset 41 Blob" ID="86" HiQnetStateVariableKey="6a87aff2-2833-4746-a87b-80c6be30325d" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="87">
								<StateVariable Name="Preset 41 Name" ID="87" HiQnetStateVariableKey="0c67795d-48a8-48bb-9ec0-f15a521692e1" ClassID="517" Version="1" DefaultValue="Preset41">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset41</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="88">
								<StateVariable Name="Preset 42 Blob" ID="88" HiQnetStateVariableKey="c1bf5519-1c5a-4b05-a501-99022a8a0e18" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="89">
								<StateVariable Name="Preset 42 Name" ID="89" HiQnetStateVariableKey="af12b545-15fa-4d5c-a76b-1966c62d4b7e" ClassID="517" Version="1" DefaultValue="Preset42">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset42</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="90">
								<StateVariable Name="Preset 43 Blob" ID="90" HiQnetStateVariableKey="1e8eab4b-2561-435e-bbb2-e8924b6723ab" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="91">
								<StateVariable Name="Preset 43 Name" ID="91" HiQnetStateVariableKey="8d80185f-f2a0-4e3f-b18a-e027ef76f98e" ClassID="517" Version="1" DefaultValue="Preset43">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset43</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="92">
								<StateVariable Name="Preset 44 Blob" ID="92" HiQnetStateVariableKey="d524fb67-4434-4629-828f-854184958b2a" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="93">
								<StateVariable Name="Preset 44 Name" ID="93" HiQnetStateVariableKey="428789d6-fb7e-4cf0-9673-b0f06e051598" ClassID="517" Version="1" DefaultValue="Preset44">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset44</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="94">
								<StateVariable Name="Preset 45 Blob" ID="94" HiQnetStateVariableKey="d6c0514e-46af-4db8-af40-809110298999" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="95">
								<StateVariable Name="Preset 45 Name" ID="95" HiQnetStateVariableKey="7307204d-364c-4fc4-a579-8558f44cda1d" ClassID="517" Version="1" DefaultValue="Preset45">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset45</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="96">
								<StateVariable Name="Preset 46 Blob" ID="96" HiQnetStateVariableKey="cb8dfc9a-0488-4808-a2ea-31ed13bc2985" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="97">
								<StateVariable Name="Preset 46 Name" ID="97" HiQnetStateVariableKey="991a6a33-526c-44d6-9651-0a93049251c9" ClassID="517" Version="1" DefaultValue="Preset46">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset46</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="98">
								<StateVariable Name="Preset 47 Blob" ID="98" HiQnetStateVariableKey="35cde38a-060c-435d-a51d-b154e38a53e4" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="99">
								<StateVariable Name="Preset 47 Name" ID="99" HiQnetStateVariableKey="70ab8453-b745-409a-8c8d-67dd2e8abd70" ClassID="517" Version="1" DefaultValue="Preset47">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset47</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="100">
								<StateVariable Name="Preset 48 Blob" ID="100" HiQnetStateVariableKey="77de4ff8-4ead-4800-9194-126628ef8061" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="101">
								<StateVariable Name="Preset 48 Name" ID="101" HiQnetStateVariableKey="81426611-a005-4184-a104-e049c61376e6" ClassID="517" Version="1" DefaultValue="Preset48">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset48</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="102">
								<StateVariable Name="Preset 49 Blob" ID="102" HiQnetStateVariableKey="764d5d34-f8fa-49be-adf0-9750fd475fc1" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="103">
								<StateVariable Name="Preset 49 Name" ID="103" HiQnetStateVariableKey="de84149a-df74-4dcf-acd2-11883a3aa615" ClassID="517" Version="1" DefaultValue="Preset49">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset49</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="104">
								<StateVariable Name="Preset 50 Blob" ID="104" HiQnetStateVariableKey="d40af186-84ba-4cff-8837-5509c377379f" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="105">
								<StateVariable Name="Preset 50 Name" ID="105" HiQnetStateVariableKey="92dd7ab2-18c3-41dc-ba6e-2ed489a94a86" ClassID="517" Version="1" DefaultValue="Preset50">
									<Min>0</Min>
									<Max>64</Max>
									<Value>Preset50</Value>
									<Flags>0</Flags>
									<Flags2>0</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="106">
								<StateVariable Name="Max Preset Number" ID="106" HiQnetStateVariableKey="05f5f1be-8ee4-4b94-8ef0-bd99103a9adb" ClassID="616" Version="1" DefaultValue="50">
									<Min>1</Min>
									<Max>50</Max>
									<Value>50</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="107">
								<StateVariable Name="Min Preset Number" ID="107" HiQnetStateVariableKey="343f50c7-0bbe-4d3a-864b-12b75af3bc69" ClassID="616" Version="1" DefaultValue="1">
									<Min>1</Min>
									<Max>50</Max>
									<Value>1</Value>
									<Flags>0</Flags>
									<Flags2>5</Flags2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="5" OBJ_ADDR="1705216">
						<Object Name="Scenes" Address="1705216" ClassID="5" Version="1" HiQnetObjectKey="73634fb1-5e6c-435c-ad6b-a4fb24835155">
							<STATE_VARIABLE SV_CLASSID="635" SV_ID="0">
								<StateVariable Name="Store Scene" ID="0" HiQnetStateVariableKey="8146bd59-5990-48d3-9ab6-9bbe93e5acfc" ClassID="635" Version="1" DefaultValue="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">FA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="635" SV_ID="1">
								<StateVariable Name="Recall Scene" ID="1" HiQnetStateVariableKey="1e1c820a-57fe-40ce-8c1e-1bb7f731a035" ClassID="635" Version="1" DefaultValue="1">
									<Data2 Len="1">AQ==</Data2>
									<Data3 Len="1">FA==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="2">
								<StateVariable Name="Scene 1 Blob" ID="2" HiQnetStateVariableKey="72c96db2-fbe8-40ec-9f6d-1ae829f94577" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="3">
								<StateVariable Name="Scene 1 Name" ID="3" HiQnetStateVariableKey="2763c40a-33b5-4b87-820d-373eb697296f" ClassID="517" Version="1" DefaultValue="Scene1">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADEA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="4">
								<StateVariable Name="Scene 2 Blob" ID="4" HiQnetStateVariableKey="28faa629-d5eb-49c4-bba8-81de6c740d25" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="5">
								<StateVariable Name="Scene 2 Name" ID="5" HiQnetStateVariableKey="013f7f8c-d421-40ab-83c4-681407b5cee7" ClassID="517" Version="1" DefaultValue="Scene2">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADIA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="6">
								<StateVariable Name="Scene 3 Blob" ID="6" HiQnetStateVariableKey="c920037b-e984-4d06-bcaa-8909631d17dd" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="7">
								<StateVariable Name="Scene 3 Name" ID="7" HiQnetStateVariableKey="07ef2669-9287-4398-a36d-a20d7f8ea476" ClassID="517" Version="1" DefaultValue="Scene3">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADMA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="8">
								<StateVariable Name="Scene 4 Blob" ID="8" HiQnetStateVariableKey="799dcd3b-606d-46c4-8074-5dd09dc94fd6" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="9">
								<StateVariable Name="Scene 4 Name" ID="9" HiQnetStateVariableKey="30a755eb-3871-4e19-b6a4-7ce8770f1699" ClassID="517" Version="1" DefaultValue="Scene4">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADQA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="10">
								<StateVariable Name="Scene 5 Blob" ID="10" HiQnetStateVariableKey="97fc7c93-79c0-4682-8529-984a9deee174" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="11">
								<StateVariable Name="Scene 5 Name" ID="11" HiQnetStateVariableKey="bf814fe6-ab68-46f8-9618-b9c02c31118e" ClassID="517" Version="1" DefaultValue="Scene5">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADUA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="12">
								<StateVariable Name="Scene 6 Blob" ID="12" HiQnetStateVariableKey="d52d4603-0f20-42a7-8ed2-b9f60a9f30af" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="13">
								<StateVariable Name="Scene 6 Name" ID="13" HiQnetStateVariableKey="ae3fd5e5-d3d5-4428-904e-142727e2ed0b" ClassID="517" Version="1" DefaultValue="Scene6">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADYA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="14">
								<StateVariable Name="Scene 7 Blob" ID="14" HiQnetStateVariableKey="d8310d28-b577-4411-a8e5-1a4a5aad388b" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="15">
								<StateVariable Name="Scene 7 Name" ID="15" HiQnetStateVariableKey="86ad1a3f-207e-458c-af91-624bf9cd83cf" ClassID="517" Version="1" DefaultValue="Scene7">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADcA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="16">
								<StateVariable Name="Scene 8 Blob" ID="16" HiQnetStateVariableKey="162e8741-ca49-4c95-bc05-e004f770cecb" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="17">
								<StateVariable Name="Scene 8 Name" ID="17" HiQnetStateVariableKey="35ff1984-05d2-4460-a615-b9859f57f19c" ClassID="517" Version="1" DefaultValue="Scene8">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADgA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="18">
								<StateVariable Name="Scene 9 Blob" ID="18" HiQnetStateVariableKey="094fec77-9b5a-4bfc-b26c-5c827f646aea" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="19">
								<StateVariable Name="Scene 9 Name" ID="19" HiQnetStateVariableKey="86c7a0e2-329a-410e-ab2d-b39cfbff6ab6" ClassID="517" Version="1" DefaultValue="Scene9">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="12">UwBjAGUAbgBlADkA</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="20">
								<StateVariable Name="Scene 10 Blob" ID="20" HiQnetStateVariableKey="14928f0c-9f3d-44c6-96a6-c7f45d416a30" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="21">
								<StateVariable Name="Scene 10 Name" ID="21" HiQnetStateVariableKey="18743f33-41ad-4a52-ad3b-4efaf47b6ed3" ClassID="517" Version="1" DefaultValue="Scene10">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEAMAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="22">
								<StateVariable Name="Scene 11 Blob" ID="22" HiQnetStateVariableKey="8b4635e0-7ab4-4c0d-9cd3-9c20c74057ea" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="23">
								<StateVariable Name="Scene 11 Name" ID="23" HiQnetStateVariableKey="d35f5a7b-0109-49ba-b6fb-67165735a710" ClassID="517" Version="1" DefaultValue="Scene11">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEAMQA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="24">
								<StateVariable Name="Scene 12 Blob" ID="24" HiQnetStateVariableKey="1c3276d0-f63b-4af8-a828-5bb9d4dbae6d" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="25">
								<StateVariable Name="Scene 12 Name" ID="25" HiQnetStateVariableKey="fe743ff2-3833-4e36-8828-6470709c0524" ClassID="517" Version="1" DefaultValue="Scene12">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEAMgA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="26">
								<StateVariable Name="Scene 13 Blob" ID="26" HiQnetStateVariableKey="8b3cbef8-2bcb-4765-b309-c9c79a4de4ce" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="27">
								<StateVariable Name="Scene 13 Name" ID="27" HiQnetStateVariableKey="386cae84-1691-4b61-b37c-b92fed0b25b0" ClassID="517" Version="1" DefaultValue="Scene13">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEAMwA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="28">
								<StateVariable Name="Scene 14 Blob" ID="28" HiQnetStateVariableKey="ea59621c-fb09-458c-9e98-46204bf4257e" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="29">
								<StateVariable Name="Scene 14 Name" ID="29" HiQnetStateVariableKey="081640c5-3bf0-4f2e-8468-2553784c0563" ClassID="517" Version="1" DefaultValue="Scene14">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEANAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="30">
								<StateVariable Name="Scene 15 Blob" ID="30" HiQnetStateVariableKey="73439563-90a1-4265-8fdf-a97682347ab7" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="31">
								<StateVariable Name="Scene 15 Name" ID="31" HiQnetStateVariableKey="0099d144-f761-47b3-b276-b8f5e027115d" ClassID="517" Version="1" DefaultValue="Scene15">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEANQA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="32">
								<StateVariable Name="Scene 16 Blob" ID="32" HiQnetStateVariableKey="711ab057-c4da-4fdc-8a8f-6118bacc77fd" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="33">
								<StateVariable Name="Scene 16 Name" ID="33" HiQnetStateVariableKey="6e6d8b39-a685-47b3-8ade-e2134765a6f1" ClassID="517" Version="1" DefaultValue="Scene16">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEANgA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="34">
								<StateVariable Name="Scene 17 Blob" ID="34" HiQnetStateVariableKey="fb7ec693-e2bb-462d-a4fe-bb5c1ea25394" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="35">
								<StateVariable Name="Scene 17 Name" ID="35" HiQnetStateVariableKey="92356971-120c-4cca-860c-0a4461003213" ClassID="517" Version="1" DefaultValue="Scene17">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEANwA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="36">
								<StateVariable Name="Scene 18 Blob" ID="36" HiQnetStateVariableKey="575c629f-3c53-42d5-94e5-910e4351576d" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="37">
								<StateVariable Name="Scene 18 Name" ID="37" HiQnetStateVariableKey="810b9476-0cb3-4a87-af33-98155a2290bb" ClassID="517" Version="1" DefaultValue="Scene18">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEAOAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="38">
								<StateVariable Name="Scene 19 Blob" ID="38" HiQnetStateVariableKey="12127132-f471-4b53-939f-deeacdf12b0e" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="39">
								<StateVariable Name="Scene 19 Name" ID="39" HiQnetStateVariableKey="74a5544e-ac26-4d6b-a919-3bf3ba35da84" ClassID="517" Version="1" DefaultValue="Scene19">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADEAOQA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="518" SV_ID="40">
								<StateVariable Name="Scene 20 Blob" ID="40" HiQnetStateVariableKey="b1e67500-05f5-4381-b589-78e430e97df1" ClassID="518" Version="1" DefaultValue="">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">//8=</Data3>
									<Data1 Len="0"></Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="517" SV_ID="41">
								<StateVariable Name="Scene 20 Name" ID="41" HiQnetStateVariableKey="1b6fb6eb-3cc6-453a-bdee-58ce8ef848f6" ClassID="517" Version="1" DefaultValue="Scene20">
									<Data2 Len="2">AAA=</Data2>
									<Data3 Len="2">QAA=</Data3>
									<Data1 Len="14">UwBjAGUAbgBlADIAMAA=</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="23" OBJ_ADDR="1709824">
						<Object Name="Power Supply" Address="1709824" ClassID="23" Version="1" HiQnetObjectKey="dfa92b3e-dd3f-4142-a6fa-25867f890ad3">
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="0">
								<StateVariable Name="Line Voltage" ID="0" HiQnetStateVariableKey="cde7923a-cab3-48e3-9c20-71855e14f488" ClassID="535" Version="1" DefaultValue="120">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AICPQw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="1">
								<StateVariable Name="Proportional Vcc" ID="1" HiQnetStateVariableKey="787df361-c1d6-4f5c-8316-667735555dfb" ClassID="535" Version="1" DefaultValue="5.1">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">w/XAQA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="2">
								<StateVariable Name="Temperature" ID="2" HiQnetStateVariableKey="076cb6c6-61c3-480a-88b0-9d149119cb5e" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="3">
								<StateVariable Name="Vcc" ID="3" HiQnetStateVariableKey="62a346a8-c70a-471d-a02d-d662e715b1b2" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACWQw==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="4">
								<StateVariable Name="Temperature Deg C" ID="4" HiQnetStateVariableKey="599e0f1c-ad58-4256-bcfe-0055f98a27d0" ClassID="535" Version="1" DefaultValue="20">
									<Data2 Len="4">AACgQQ==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MgA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="24" OBJ_ADDR="1710080">
						<Object Name="Fan Control" Address="1710080" ClassID="24" Version="1" HiQnetObjectKey="84830b5a-fa38-4f19-a35c-0ff3b30cbf27">
							<STATE_VARIABLE SV_CLASSID="741" SV_ID="0">
								<StateVariable Name="Mode" ID="0" HiQnetStateVariableKey="dba1397b-c64b-48f1-9a71-c8227f5a8e56" ClassID="741" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">Ag==</Data3>
									<Data1 Len="1">AA==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Aggressiveness" ID="1" HiQnetStateVariableKey="bb26e564-3836-45ee-947a-8bd2d5ac158f" ClassID="733" Version="1" DefaultValue="10">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AABwQQ==</Data3>
									<Data1 Len="4">AAAgQQ==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="2">
								<StateVariable Name="Amp Fan Setpoint" ID="2" HiQnetStateVariableKey="764bc2f6-8c40-4e34-a395-69d7a09309c6" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="3">
								<StateVariable Name="Amp Fan Process Variable" ID="3" HiQnetStateVariableKey="8c7c418b-3ed1-4385-8830-f0cc65d7af71" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="4">
								<StateVariable Name="Power Supply Fan Setpoint" ID="4" HiQnetStateVariableKey="4a487815-4a8a-43bb-82a0-fb4fcbbdbe81" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="5">
								<StateVariable Name="Power Supply Fan Process Variable" ID="5" HiQnetStateVariableKey="f3b46190-23f2-4aa1-bec0-167acfefc829" ClassID="535" Version="1" DefaultValue="0">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Amp Fan Test Setpoint" ID="6" HiQnetStateVariableKey="d0fa63da-54e1-4e32-99bd-85927d2bd87a" ClassID="733" Version="1" DefaultValue="0.5">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<Data1 Len="4">AAAAPw==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="7">
								<StateVariable Name="Power Supply Fan Test Setpoint" ID="7" HiQnetStateVariableKey="10ac5ac0-8313-4dab-b6dd-7f49514a029f" ClassID="733" Version="1" DefaultValue="0.5">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<Data1 Len="4">AAAAPw==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="8">
								<StateVariable Name="Power Supply Fan Setpoint Multiplier" ID="8" HiQnetStateVariableKey="481638d2-790b-492d-bc97-abe03d40e87f" ClassID="733" Version="1" DefaultValue="1">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<Data1 Len="4">AACAPw==</Data1>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="9">
								<StateVariable Name="Error" ID="9" HiQnetStateVariableKey="9b2a65d4-7fca-4ae0-aaad-91e057961864" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="28" OBJ_ADDR="1776640">
						<Object Name="Governor" Address="1776640" ClassID="28" Version="1" HiQnetObjectKey="17586c0d-47dd-4d3d-be1e-235e1e3d819f">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="f93425e8-1038-4d1d-93d8-e674a05df575" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Attack" ID="1" HiQnetStateVariableKey="802c9878-502f-45a3-8a62-79ec1f5041d8" ClassID="733" Version="1" DefaultValue="4">
									<Data2 Len="4">AACAPw==</Data2>
									<Data3 Len="4">AABwQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Release" ID="2" HiQnetStateVariableKey="8f0039d7-cc6e-4f6a-bcfa-a232ccd158bb" ClassID="733" Version="1" DefaultValue="10">
									<Data2 Len="4">AACAPw==</Data2>
									<Data3 Len="4">AABwQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Threshold" ID="3" HiQnetStateVariableKey="381172d5-64ce-4f4e-a734-b302858989f3" ClassID="733" Version="1" DefaultValue="1500">
									<Data2 Len="4">AAAgQQ==</Data2>
									<Data3 Len="4">AEAcRg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Tau" ID="4" HiQnetStateVariableKey="a3875f8a-c9ff-482e-9ae8-f6b1a773bfb6" ClassID="733" Version="1" DefaultValue="2">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="Deadband" ID="5" HiQnetStateVariableKey="6336b90c-cbfb-4105-aa16-ed745f6c2fbb" ClassID="733" Version="1" DefaultValue="2">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AADIQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="6">
								<StateVariable Name="Hold" ID="6" HiQnetStateVariableKey="4c4cfc41-fdec-49b3-a5c4-053d5101c905" ClassID="733" Version="1" DefaultValue="3">
									<Data2 Len="4">zczMPQ==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="7">
								<StateVariable Name="Ch1 Power Meter" ID="7" HiQnetStateVariableKey="a51280e8-6005-4b48-8d1d-ce6521fb3eae" ClassID="535" Version="1" DefaultValue="-1E+37">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="8">
								<StateVariable Name="Ch1 Gain Meter" ID="8" HiQnetStateVariableKey="1d169cad-3eb3-4b3b-8555-7933fc5bb32a" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="535" SV_ID="9">
								<StateVariable Name="Ch2 Power Meter" ID="9" HiQnetStateVariableKey="6c96faf7-6ac3-4a73-b308-a47f0534d8ac" ClassID="535" Version="1" DefaultValue="-1E+37">
									<Data2 Len="4">wr3w/A==</Data2>
									<Data3 Len="4">wr3wfA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="10">
								<StateVariable Name="Ch2 Gain Meter" ID="10" HiQnetStateVariableKey="bf04383e-d253-47d0-80eb-d86401c3b2cd" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="29" OBJ_ADDR="1776896">
						<Object Name="Thermal Level Control" Address="1776896" ClassID="29" Version="1" HiQnetObjectKey="09119ef4-ce62-401d-9bd2-42220bc0a804">
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="0">
								<StateVariable Name="Power Supply Temp Threshold" ID="0" HiQnetStateVariableKey="662f8c03-dd20-4935-b353-95142e7a3d2c" ClassID="733" Version="1" DefaultValue="80">
									<Data2 Len="4">AADIQQ==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Power Supply Temp Slope" ID="1" HiQnetStateVariableKey="17f4ea2d-6b0b-4918-977d-049ea612fa6c" ClassID="733" Version="1" DefaultValue="2">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Power Supply Temp Tau" ID="2" HiQnetStateVariableKey="4091d77b-9250-4a89-a64e-bf53a2b22df0" ClassID="733" Version="1" DefaultValue="0.25">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Channel Temp Threshold" ID="3" HiQnetStateVariableKey="c51b3a24-fcc9-440b-8003-1a11c44cddfe" ClassID="733" Version="1" DefaultValue="70">
									<Data2 Len="4">AADIQQ==</Data2>
									<Data3 Len="4">AADIQg==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Channel Temp Slope" ID="4" HiQnetStateVariableKey="1813c82e-61da-4958-ac8b-4cc9aaddc034" ClassID="733" Version="1" DefaultValue="1.5">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="5">
								<StateVariable Name="Channel Temp Tau" ID="5" HiQnetStateVariableKey="06102dd4-abf7-4609-a1c0-9959bff13002" ClassID="733" Version="1" DefaultValue="0.25">
									<Data2 Len="4">AAAAAA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="38" OBJ_ADDR="1779200">
						<Object Name="Vcc Droop Limiter" Address="1779200" ClassID="38" Version="1" HiQnetObjectKey="7022db2c-39e3-4c27-b7b7-5ba68f3b4e4c">
							<STATE_VARIABLE SV_CLASSID="512" SV_ID="0">
								<StateVariable Name="Enable" ID="0" HiQnetStateVariableKey="cc7b0263-95b5-43c8-9a14-b9a6c5ed44ba" ClassID="512" Version="1" DefaultValue="1">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="1">
								<StateVariable Name="Attack" ID="1" HiQnetStateVariableKey="a4b57ed1-05f2-406e-9c55-c379b1fedf34" ClassID="733" Version="1" DefaultValue="0.025">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="2">
								<StateVariable Name="Release" ID="2" HiQnetStateVariableKey="03a471e1-87cd-42f8-bdda-dd54a3009969" ClassID="733" Version="1" DefaultValue="0.05">
									<Data2 Len="4">CtcjPA==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="3">
								<StateVariable Name="Threshold" ID="3" HiQnetStateVariableKey="6d34079d-4b8a-4a14-9c7f-d252f190c493" ClassID="733" Version="1" DefaultValue="0.001">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">AACAPw==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="733" SV_ID="4">
								<StateVariable Name="Hold" ID="4" HiQnetStateVariableKey="759db9d2-0c9a-415e-85c9-ddadfe9b11ee" ClassID="733" Version="1" DefaultValue="0.01">
									<Data2 Len="4">bxKDOg==</Data2>
									<Data3 Len="4">AAAgQQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="531" SV_ID="5">
								<StateVariable Name="Status" ID="5" HiQnetStateVariableKey="f650722a-5805-43c6-a0cf-bd949bc9474a" ClassID="531" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
							<STATE_VARIABLE SV_CLASSID="646" SV_ID="6">
								<StateVariable Name="Gain Meter" ID="6" HiQnetStateVariableKey="facbfad5-4f28-4772-8493-812691468a6f" ClassID="646" Version="1" DefaultValue="200">
									<Data2 Len="1">KA==</Data2>
									<Data3 Len="1">yA==</Data3>
									<DataF Len="2">MwA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
					<OBJECT OBJ_CLASSID="32" OBJ_ADDR="1843200">
						<Object Name="Mfg Test" Address="1843200" ClassID="32" Version="1" HiQnetObjectKey="ad833faf-a7df-48cf-8cd5-dc2038be5961">
							<STATE_VARIABLE SV_CLASSID="616" SV_ID="0">
								<StateVariable Name="Restore Factory Defaults" ID="0" HiQnetStateVariableKey="a343989f-4658-4c2f-94de-c9507e11c45d" ClassID="616" Version="1" DefaultValue="0">
									<Data2 Len="1">AA==</Data2>
									<Data3 Len="1">AQ==</Data3>
									<DataF Len="2">MQA=</DataF>
									<DataF2 Len="2">MAA=</DataF2>
									<Data4 Len="1">AA==</Data4>
								</StateVariable>
							</STATE_VARIABLE>
						</Object>
					</OBJECT>
				</Object>
				<VirtualDevice Index="0" Version="1" />
				<NodeManager Version="1" SoftwareVersion="1.1.4.3" DeveloperAccessRights="0" HopCount="5" VenueTableSize="512" UserNameA="" UserNameB="" UserNameC="" UserNameD="" DevFuncPermsA="0" DevFuncPermsB="0" DevFuncPermsC="0" DevFuncPermsD="0" AddressMode="0" DeviceState="0">
					<SerialNumber Len="16">AAAAAAAAAAAAAAAKQPwCeQ==</SerialNumber>
					<UserPasswordA Len="0"></UserPasswordA>
					<UserPasswordB Len="0"></UserPasswordB>
					<UserPasswordC Len="0"></UserPasswordC>
					<UserPasswordD Len="0"></UserPasswordD>
					<AdminPassword Len="0"></AdminPassword>
					<VenueRecallCollection />
				</NodeManager>
			</VIRTUAL_DEVICE>
		</Node>
	</NODE>
</Device>