# Speaker Preset View

Speaker Preset view is available while in Design Mode and Tune Mode and is used to change speaker presets, speaker crossover, and subwoofer orientation settings. With Speaker Preset view active, devices in the Workspace will overlay a set of model specific controls to define and change the speaker specific options. When connected and in-sync, the changes made to the devices are in real-time, if the system is disconnected, the changes will be sent to the devices once they are connected.

## Available Speaker Settings

Graphic | Setting | Effects
--- | --- | ---
| HPF Setting | Adjusts the high pass filter of the speaker or array
| Speaker Preset | Adjust the preset of the speaker or array, more information on the effect of each preset can be found in the User Manual for that product.

*Actual settings of each device will vary

## Available Subwoofer Settings

Graphic | Setting | Effects
--- | --- | ---
| LPF Setting | Adjusts the low pass filter of the subwoofer or distributed array
| Orientation | Change the device orientation to implement cardioid subwoofer arrays

*Actual settings of each device will vary

## Changing Speaker Settings

Modifying speaker settings in the Speaker Preset System View has a varying effect on the speakers depending on the connection state.

State | Active Mode | Outcome
--- | --- | ---
| Design Mode | Speaker preset settings will be pushed to the devices immediately once connected and synchronized in connect mode.
| Tune Mode | Changes to settings in Speaker Preset view will take effect on connected devices in real time. A short audible drop will occur as the settings are applied.