# Gain View

The Gain View displays an adjustable gain setting for each respective device in the Workspace. When connected and in-sync, the changes made to the devices are in real-time, if the system is disconnected, the changes will be sent to the devices once they are connected.

## Adjusting a Gain Control

Any gain control can be adjusted using the or the buttons located next to the gain value.

A gain value can also be manually entered by double clicking on the gain value and typing in a new one using the onscreen numeric keypad or a keyboard.

## Relative Gain Controls

The icon in the array header can be selected to make relative gain adjustments to all members of a System Group or an individual array depending on the Linking Options selected. The Relative Gain control will increment all members of an array by the value entered in the Relative Gain adjustment control box, preserving any offset that may exist between individual devices within an array.

##

## Unequal DSP Indicator

In the event that one (or multiple) devices within a Subwoofer Array have a gain value that is not equal to the gain value of the rest of the array, a small yellow indicator will appear next to that gain value. This unequal DSP situation can be resolved by re-entering the intended gain value and hitting enter, the software will resend the correct value to all devices within the array and as a result the devices which previously had differing values will be re-aligned with the rest of the array. In most cases, the Unequal DSP indicator will be triggered when a gain setting is manually changed via the LCD screen on a single device or in the Device Panel utility. The Device Panel Utility can always be used to interrogate individual devices and locate the device with the value offset.